For 1990-2009 cars

Connector 1: | X106 Engine Harness to Intake Harness
Connector 2: | X107 Engine Harness to Intake Harness
Connector 3: | X110 Body Harness to Body Subharness (w/o Front Defogger)
Connector 4: | X110 Body Harness to Body Subharness (Front Defogger)
Connector 5: | X111 Body Harness to Body Subharness (RHD)
Connector 6: | X112 Body Harness to Body Subharness (RHD)
Connector 7: | X112 Body Harness to Body Subharness (LHD)
Connector 8: | X113 Body Harness to Body Subharness (w/o C24)
Connector 9: | X114 Engine Extension Harness to Engine Harness (RHD)
Connector 10: | X202 I/P Harness to Body Harness
Connector 11: | X203 I/P Harness to Body Harness
Connector 12: | X204 I/P Harness to Body Harness
Connector 13: | X205 I/P Harness to Body Harness
Connector 14: | X206 Roof Harness to Body Harness (w/o C24)
Connector 15: | X206 Roof Harness to Body Harness (w/C24)
Connector 16: | X207 I/P Harness to TCM Harness
Connector 17: | X208 SIR Harness to I/P Harness
Connector 18: | X210 I/P Harness to Lock Housing Harness
Connector 19: | X211 I/P Harness to A/C Harness (Manual A/C)
Connector 20: | X211 I/P Harness to A/C Harness (Auto A/C)
Connector 21: | X212 I/P Harness to Ashtray Harness
Connector 22: | X213 I/P Harness to Body Harness
Connector 23: | X214 I/P Harness to Body Harness
Connector 24: | X216 Engine Harness to I/P Harness
Connector 25: | X218 Engine Harness to Body Harness
Connector 26: | X219 Subwoofer Speaker Harness to Body Harness
Connector 27: | X220 Engine Harness to Body Harness (Diesel)
Connector 28: | X301 Body Harness to Driver Seat Harness
Connector 29: | X302 Body Harness to Passenger Seat Harness
Connector 30: | X303 SIR Harness to Body Harness
Connector 31: | X351 Body Harness to Driver Door Harness
Connector 32: | X352 Body Harness to Driver Door Harness
Connector 33: | X361 Body Harness to Passenger Door Harness
Connector 34: | X362 Body Harness to Passenger Door Harness
Connector 35: | X371 Body Harness to Left Rear Door Harness
Connector 36: | X381 Body Harness to Right Rear Door Harness
Connector 37: | X401 Trunk Room Harness to Body Harness
Connector 38: | X402 Trunk Lid Harness to Body Harness
Connector 39: | X403 Trunk Room Harness to Rear Bumper Harness (T98/UD7)
Connector 40: | X404 Body Harness to Fuel Pump Harness

### X106 Engine Harness to Intake Harness

#### Connector Part Information

- OEM: PB625-12027
- Service: N/A
- Description: 12-Way F Sealed (BK)

#### Connector Part Information

- OEM: PB621-12020
- Service: N/A
- Description: 12-Way M Sealed (BK)

#### X106 Engine Harness to Intake Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BU | -- | Ignition Coil 4 Control | 1 | BU | -- | Ignition Coil 4 Control
2 | GN | -- | Ignition Coil 5 Control | 2 | GN | -- | Ignition Coil 5 Control
3 | GY | -- | Ignition Coil 6 Control | 3 | GY | -- | Ignition Coil 6 Control
4 | PK | -- | Ignition Voltage | 4 | PK | -- | Ignition Voltage
5 | PK | -- | Ignition Voltage | 5 | PK/BK | -- | Ignition Voltage
6 | YE | -- | ECT Signal | 6 | YE | -- | ECT Signal
7 | YE | -- | Ignition Coil 3 Control | 7 | YE | -- | Ignition Coil 3 Control
8 | OG | -- | Ignition Coil 2 Control | 8 | OG | -- | Ignition Coil 2 Control
9 | PU | -- | Ignition Coil 1 Control | 9 | PU | -- | Ignition Coil 1 Control
10 | BK | -- | Ground | 10 | BK | -- | Ground
11 | BK | -- | Ignition Coil Shield Ground | 11 | BK | -- | Ignition Coil Shield Ground
12 | BN | -- | Low Ref - ECT Sensor | 12 | BN | -- | Low Ref - ECT Sensor

### X107 Engine Harness to Intake Harness

#### Connector Part Information

- OEM: PB625-06027
- Service: N/A
- Description: 6-Way F Sealed BK

#### Connector Part Information

- OEM: PB621-06020
- Service: N/A
- Description: 6-Way M Sealed BK

#### X107 Engine Harness to Intake Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-BU/BK | -- | Fuel Injector 4 Control | 1 | L-BU/BK | -- | Fuel Injector 4 Control
2 | BN/WH | -- | Fuel Injector 5 Control | 2 | BN/WH | -- | Fuel Injector 5 Control
3 | YE/BK | -- | Fuel Injector 6 Control | 3 | YE/BK | -- | Fuel Injector 6 Control
4 | BN | -- | Fuel Injector 1 Control | 4 | BN | -- | Fuel Injector 1 Control
5 | L-GN/BK | -- | Fuel Injector 2 Control | 5 | L-GN/BK | -- | Fuel Injector 2 Control
6 | PK/BK | -- | Fuel Injector 3 Control | 6 | PK/BK | -- | Fuel Injector 3 Control

### X110 Body Harness to Body Subharness (w/o Front Defogger)

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP Series Sealed (BK)

#### Connector Part Information

- OEM: PB621-02020
- Service: N/A
- Description: 2-Way M NMWP Series Sealed (BK)

#### X110 Body Harness to Body Subharness (w/o Front Defogger)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN/WH | -- | Wheel Speed Sensor Signal | 1 | BN/WH | -- | Wheel Speed Sensor Signal
2 | D-BU/WH | -- | Wheel Speed Sensor Return | 2 | D-BU/WH | -- | Wheel Speed Sensor Return

### X110 Body Harness to Body Subharness (Front Defogger)

#### Connector Part Information

- OEM: PB625-04027
- Service: N/A
- Description: 4-Way F NMWP Series Sealed (BK)

#### Connector Part Information

- OEM: PB621-02020
- Service: N/A
- Description: 4-Way M NMWP Series Sealed (BK)

#### X110 Body Harness to Body Subharness (Front Defogger)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | -- | Ground (Holden, Euro/Gen, RHD Diesel) | 1 | BK | -- | Ground (Holden, Euro/Gen, RHD Diesel)
2 | PU | -- | Defog Element Supply Voltage | 2 | PU | -- | Defog Element Supply Voltage
3 | BN/WH | -- | Right Front Wheel Speed Sensor Signal | 3 | BN/WH | -- | Right Front Wheel Speed Sensor Signal
4 | D-BU/WH | -- | Right Front Wheel Speed Sensor Return | 4 | D-BU/WH | -- | Right Front Wheel Speed Sensor Return

### X111 Body Harness to Body Subharness (RHD)

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F Sealed BK

#### Connector Part Information

- OEM: PB621-02020
- Service: N/A
- Description: 2-Way M Sealed BK

#### X111 Body Harness to Body Subharness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-BU | -- | Wheel Speed Sensor Signal | 1 | D-BU | -- | Wheel Speed Sensor Signal
2 | L-GN | -- | Wheel Speed Sensor Return | 2 | L-GN | -- | Wheel Speed Sensor Return

### X112 Body Harness to Body Subharness (RHD)

#### Connector Part Information

- OEM: PB625-08027
- Service: N/A
- Description: 8-Way F Sealed BK

#### Connector Part Information

- OEM: PB621-08020
- Service: N/A
- Description: 8-Way M Sealed BK

#### X112 Body Harness to Body Subharness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK | -- | Battery Positive Voltage | 1 | PK | -- | Battery Positive Voltage
2 | BN/WH | -- | Wiper Return Position Signal | 2 | BN/WH | -- | Wiper Return Position Signal
3 | BK | -- | Ground | 3 | BK | -- | Ground
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | D-GN | -- | Windshield Wiper Switch Output | 6 | D-GN | -- | Windshield Wiper Switch Output
7 | PU | -- | Windshield Wiper Motor Input | 7 | PU | -- | Windshield Wiper Motor Input
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

### X112 Body Harness to Body Subharness (LHD)

#### Connector Part Information

- OEM: PB625-06027
- Service: N/A
- Description: 6-Way F Sealed BK

#### Connector Part Information

- OEM: PB621-06020
- Service: N/A
- Description: 6-Way M Sealed BK

#### X112 Body Harness to Body Subharness (LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK | -- | Ignition Voltage | 1 | PK | -- | Ignition Voltage
2 | D-BU | -- | Wiper Speed 2 Signal | 2 | D-BU | -- | Wiper Speed 2 Signal
3 | L-GN | -- | Wiper Speed 1 Signal | 3 | L-GN | -- | Wiper Speed 1 Signal
4 | BN/WH | -- | Brake Fluid Level Signal | 4 | BN/WH | -- | Brake Fluid Level Signal
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used

### X113 Body Harness to Body Subharness (w/o C24)

#### Connector Part Information

- OEM: PB625-08027
- Service: N/A
- Description: 8-Way F Sealed BK

#### Connector Part Information

- OEM: PB621-08020
- Service: N/A
- Description: 8-Way M Sealed BK

#### X113 Body Harness to Body Subharness (w/o C24)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | BN/WH | -- | Wiper Return Position Signal (RHD) | 2 | BN/WH | -- | Wiper Return Position Signal (RHD)
3 | PK | -- | Battery Positive Voltage (Diesel) | 3 | PK | -- | Battery Positive Voltage (Diesel)
4 | BN/WH | -- | Brake Fluid Level Signal | 4 | BN/WH | -- | Brake Fluid Level Signal
5 | WH/BK | -- | ABS Warning Lamp Control (LHD) | 5 | WH/BK | -- | ABS Warning Lamp Control (LHD)
BK | -- | Ground (RHD) | BK | -- | Ground (RHD)
6 | D-GN | -- | Windshield Wiper Switch Output - Low (RHD) | 6 | D-GN | -- | Windshield Wiper Switch Output - Low (RHD)
7 | PU | -- | Windshield Wiper Switch Output - High (RHD) | 7 | PU | -- | Windshield Wiper Switch Output - High (RHD)
8 | PK | -- | Ignition Voltage | 8 | PK | -- | Ignition Voltage
BK | -- | Ground | BK | -- | Ground

### X114 Engine Extension Harness to Engine Harness (RHD)

#### Connector Part Information

- OEM: 1743059-2
- Service: N/A
- Description: 36-Way F Sealed BK

#### Connector Part Information

- OEM: 1743062-2
- Service: N/A
- Description: 36-Way M Sealed BK

#### X114 Engine Extension Harness to Engine Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK/BK | -- | Ignition Voltage | 1 | PK/BK | -- | Ignition Voltage
BN | -- | PTC 3 Relay Output (Diesel) | BN | -- | PTC 3 Relay Output (Diesel)
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | PU | -- | Low Reference | 3 | PU | -- | Low Reference
4 | BN | -- | ECM CAN Low | 4 | BN | -- | ECM CAN Low
5 | L-GN/BK | -- | Rough Road Signal | 5 | L-GN/BK | -- | Rough Road Signal
6 | YE | -- | Clutch Switch Signal | 6 | YE | -- | Clutch Switch Signal
7 | BN/WH | -- | ECM CAN High | 7 | BN/WH | -- | ECM CAN High
8 | PK | -- | Ignition Voltage | 8 | PK | -- | Ignition Voltage
9 | BN | -- | Low Reference | 9 | BN | -- | Low Reference
10 | L-BU | -- | APP Sensor 2 Signal | 10 | L-BU | -- | APP Sensor 2 Signal
11 | OG | -- | Fuel Consumption Signal | 11 | OG | -- | Fuel Consumption Signal
12 | L-BU | -- | Stop Lamp Switch Output | 12 | L-BU | -- | Stop Lamp Switch Output
13 | WH/BK | -- | WSS Signal - LF (Diesel) | 13 | WH/BK | -- | WSS Signal - LF (Diesel)
GN/WH | -- | VSS Signal (Gas) | GN/WH | -- | VSS Signal (Gas)
14 | WH | -- | Engine RPM Signal | 14 | WH | -- | Engine RPM Signal
15 | YE/BK | -- | PTC Relay 2 Output (Diesel) | 15 | YE/BK | -- | PTC Relay 2 Output (Diesel)
16 | BU | -- | APP Sensor 1 Signal | 16 | BU | -- | APP Sensor 1 Signal
17 | WH/BK | -- | 5V Reference | 17 | WH/BK | -- | 5V Reference
18 | YE | -- | Diesel Particulate Indicator Control | 18 | YE | -- | Diesel Particulate Indicator Control
19 | BN | -- | Charge Warning Indicator | 19 | BN | -- | Charge Warning Indicator
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | D-BU/WH | -- | Fuel Level Signal | 21 | D-BU/WH | -- | Fuel Level Signal
22 | L-BU | -- | 5V Reference | 22 | L-BU | -- | 5V Reference
23 | GN | -- | 5V Reference | 23 | GN | -- | 5V Reference
24 | BN/WH | -- | WIF Indicator Control (Diesel) | 24 | BN/WH | -- | WIF Indicator Control (Diesel)
25 | -- | -- | Not Used | 25 | -- | -- | Not Used
26 | WH/BK | -- | PTC Request (Diesel) | 26 | WH/BK | -- | PTC Request (Diesel)
27 | YE | -- | Sensor Ground | 27 | YE | -- | Sensor Ground
28 | L-GN/BK | -- | Ambient Temp Signal | 28 | L-GN/BK | -- | Ambient Temp Signal
29 | OG/BK | -- | PNP Switch Control | 29 | OG/BK | -- | PNP Switch Control
BU/WH | -- | PTC 1 Relay Output (Diesel) | BU/WH | -- | PTC 1 Relay Output (Diesel)
GN | -- | VSS Signal (M/T) | GN | -- | VSS Signal (M/T)
30 | BK | -- | Low Reference (Gas) | 30 | BK | -- | Low Reference (Gas)
YE/BK | -- | Glow Plug Indicator Control (Diesel) | L-BU | -- | Glow Plug Indicator Control (Diesel)
31 | D-GN | -- | FTP Sensor Signal | 31 | D-GN | -- | FTP Sensor Signal
32 | PU | -- | Evap Canister SV Control | 32 | PU | -- | Evap Canister SV Control
OG/BK | -- | PNP Switch Control (Diesel) | OG/BK | -- | PNP Switch Control (Diesel)
GN | -- | VSS Signal (Diesel M/T) | GN | -- | VSS Signal (Diesel M/T)
33 | L-BU/BK | -- | Cruise Switch Ground | 33 | L-BU/BK | -- | Cruise Switch Ground
34 | WH | -- | Cruise Indicator Control | 34 | WH | -- | Cruise Indicator Control
35 | GY | -- | Cruise Switch Signal | 35 | GY | -- | Cruise Switch Signal
36 | BN | -- | Oil Pressure Switch Signal | 36 | BN | -- | Oil Pressure Switch Signal

### X202 I/P Harness to Body Harness

-- | --

#### Connector Part Information

- OEM: MG612469
- Service: N/A
- Description: 23-Way F

#### Connector Part Information

- OEM: MG622471
- Service: N/A
- Description: 23-Way M

#### X202 I/P Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | YE | 190 | Left Folding Mirror Motor Extend Control (DM4) | 2 | YE | 190 | Left Folding Mirror Motor Extend Control (DM4)
3 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 3 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
4 | D-BU | 1729 | Electronic Control Unit 12 Volt Reference | 4 | D-BU | 1729 | Electronic Control Unit 12 Volt Reference
5 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 5 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
6 | L-BU | 191 | Left Folding Mirror Motor Retract Control (DM4) | 6 | L-BU | 191 | Left Folding Mirror Motor Retract Control (DM4)
7 | D-GN/BK | 1798 | Low Reference | 7 | D-GN/BK | 1798 | Low Reference
8 | PU/WH | 5754 | Amplifier Powered Woofer Control (1) (U64) | 8 | PU/WH | 5754 | Amplifier Powered Woofer Control (1) (U64)
9 | WH | 315 | Right Subwoofer Speaker (-) | 9 | WH | 315 | Right Subwoofer Speaker (-)
10 | BK/WH | 1559 | Low Reference (LHD) | 10 | BK/WH | 1559 | Low Reference
BK/WH | 1559 | Low Reference
11 | PK/BK | 5755 | Amplifier Powered Woofer Control (2) (U64) | 11 | PK/BK | 5755 | Amplifier Powered Woofer Control (2) (U64)
12 | D-GN | 1795 | Right Subwoofer Speaker (+) | 12 | D-GN | 1795 | Right Subwoofer Speaker (+)
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | BN | 1890 | Mirror Common | 14 | GY | 1890 | Mirror Common
BN | 1890 | Mirror Common
BN | 1890 | Mirror Common
15 | D-BU/WH | 6985 | Front Wiper Auto / Interval Resistance Coded (C24) | 15 | D-BU/WH | 6985 | Front Wiper Auto / Interval Resistance Coded (C24)
16 | D-GN/WH | 762 | A/C Request Signal | 16 | D-GN/WH | 762 | A/C Request Signal
17 | GY/WH | 1657 | ABS Solenoid Control (1) | 17 | GY/WH | 1657 | ABS Solenoid Control (1)
18-19 | -- | -- | Not Used | 18-19 | -- | -- | Not Used
20 | RD/WH | 1340 | Battery Positive Voltage | 20 | RD/WH | 1340 | Battery Positive Voltage
21 | RD/BK | 242 | Battery Positive Voltage | 21 | RD/BK | 242 | Battery Positive Voltage
22 | PU/WH | 1293 | Defogger Supply Voltage | 22 | PU/WH | 1293 | Defogger Supply Voltage
23 | YE | 5 | Crank Voltage | 23 | YE | 5 | Crank Voltage

### X203 I/P Harness to Body Harness

#### Connector Part Information

- OEM: MG651882-3
- Service: N/A
- Description: 16-Way F (YE)

#### Connector Part Information

- OEM: MG641884
- Service: N/A
- Description: 16-Way M (YE)

#### X203 I/P Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | WH | 1080 | Illumination Relay Control | 1 | WH | 1080 | Illumination Relay Control
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | BN | 41 | Ignition 3 Voltage | 3 | BN | 41 | Ignition 3 Voltage
4 | GY | 161 | Antenna Power | 4 | GY | 161 | Antenna Power
5 | GY | 118 | LF (RF RHD) Speaker Output (-) | 5 | GY | 118 | LF (RF RHD) Speaker Output (-)
GY | 118 | LF (RF RHD) Speaker Output (-)
6 | YE | 116 | Left Rear Speaker Output (-) | 6 | YE | 116 | Left Rear Speaker Output (-)
7 | PK | 939 | Battery Positive Voltage | 7 | PK | 939 | Battery Positive Voltage
PK | 939 | Battery Positive Voltage (C24)
8 | RD/WH | 1642 | Battery Positive Voltage | 8 | RD/WH | 1642 | Battery Positive Voltage
9 | BN | 1739 | Ignition 1 Voltage | 9 | BN | 1739 | Ignition 1 Voltage
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | BN | 201 | Left Front Speaker Output (+) | 11 | BN | 201 | Left Front Speaker Output (+)
BN | 201 | Left Front Speaker Output (+)
12 | WH | 119 | Left Rear Speaker Output (+) | 12 | WH | 119 | Left Rear Speaker Output (+)
13 | RD/BK | 742 | Battery Voltage | 13 | RD/BK | 742 | Battery Voltage
14 | RD/BK | 642 | Battery Voltage | 14 | RD/BK | 642 | Battery Voltage
15 | RD/WH | 1740 | Battery Positive Voltage | 15 | RD/WH | 1740 | Battery Positive Voltage
16 | BN | 126 | Left Front Door Open Switch Signal | 16 | BN | 126 | Left Front Door Open Switch Signal
BN | 126 | Left Front Door Open Switch Signal

### X204 I/P Harness to Body Harness

#### Connector Part Information

- OEM: MG651086
- Service: N/A
- Description: 22-Way F 090 II Series (NA)

#### Connector Part Information

- OEM: MG641089
- Service: N/A
- Description: 22-Way M 090 II Series (NA)

#### X204 I/P Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage | 1 | RD/WH | -- | Battery Positive Voltage
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | L-GN | -- | Backup Lamp Control | 3 | L-GN | -- | Backup Lamp Control
4 | D-GN | -- | Wiper Switch Signal | 4 | D-GN/WH | -- | Wiper Switch Signal
5 | RD/WH | -- | Multifunction Control Module Output | 5 | RD/WH | -- | Multifunction Control Module Output
6 | RD/WH | -- | Headlamp High Relay Control | 6 | RD/WH | -- | Headlamp High Relay Control
7 | OG | -- | Fuel Level Signal | 7 | OG | -- | Fuel Level Signal
8 | D-GN | -- | Windshield Wiper Motor Control | 8 | D-GN | -- | Windshield Wiper Motor Control
9 | OG | -- | Windshield Washer Pump Control | 9 | OG | -- | Windshield Washer Pump Control
10 | PU | -- | Windshield Wiper Motor High Speed | 10 | PU | -- | Windshield Wiper Motor High Speed
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | OG/BK | -- | Rear Compartment Signal | 12 | OG/BK | -- | Rear Compartment Signal
13 | L-BU | -- | Stop Lamp Switch Output | 13 | L-BU | -- | Stop Lamp Switch Output
14 | BN | -- | Ignition Voltage | 14 | BN | -- | Ignition Voltage
15 | YE | -- | Ignition Voltage | 15 | YE | -- | Ignition Voltage
16 | PK | -- | Ignition Voltage | 16 | PK | -- | Ignition Voltage
17 | GY | -- | Fuel Pump Relay Output | 17 | GY | -- | Fuel Pump Relay Output
18 | -- | -- | Not Used | 18 | -- | -- | Not Used
19 | -- | -- | Not Used | 19 | -- | -- | Not Used
20 | PK | -- | Ignition Voltage | 20 | PK | -- | Ignition Voltage
21 | L-BU | -- | Windshield Wiper Switch Signal | 21 | L-BU | -- | Windshield Wiper Switch Signal
22 | BN | -- | Windshield Wiper Park Signal | 22 | BN/WH | -- | Windshield Wiper Park Signal

### X205 I/P Harness to Body Harness

#### Connector Part Information

- OEM: MG651563
- Service: N/A
- Description: 23-Way F (WH)

#### Connector Part Information

- OEM: MG641560
- Service: N/A
- Description: 23-Way M (WH)

#### X205 I/P Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | -- | Horn Relay Output | 1 | BN | -- | Horn Relay Output
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | WH | -- | Driver Mirror Left/Right Control | 3 | WH | -- | Driver Mirror Left/Right Control
4 | YE | -- | Driver Mirror Up/Down Control | 4 | YE | -- | Driver Mirror Up/Down Control
5 | BU/WH | -- | MIL Indicator Control | 5 | BU/WH | -- | MIL Indicator Control
6 | L-BU | -- | Tamper Switch Signal | 6 | L-BU | -- | Tamper Switch Signal
7 | BN | -- | Driver Door Signal (RHD Diesel) | 7 | BN | -- | Driver Door Signal (RHD Diesel)
YE | -- | Fuel Warning Lamp Signal (LHD) | YE | -- | Fuel Warning Lamp Signal (LHD)
8 | BN/WH | -- | Brake Fluid Level Signal | 8 | BN/WH | -- | Brake Fluid Level Signal
9 | D-GN | -- | Coolant Temp Gage Control | 9 | D-GN | -- | Coolant Temp Gage Control
10 | GY | -- | PAS Indicator Control | 10 | GY | -- | PAS Indicator Control
11 | BU/WH | -- | Power Steering Control Module Serial Data | 11 | BU/WH | -- | Power Steering Control Module Serial Data
12 | -- | -- | Not Used | 12 | -- | -- | Not Used
13 | L-GN/BK | -- | SSPS Indicator Control | 13 | L-GN/BK | -- | SSPS Indicator Control
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
PU/WH | -- | Subwoofer Ground (RHD w/ amp) | PU/WH | -- | Subwoofer Ground (RHD w/ amp)
15 | PK/BK | -- | Remote Subwoofer on (RHD w/ amp) | 15 | PK/BK | -- | Remote Subwoofer on (RHD w/ amp)
BN | -- | Headlamp Leveling Switch Output | BN | -- | Headlamp Leveling Switch Output
16 | L-GN | -- | Headlamp Low Relay Output | 16 | L-GN | -- | Headlamp Low Relay Output
17 | D-GN | -- | TCS Active Indicator Control | 17 | D-GN | -- | TCS Active Indicator Control
18 | D-GN/BK | -- | ABS Warning Lamp Control | 18 | D-GN/BK | -- | ABS Warning Lamp Control
19 | PU | -- | TCS Indicator Control | 19 | PU | -- | TCS Indicator Control
20 | L-BU | -- | TCS Switch Input | 20 | L-BU | -- | TCS Switch Input
21 | D-GN/WH | -- | Front Fog Lamp Relay Control | 21 | D-GN/WH | -- | Front Fog Lamp Relay Control
22 | OG | -- | Rear Fog Lamp Control (LHD Diesel) | 22 | OG | -- | Rear Fog Lamp Control (LHD Diesel)
23 | OG | -- | Rear Fog Lamp Control | 23 | OG | -- | Rear Fog Lamp Control
D-BU/WH | -- | Fuel Level Signal (LHD Diesel) | D-BU/WH | -- | Fuel Level Signal (LHD Diesel)

### X206 Roof Harness to Body Harness (w/o C24)

#### Connector Part Information

- OEM: 936092-1
- Service: N/A
- Description: 10-Way F 090 III Series, Sealed (NA)

#### Connector Part Information

- OEM: 936129-1
- Service: N/A
- Description: 10-Way M 090 III Series, Sealed (NA)

#### X206 Roof Harness to Body Harness (w/o C24)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 450 | Ground | 1 | BK | 550 | Ground
2 | L-GN | 24 | Back up Lamps Supply Voltage | 2 | L-GN | 24 | Back up Lamps Supply Voltage
3 | PK | 839 | Ignition 1 Voltage | 3 | PK | 839 | Ignition 1 Voltage
4 | OG | 930 | Not Used | 4 | -- | -- | Not Used
5 | BN | 6136 | Passenger Compartment Lamp Suuply Voltage | 5 | RD/WH | 640 | Passenger Compartment Lamp Supply Voltage
6 | D-GN | 654 | Not Used | 6 | -- | -- | Not Used
7 | RD/WH | 840 | Battery Positive Voltage | 7 | RD/WH | 840 | Battery Positive Voltage
8 | OG | 6815 | Center Dome Lamp Input | 8 | D-BU/WH | 6815 | Center Dome Lamp Input
9 | WH | 655 | Not Used | 9 | -- | -- | Not Used
10 | YE | 43 | Ignition Voltage | 10 | YE | 43 | Ignition Voltage

### X206 Roof Harness to Body Harness (w/C24)

#### Connector Part Information

- OEM: 926204-1
- Service: N/A
- Description: 18-Way F 090 III Series (NA)

#### Connector Part Information

- OEM: 936213-1
- Service: N/A
- Description: 18-Way M 090 III Series (NA)

#### X206 Roof Harness to Body Harness (w/C24)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN | 227 | Wiper Speed 1 Signal | 1 | L-GN | 227 | Wiper Speed 1 Signal
2 | OG | 228 | Washer Switch Signal | 2 | OG | 228 | Washer Switch Signal
3 | BK | 450 | Ground | 3 | BK | 550 | Ground
4 | L-GN | 24 | Backup Lamps Supply Voltage | 4 | L-GN | 24 | Backup Lamps Supply Voltage
5 | PK | 839 | Ignition 1 Voltage | 5 | PK | 839 | Ignition 1 Voltage
6 | YE | 43 | Ignition Voltage | 6 | YE | 43 | Ignition Voltage
7 | D-BU/WH | 6985 | Wiper Intermittent Signal | 7 | D-BU/WH | 6985 | Wiper Intermittent Signal
8 | D-BU | 04 | Wiper Speed 2 Signal | 8 | D-BU | 94 | Wiper Speed 2 Signal
9 | -- | -- | Not Used | 9 | -- | -- | Not Used
10 | BN/WH | 96 | Wiper Park Signal | 10 | BN/WH | 196 | Wiper Park Signal
11 | D-GN | 920 | Not Used | 11 | -- | -- | Not Used
12 | BN | 6136 | Passenger Compartment Lamp Supply Voltage | 12 | OG/BK | 640 | Passenger Compartment Lamp Supply Voltage
13 | D-GN | 654 | Cellular Telephone Microphone Low Reference | 13 | D-GN | 654 | Cellular Telephone Microphone Low Reference
14 | RD/WH | 840 | Battery Positive Voltage | 14 | RD/WH | 840 | Battery Positive Voltage
15 | OG | 6815 | Center Dome Lamp Supply Voltage | 15 | D-BU/WH | 6815 | Center Dome Lamp Supply Voltage
16 | D-GN | 655 | Not Used | 16 | -- | -- | Not Used
17 | PK | 1939 | Ignition Voltage | 17 | PK | 939 | Ignition Voltage
18 | -- | -- | Not Used | 18 | -- | -- | Not Used

### X207 I/P Harness to TCM Harness

#### Connector Part Information

- OEM: MG610837
- Service: N/A
- Description: 22-Way F WH

#### Connector Part Information

- OEM: MG620838
- Service: N/A
- Description: 22-Way M WH

#### X207 I/P Harness to TCM Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-GN | -- | VSS Signal | 1 | D-GN | -- | VSS Signal (LHD)
L-GN/WH | -- | VSS Signal (RHD)
2 | BN/BK | -- | CAN High | 2 | BN/BK | -- | CAN High
3 | PK/BK | -- | PNP Switch Control | 3 | PK/BK | -- | PNP Switch Control
4 | L-GN/WH | -- | Shift Lock Solenoid Supply Voltage | 4 | L-GN/WH | -- | Shift Lock Solenoid Supply Voltage
5 | L-GN | -- | WINTER Mode Indicator Control | 5 | D-BU/WH | -- | WINTER Mode Indicator Control
6 | BN | -- | CAN Low | 6 | BN | -- | CAN Low
7 | BK/WH | -- | PNP Switch Ground | 7 | BK/WH | -- | PNP Switch Ground
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | L-BU | -- | Stop Lamp Switch Output | 9 | L-BU | -- | Stop Lamp Switch Output
10 | PK | -- | Ignition Voltage | 10 | PK | -- | Ignition Voltage
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | PK | -- | Ignition Voltage | 12 | PK | -- | Ignition Voltage
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | D-GN | -- | Serial Data | 14 | D-GN | -- | Serial Data
15 | PU | -- | Tap up Signal (TCM) | 15 | PU | -- | Tap up Signal (TCM)
16 | L-GN | -- | Park/Neutral Position (PNP) Switch Output | 16 | L-GN | -- | Park/Neutral Position (PNP) Switch Output
17 | RD/WH | -- | Battery Positive Voltage | 17 | RD/WH | -- | Battery Positive Voltage (LHD)
OG | -- | Battery Positive Voltage (RHD)
18 | BN | -- | Driver Shift Control (TCM) | 18 | BN | -- | Driver Shift Control (TCM)
19 | BN | -- | Tap Down Signal (TCM) | 19 | BN | -- | Tap Down Signal (TCM)
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | -- | -- | Not Used | 21 | -- | -- | Not Used
22 | -- | -- | Not Used | 22 | -- | -- | Not Used

### X208 SIR Harness to I/P Harness

#### Connector Part Information

- OEM: MG651881
- Service: N/A
- Description: 16-Way F WH

#### Connector Part Information

- OEM: MG641883
- Service: N/A
- Description: 16-Way M WH

#### X208 SIR Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | YE | -- | Driver Seat Belt Warning Indicator Control | 2 | YE | -- | Driver Seat Belt Warning Indicator Control
3 | OG | -- | Crash Signal | 3 | OG | -- | Crash Signal
4 | PK | -- | Ignition Voltage | 4 | PK | -- | Ignition Voltage
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | GN/WH | -- | VSS Signal | 6 | GN/WH | -- | VSS Signal
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | -- | -- | Not Used | 9 | -- | -- | Not Used
10 | PU/WH | -- | Passenger Seatbelt Warning Indicator Control (LHD Diesel) | 10 | PU | -- | Passenger Seatbelt Warning Indicator Control
PU | -- | Passenger Seatbelt Warning Indicator Control
11 | L-GN | -- | Chime Signal | 11 | L-GN | -- | Chime Signal
12 | WH/BK | -- | Serial Data | 12 | WH/BK | -- | Serial Data
13 | BN | -- | Airbag Warning Indicator Control | 13 | BN | -- | Airbag Warning Indicator Control
14 | GN/WH | - | PASSENGER AIRBAG OFF Indicator Control | 14 | GN/WH | -- | PASSENGER AIRBAG OFF Indicator Control
L-BU | -- | PASSENGER AIRBAG OFF Indicator Control (LHD Diesel)
15 | -- | -- | Not Used | 15 | -- | -- | Not Used
16 | -- | -- | Not Used | 16 | -- | -- | Not Used

### X210 I/P Harness to Lock Housing Harness

#### Connector Part Information

- OEM: 368541-1
- Service: N/A
- Description: 10-Way F WH

#### Connector Part Information

- OEM: 368506
- Service: N/A
- Description: 10-Way M WH

#### X210 I/P Harness to Lock Housing Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN | -- | Theft Data In | 1 | L-GN | -- | Theft Data In
2 | BN/WH | -- | Theft Data Out | 2 | BN/WH | -- | Theft Data Out
3 | YE/BK | -- | Theft Power Supply | 3 | YE/BK | -- | Theft Power Supply
4 | BK/WH | -- | Ground | 4 | BK/WH | -- | Ground
5 | BK | -- | Ground | 5 | BK | -- | Ground
6 | D-BU/WH | -- | Key Illumination Input | 6 | D-BU/WH | -- | Key Illumination Input
7 | L-GN | -- | Key Reminder Switch Output | 7 | L-GN | -- | Key Reminder Switch Output
8 | RD/WH | -- | Battery Positive Voltage | 8 | RD/WH | -- | Battery Positive Voltage
9 | -- | -- | Not Used | 9 | -- | -- | Not Used
10 | -- | -- | Not Used | 10 | -- | -- | Not Used

### X211 I/P Harness to A/C Harness (Manual A/C)

#### Connector Part Information

- OEM: 85113-1
- Service: N/A
- Description: 15-Way F WH

#### Connector Part Information

- OEM: 85114-1
- Service: N/A
- Description: 15-Way M WH

#### X211 I/P Harness to A/C Harness (Manual A/C)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | D-GN/WH | -- | AC Request Signal | 2 | D-GN/WH | -- | AC Request Signal
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | BN/WH | -- | Illumination Voltage | 4 | BN/WH | -- | Illumination Voltage
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BN | -- | Ignition Voltage | 6 | BN | -- | Ignition Voltage
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | RD/WH | -- | Battery Positive Voltage | 9 | RD/WH | -- | Battery Positive Voltage
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | YE/BK | -- | Blower Relay Output | 12 | YE | -- | Blower Relay Output
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | -- | -- | Not Used | 15 | -- | -- | Not Used

### X211 I/P Harness to A/C Harness (Auto A/C)

#### Connector Part Information

- OEM: MG651881
- Service: N/A
- Description: 16-Way F WH

#### Connector Part Information

- OEM: MG641883
- Service: N/A
- Description: 16-Way M WH

#### X211 I/P Harness to A/C Harness (Auto A/C)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN/WH | -- | Illumination Voltage | 1 | BN/WH | -- | Illumination Voltage
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | D-GN/WH | -- | A/C Request | 3 | D-GN/WH | -- | A/C Request
4 | YE | -- | Sensor Ground | 4 | YE | -- | Sensor Ground
5 | RD/WH | -- | Battery Positive Voltage | 5 | OG | -- | Battery Positive Voltage
6 | WH/BK | -- | PTC Request | 6 | WH/BK | -- | PTC Request
7 | YE/BK | -- | Blower Relay Output | 7 | YE | -- | Blower Relay Output
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BN | -- | Ignition Voltage | 9 | BN | -- | Ignition Voltage
10 | GN/WH | -- | VSS Signal | 10 | GN/RD | -- | VSS Signal
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | D-GN/WH | -- | Wiper Switch Signal | 12 | D-GN/WH | -- | Wiper Switch Signal
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | YE | -- | Sun Load Signal | 15 | L-BU/BK | -- | Sun Load Signal
16 | L-GN/BK | -- | Ambient Temp Signal | 16 | L-GN/BK | -- | Ambient Temp Signal

### X212 I/P Harness to Ashtray Harness

#### Connector Part Information

- OEM: MG612225
- Service: N/A
- Description: 4-Way F WH

#### Connector Part Information

- OEM: MG622226
- Service: N/A
- Description: 4-Way M WH

#### X212 I/P Harness to Ashtray Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-GN | -- | Ashtray Lamp Output | 1 | D-GN | -- | Ashtray Lamp Output
2 | BK | -- | Ground | 2 | BK | -- | Ground
3 | BN/WH | -- | Illumination Supply Voltage | 3 | BN/WH | -- | Illumination Supply Voltage
4 | YE | -- | Ignition Voltage | 4 | YE | -- | Ignition Voltage

### X213 I/P Harness to Body Harness

#### Connector Part Information

- OEM: MG651563
- Service: N/A
- Description: 23-Way F WH

#### Connector Part Information

- OEM: MG641560
- Service: N/A
- Description: 23-Way M WH

#### X213 I/P Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK/WH | -- | Subwoofer Output (-) (LHD) | 1 | BK/WH | -- | Subwoofer Output (-) (LHD)
2 | GY | -- | Door Open Signal | 2 | GY | -- | Door Open Signal
3 | YE | -- | Low Fuel Signal | 3 | YE | -- | Low Fuel Signal
4 | BN | -- | Headlamp Leveling Switch Output (RHD) | 4 | BN | -- | Headlamp Leveling Switch Output (RHD)
5 | WH | -- | Passenger Door Signal | 5 | WH | -- | Passenger Door Signal
6 | BN | -- | Park Brake Signal | 6 | BN | -- | Park Brake Signal
7 | L-GN/BK | -- | Rough Road Signal | 7 | L-GN/BK | -- | Rough Road Signal
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | RD/WH | -- | Passenger Mirror Up/Down Control | 9 | RD/WH | -- | Passenger Mirror Up/Down Control
10 | BN | -- | Passenger OSRV Common | 10 | GY | -- | Passenger OSRV Common
GY | --
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | PU/WH | -- | Subwoofer Ground (LHD) | 12 | PU/WH | -- | Subwoofer Ground (LHD)
13 | PK/BK | -- | Remote Sub ON (LHD) | 13 | PK/BK | -- | Remote Sub ON (LHD)
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | D-GN/WH | -- | 5V Reference | 15 | D-GN/WH | -- | 5V Reference
16 | D-GN | -- | Vertical Signal | 16 | D-GN | -- | Vertical Signal
17 | D-GN | -- | Traction Control Active Signal | 17 | D-GN | -- | Traction Control Active Signal
18 | D-GN/BK | -- | ABS Warning Lamp Control | 18 | D-GN/BK | -- | ABS Warning Lamp Control
19 | -- | -- | Not Used | 19 | -- | -- | Not Used
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | RD | -- | Horizontal Signal | 21 | RD | -- | Horizontal Signal
22 | PU | -- | Passenger Mirror Left/Right Control | 22 | PU | -- | Passenger Mirror Left/Right Control
23 | -- | -- | Not Used | 23 | -- | -- | Not Used

### X214 I/P Harness to Body Harness

-- | --

#### Connector Part Information

- OEM: MG612469
- Service: N/A
- Description: 23-Way F 090/187 Hybrid Series (NA)

#### Connector Part Information

- OEM: MG622471
- Service: N/A
- Description: 23-Way M 090/187 Hybrid Series (NA)

#### X214 I/P Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN/BK | 2500 | High Speed GMLAN Serial Data (+) | 1 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | BN | 2501 | High Speed GMLAN Serial Data (-) | 3 | BN | 2501 | High Speed GMLAN Serial Data (-)
4 | WH/BK | 5043 | Serial Data | 4 | WH/BK | 5043 | Serial Data
WH/BK | 5043 | Serial Data
5 | D-GN/WH | 817 | Vehicle Speed Signal | 5 | D-GN/WH | 817 | Vehicle Speed Signal
6 | D-BU | 46 | Right Rear Speaker (+) | 6 | D-BU | 46 | Right Rear Speaker (+)
7 | L-BU | 115 | Right Rear Speaker Signal (-) | 7 | L-BU | 115 | Right Rear Speaker Signal (-)
8 | D-BU/WH | 1936 | Primary Fuel Level Sensor Signal | 8 | D-BU/WH | 1936 | Primary Fuel Level Sensor Signal
9-11 | -- | -- | Not Used | 9-11 | -- | -- | Not Used
12 | D-BU/WH | 1640 | Battery Positive Voltage | 12 | D-BU/WH | 1640 | Battery Positive Voltage
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | D-GN | 117 | Right Front Speaker Signal (-) | 14 | D-GN | 117 | Right Front Speaker Signal (-)
D-GN | 117 | Right Front Speaker Signal (-)
15 | L-GN | 200 | Right Front Speaker (+) | 15 | L-GN | 200 | Right Front Speaker (+)
L-GN | 200 | Right Front Speaker (+)
16-18 | -- | -- | Not Used | 16-18 | -- | -- | Not Used
19 | OG | 267 | Mirror Heater Element Voltage | 19 | OG | 267 | Mirror Heater Element Voltage
OG | 267 | Mirror Heater Element Voltage | OG | 267 | Mirror Heater Element Voltage
20 | BN | 241 | Ignition 3 Voltage | 20 | GY | 241 | Ignition 3 Voltage
21 | PK | 639 | Ignition 1 Voltage | 21 | PK | 639 | Ignition 1 Voltage
22-23 | -- | -- | Not Used | 22-23 | -- | -- | Not Used

### X216 Engine Harness to I/P Harness

#### Connector Part Information

- OEM: MG611810-41
- Service: N/A
- Description: 20-Way F WH

#### Connector Part Information

- OEM: MG652426
- Service: N/A
- Description: 20-Way M WH

#### X216 Engine Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN/BK | -- | Ambient Temp Signal | 1 | L-GN/BK | -- | Ambient Temp Signal
2 | GN/WH | -- | VSS Signal | 2 | GN/WH | -- | VSS Signal
3 | YE | -- | Diesel Particulate Indicator Control (Diesel) | 3 | YE | -- | Diesel Particulate Indicator Control (Diesel)
4 | L-BU/BK | -- | Cruise Switch Ground | 4 | WH/BK | -- | Cruise Switch Ground
5 | GY | -- | Cruise Switch Signal | 5 | GY | -- | Cruise Switch Signal
6 | YE/BK | -- | Glow Plug Indicator Control | 6 | L-BU | -- | Glow Plug Indicator Control
7 | BN/WH | -- | CAN High | 7 | BN/WH | -- | CAN High (LHD)
BN//BK | -- | CAN High (RHD)
BN/BK | -- | CAN High
8 | BN | -- | Oil Pressure Switch Signal | 8 | BN | -- | Oil Pressure Switch Signal
9 | WH | -- | Engine RPM Signal | 9 | WH | -- | Engine RPM Signal
10 | BN/WH | -- | WIF Indicator Control (Diesel) | 10 | BN/WH | -- | WIF Indicator Control (Diesel)
11 | PK | -- | Ignition Voltage | 11 | PK | -- | Ignition Voltage
12 | BN | -- | Charge Warning Indicator | 12 | BN | -- | Charge Warning Indicator
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | WH | -- | Cruise Indicator Control | 14 | WH | -- | Cruise Indicator Control
15 | OG/BK | -- | PNP Switch Control | 15 | PK/BK | -- | PNP Switch Control
15 | GN | -- | VSS Signal (M/T) | 15 | GN | -- | VSS Signal (M/T)
GN | -- | VSS Signal (M/T) (LHD Diesel)
16 | OG | -- | Fuel Consumption Signal | 16 | OG | -- | Fuel Consumption Signal
17 | WH/BK | -- | PTC Request | 17 | WH/BK | -- | PTC Request
18 | BN | -- | CAN Low | 18 | BN | -- | CAN Low
BN | -- | CAN Low
19 | L-BU | -- | Stop Lamp Switch Output | 19 | L-BU | -- | Stop Lamp Switch Output
20 | YE | -- | Sensor Ground | 20 | YE | -- | Sensor Ground

### X218 Engine Harness to Body Harness

#### Connector Part Information

- OEM: MG651068
- Service: N/A
- Description: 15-Way F WH

#### Connector Part Information

- OEM: MG641071
- Service: N/A
- Description: 15-Way M WH

#### X218 Engine Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN/BK | -- | Rough Road Signal | 1 | L-GN/BK | -- | Rough Road Signal
WH/BK | -- | Rough Road Signal (Diesel)
2 | PU | -- | Evap Canister SV Control (2.5L) | 2 | PU | -- | Evap Canister SV Control (2.5L)
3 | YE | -- | Clutch Switch Signal | 3 | YE | -- | Clutch Switch Signal
4 | GN | -- | 5V Reference | 4 | GN | -- | 5V Reference
5 | D-BU/WH | -- | Fuel Level Signal | 5 | D-BU/WH | -- | Fuel Level Signal
6 | WH/BK | -- | 5V Reference | 6 | WH/BK | -- | 5V Reference
7 | L-BU | -- | APP Sensor 2 Signal | 7 | L-BU | -- | APP Sensor 2 Signal
8 | GY | -- | 5V Reference (LHD) | 8 | GY/BK | -- | 5V Reference
L-BU | -- | 5V Reference (RHD)
9 | PU | -- | Low Reference | 9 | PU | -- | Low Reference
10 | PU | -- | Brake Engaged (BTSI) | 10 | PU | -- | Brake Engaged (BTSI)
11 | BU | -- | APP Sensor 1 Signal | 11 | BU | -- | APP Sensor 1 Signal
12 | BK | -- | Low Reference (2.5L) | 12 | BK | -- | Low Reference (2.5L)
13 | BN | -- | Low Reference | 13 | BN | -- | Low Reference
14 | PK/BK | -- | Ignition Voltage | 14 | PK/BK | -- | Ignition Voltage
15 | L-BU | -- | Stop Lamp Switch Output (2.0L, Diesel) | 15 | L-BU | -- | Stop Lamp Switch Output
D-GN | -- | Stop Lamp Switch Output (2.5L)

### X219 Subwoofer Speaker Harness to Body Harness

#### Connector Part Information

- OEM: 174932-1
- Service: N/A
- Description: 10-Way F WH

#### Connector Part Information

- OEM: 174931
- Service: N/A
- Description: 10-Way M WH

#### X219 Subwoofer Speaker Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | PK/BK | -- | Remote Subwoofer On | 5 | PK | -- | Remote Subwoofer On
6 | BK/WH | -- | Subwoofer Output (-) | 6 | BK | -- | Subwoofer Output (-)
7 | RD/WH | -- | Battery Positive Voltage | 7 | OG | -- | Battery Positive Voltage
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | PU/WH | -- | Subwoofer Ground | 9 | PU | -- | Subwoofer Ground
10 | D-GN | -- | Subwoofer Output (+) | 10 | D-GN | -- | Subwoofer Output (+)

### X220 Engine Harness to Body Harness (Diesel)

#### Connector Part Information

- OEM: MG612225
- Service: N/A
- Description: 4-Way F WH

#### Connector Part Information

- OEM: MG622226
- Service: N/A
- Description: 4-Way M WH

#### X220 Engine Harness to Body Harness (Diesel)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | -- | PTC 3 Relay Output | 1 | BN | -- | PTC 3 Relay Output
2 | YE/BK | -- | PTC 2 Relay Output | 2 | YE/BK | -- | PTC 2 Relay Output
3 | BU/WH | -- | PTC 1 Relay Output | 3 | BU/WH | -- | PTC 1 Relay Output
4 | -- | -- | Not Used | 4 | -- | -- | Not Used

### X301 Body Harness to Driver Seat Harness

#### Connector Part Information

- OEM: MG610047
- Service: N/A
- Description: 4-Way F GY

#### Connector Part Information

- OEM: MG620046
- Service: N/A
- Description: 4-Way M GY

#### X301 Body Harness to Driver Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | -- | Ground | 1 | BK | -- | Ground
2 | BK | -- | Ground | 2 | RD/WH | -- | Ground
3 | OG/BK | -- | Battery Positive Voltage | 3 | RD | -- | Battery Positive Voltage
4 | L-BU | -- | Heated Seat Switch Output | 4 | D-GN | -- | Heated Seat Switch Output

### X302 Body Harness to Passenger Seat Harness

#### Connector Part Information

- OEM: MG610047
- Service: N/A
- Description: 4-Way F GY

#### Connector Part Information

- OEM: MG620046
- Service: N/A
- Description: 4-Way M GY

#### X302 Body Harness to Passenger Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | BK | -- | Ground | 2 | BK | -- | Ground
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | D-BU/WH | -- | Heated Seat Switch Output | 4 | D-BU/WH | -- | Heated Seat Switch Output

### X303 SIR Harness to Body Harness

#### Connector Part Information

- OEM: MG612225
- Service: N/A
- Description: 4-Way F WH

#### Connector Part Information

- OEM: MG622226
- Service: N/A
- Description: 4-Way M WH

#### X303 SIR Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | WH/BK | -- | Right Inflatable Restraint Roof Rail Module - Low Signal | 1 | BN | -- | Right Inflatable Restraint Roof Rail Module - Low Signal
2 | YE/BK | -- | Right Inflatable Restraint Roof Rail Module - High Signal | 2 | YE/BK | -- | Right Inflatable Restraint Roof Rail Module - High Signal
3 | PK | -- | Left Inflatable Restraint Roof Rail Module - Low Signal | 3 | BU/WH | -- | Left Inflatable Restraint Roof Rail Module - Low Signal
4 | PU/WH | -- | Left Inflatable Restraint Roof Rail Module - High Signal | 4 | -- | -- | Left Inflatable Restraint Roof Rail Module - High Signal

### X351 Body Harness to Driver Door Harness

#### Connector Part Information

- OEM: MG611810-4
- Service: N/A
- Description: 18-Way F GY

#### Connector Part Information

- OEM: MG621807
- Service: N/A
- Description: 18-Way M GY

#### X351 Body Harness to Driver Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/BK | -- | Window Switch Drivers Express Down Signal | 1 | D-BU/WH | -- | Door Window Switch Drivers Express Down Signal
2 | OG | -- | Window Relay Output (Driver Safety) | 2 | OG | -- | Window Relay Output (Driver Safety)
2 | D-BU | -- | Window Switch Driver Up Signal | 2 | YE | -- | Window Switch Driver Up Signal
3 | GY | -- | Ignition Voltage | 3 | GY | -- | Ignition Voltage
4 | L-BU | -- | Door Lock Input Signal | 4 | L-BU | -- | Door Lock Input Signal
5 | GY | -- | Door Ajar Signal | 5 | GY | -- | Door Ajar Signal
6 | BN | -- | Window Master Switch Passenger Front Down Signal | 6 | BN | -- | Window Master Switch Passenger Front Down Signal
7 | WH | -- | Door Unlock Input Signal | 7 | WH | -- | Door Unlock Input Signal
8 | D-GN | -- | Window Master Switch Left Rear Up Signal | 8 | D-GN | -- | Window Master Switch Left Rear Up Signal
9 | L-GN | -- | Window Master Switch Right Rear Up Signal | 9 | L-GN | -- | Window Master Switch Right Rear Up Signal
10 | GY | -- | Left Front Speaker Output (-) | 10 | GY | -- | Left Front Speaker Output (-)
GY | -- | Left Front Speaker Output (-) (w/amp)
11 | BN/WH | -- | Window Switch Drivers Express Up Signal | 11 | BN/WH | -- | Window Switch Drivers Express Up Signal
12 | BN | -- | Window Switch Driver Down Signal | 12 | BN | -- | Window Switch Driver Down Signal
13 | L-BU | -- | Heated Seat Switch Output | 13 | L-BU | -- | Heated Seat Switch Output
14 | PU | -- | Window Master Switch Left Rear Down Signal | 14 | PU | -- | Window Master Switch Left Rear Down Signal
15 | PU/WH | -- | Window Master Switch Right Rear Down Signal | 15 | PU | -- | Window Master Switch Right Rear Down Signal
16 | BN | -- | Left Front Speaker Output (+) | 16 | BN | -- | Left Front Speaker Output (+)
BN | -- | Left Front Speaker Output (+) (w/amp)
17 | OG | -- | Window Switch Driver Express Down Signal | 17 | OG | -- | Window Switch Driver Express Down Signal
18 | L-BU | -- | Window Switch Passenger Up Signal | 18 | L-BU | -- | Window Switch Passenger Up Signal

### X352 Body Harness to Driver Door Harness

#### Connector Part Information

- OEM: MG611809
- Service: N/A
- Description: 18-Way F WH

#### Connector Part Information

- OEM: MG621807
- Service: N/A
- Description: 18-Way M GY

#### X352 Body Harness to Driver Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | -- | Door Unlock Signal | 1 | BN | -- | Door Unlock Signal
2 | BK | -- | Ground | 2 | BK | -- | Ground
3 | L-BU | -- | Folding Mirror Motor Retract Control | 3 | L-BU | -- | Folding Mirror Motor Retract Control
4 | YE | -- | Folding Mirror Motor Extend Control | 4 | YE | -- | Folding Mirror Motor Extend Control
5 | GY | -- | Door Lock Signal | 5 | GY | -- | Door Lock Signal
6 | PK/BK | -- | Window Master Switch Lockout Signal | 6 | PK/BK | -- | Window Master Switch Lockout Signal
7 | WH | -- | Courtesy Lamp Control | 7 | WH | -- | Courtesy Lamp Control
8 | L-BU | -- | OSRVM Control - Driver (LHD) (Passenger - RHD) | 8 | L-BU | -- | OSRVM Control - Driver (LHD) (Passenger - RHD)
9 | -- | -- | Not Used | 9 | -- | -- | Not Used
10 | D-BU/WH | -- | Driver Door Step Lamp Control | 10 | RD/WH | -- | Driver Door Step Lamp Control
11 | L-BU | -- | Driver Door Tamper Signal | 11 | L-BU | -- | Driver Door Tamper Signal
12 | RD/WH | -- | Battery Positive Voltage | 12 | RD | -- | Battery Positive Voltage (All others)
12 | RD/WH | -- | Battery Positive Voltage (RHD Diesel, EURO/GEN)
13 | BN | -- | Left Front Door Open Switch Signal | 13 | BN | -- | Left Front Door Open Switch Signal
14 | BN | -- | Trunk Contact Signal | 14 | BN | -- | Trunk Contact Signal
15 | GY | -- | Driver Mirror Common | 15 | BN | -- | Driver Mirror Common
16 | WH | -- | Driver Mirror Left/Right Control | 16 | WH | -- | Driver Mirror Left/Right Control
17 | YE | -- | Driver Mirror Up/Down Control | 17 | YE | -- | Driver Mirror Up/Down Control
18 | OG | -- | Window Relay Output | 18 | OG | -- | Window Relay Output

### X361 Body Harness to Passenger Door Harness

#### Connector Part Information

- OEM: MG611810-4
- Service: N/A
- Description: 18-Way F GY

#### Connector Part Information

- OEM: MG621807
- Service: N/A
- Description: 18-Way M GY

#### X361 Body Harness to Passenger Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK/BK | -- | Window Master Switch Lockout Signal | 1 | D-BU | -- | Window Master Switch Lockout Signal
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | GY | -- | Ignition Voltage | 3 | GY | -- | Ignition Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | L-GN | -- | Right Front Speaker Output (+) | 5 | L-GN/BK | -- | Right Front Speaker Output (+)
L-GN | -- | Right Front Speaker Output (+) (w/amp)
6 | D-GN | -- | Right Front Speaker Output (-) | 6 | D-GN | -- | Right Front Speaker Output (-)
D-GN | -- | Right Front Speaker Output (-) (w/amp)
7 | L-BU | -- | Window Master Switch Passenger Front Up Signal | 7 | L-BU | -- | Window Master Switch Right Front Up Signal
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BN | -- | Window Master Switch Passenger Front Down Signal | 9 | BN | -- | Window Master Switch Passenger Front Down Signal
10 | L-BU | -- | Passenger Door Tamper Signal | 10 | L-BU | -- | Passenger Door Tamper Signal
11 | D-BU/WH | -- | Heated Seat Switch Output | 11 | D-BU/WH | -- | Heated Seat Switch Output
12 | WH | -- | Courtesy Lamp Control | 12 | WH | -- | Courtesy Lamp Control
13-15 | -- | -- | Not Used | 13-15 | -- | -- | Not Used
16 | BK | -- | Ground | 16 | BK | -- | Ground
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | GY | -- | Door Ajar Signal - Passenger | 18 | GY | -- | Door Ajar Signal - Passenger

### X362 Body Harness to Passenger Door Harness

#### Connector Part Information

- OEM: MG611809
- Service: N/A
- Description: 18-Way F WH

#### Connector Part Information

- OEM: MG621807
- Service: N/A
- Description: 18-Way M GY

#### X362 Body Harness to Passenger Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | -- | Passenger Mirror Up/Down Control | 1 | BN | -- | Passenger Mirror Up/Down Control
2 | D-BU | -- | OSRVM Passenger Control (LHD) | 2 | D-BU | -- | OSRVM Passenger Control (LHD)
L-BU | -- | OSRVM Driver Control (RHD) | L-BU | -- | OSRVM Driver Control (RHD)
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | D-BU/WH | -- | Passenger Door Step Lamp Control | 4 | RD/WH | -- | Passenger Door Step Lamp Control
5 | D-GN | -- | Mirror Vertical Signal (w/Folding Mirror) | 5 | D-GN | -- | Mirror Vertical Signal (w/Power fold)
6 | BK | -- | Ground | 6 | BK | -- | Ground
D-BU | -- | Sensor Ground (w/Folding Mirror) | D-BU | -- | Sensor Ground (w/Folding Mirror)
7 | PU | -- | Passenger Mirror Left/Right Control | 7 | PU | -- | Passenger Mirror Left/Right Control
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | L-BU | -- | Folding Mirror Motor Control - Extend (w/Folding Mirror) | 9 | L-BU | -- | Folding Mirror Motor Retract Control
10 | GY | -- | Door Lock Signal | 10 | GY | -- | Door Lock Signal
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | D-GN/WH | -- | 5 Volt Reference (w/Folding Mirror) | 12 | D-GN/WH | -- | 5 Volt Reference (w/Folding Mirror)
13 | GY | -- | Passenger Mirror Common | 13 | GY | -- | Passenger Mirror Common
14 | L-BU | -- | Door Lock Input Signal | 14 | L-BU | -- | Door Lock Input Signal
15 | YE | -- | Folding Mirror Motor Control Retract (w/Folding Mirror) | 15 | YE | -- | Folding Mirror Motor Control Retract (w/Folding Mirror)
16 | BN | -- | Door Unlock Signal | 16 | BN | -- | Door Unlock Signal
17 | WH | -- | Door Unlock Input Signal | 17 | WH | -- | Door Unlock Input Signal
18 | RD | -- | Mirror Horizontal Signal (w/Folding Mirror) | 18 | RD | -- | Mirror Horizontal Signal (w/Folding Mirror)

### X371 Body Harness to Left Rear Door Harness

#### Connector Part Information

- OEM: MG610688
- Service: N/A
- Description: 21-Way F WH

#### Connector Part Information

- OEM: MG620689
- Service: N/A
- Description: 21-Way M WH

#### X371 Body Harness to Left Rear Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK/BK | -- | Window Master Switch Lockout Signal | 1 | PK/D-BU | -- | Window Master Switch Lockout Signal
2 | D-GN | -- | Window Master Switch Left Rear Up Signal | 2 | D-GN | -- | Window Master Switch Left Rear Up Signal
3 | PU | -- | Window Master Switch Left Rear Down Signal | 3 | PU | -- | Window Master Switch Left Rear Down Signal
4 | WH | -- | Courtesy Lamp Control | 4 | WH | -- | Courtesy Lamp Control
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BK | -- | Ground | 6 | BK | -- | Ground
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | WH | -- | Left Rear Speaker Output (+) | 8 | WH | -- | Left Rear Speaker Output (+)
WH | -- | Left Rear Speaker Output (+) (w/amp)
9 | YE | -- | Left Rear Speaker Output (-) | 9 | YE | -- | Left Rear Speaker Output (-)
YE | -- | Left Rear Speaker Output (-) (w/amp)
10-11 | -- | -- | Not Used | 10-11 | -- | -- | Not Used
12 | GY | -- | Courtesy Lamp Control | 12 | GY | -- | Courtesy Lamp Control
13-14 | -- | -- | Not Used | 13-14 | -- | -- | Not Used
15 | GY | -- | Door Lock Signal | 15 | GY | -- | Door Lock Signal
16-20 | -- | -- | Not Used | 16-20 | -- | -- | Not Used
21 | BN | -- | Door Signal | 21 | BN | -- | Door Signal

### X381 Body Harness to Right Rear Door Harness

#### Connector Part Information

- OEM: MG610688
- Service: N/A
- Description: 21-Way F WH

#### Connector Part Information

- OEM: MG620689
- Service: N/A
- Description: 21-Way M WH

#### X381 Body Harness to Right Rear Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK/BK | -- | Window Master Switch Lockout Signal | 1 | PK/D-BU | -- | Window Master Switch Lockout Signal
2 | L-GN | -- | Window Master Switch Right Rear Up Signal | 2 | D-GN | -- | Window Master Switch Right Rear Up Signal
3 | PU/WH | -- | Window Master Switch Right Rear Down Signal | 3 | PU | -- | Window Master Switch Right Rear Down Signal
4 | WH | -- | Courtesy Lamp Control | 4 | WH | -- | Courtesy Lamp Control
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BK | -- | Ground | 6 | BK | -- | Ground
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | D-BU | -- | Right Rear Speaker Output (+) | 8 | WH | -- | Right Rear Speaker Output (+)
D-BU | -- | Right Rear Speaker Output (+) (w/amp)
9 | L-BU | -- | Right Rear Speaker Output (-) | 9 | YE | -- | Right Rear Speaker Output (-)
L-BU | -- | Right Rear Speaker Output (-) (w/amp)
10-11 | -- | -- | Not Used | 10-11 | -- | -- | Not Used
12 | GY | -- | Courtesy Lamp Control | 12 | GY | -- | Courtesy Lamp Control
13-14 | -- | -- | Not Used | 13-14 | -- | -- | Not Used
15 | GY | -- | Door Lock Signal | 15 | GY | -- | Door Lock Signal
16-20 | -- | -- | Not Used | 16-20 | -- | -- | Not Used
21 | BN | -- | Door Signal | 21 | BN | -- | Door Signal

### X401 Trunk Room Harness to Body Harness

-- | --

#### Connector Part Information

- OEM: HS015-16015
- Service: N/A
- Description: 16-Way F CS Series

#### Connector Part Information

- OEM: HS011-16016
- Service: N/A
- Description: 16-Way M CS Series

#### X401 Trunk Room Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | BN/WH | 309 | Right Park Lamp Supply Voltage
2 | L-GN | 24 | Backup Lamp Supply Voltage (UD7) | 2 | L-GN | 24 | Backup Lamp Supply Voltage (UD7)
3 | OG | 122 | Rear Fog Lamp Supply Voltage (T98) | 3 | OG | 122 | Rear Fog Lamp Supply Voltage
4 | GY | 2555 | Rear Park Assist Disable Signal (UD7) | 4 | GY | 2555 | Rear Park Assist Disable Signal (UD7)
5 | L-BU | 1134 | Park Brake Switch Signal (UD7) | 5 | BN | 133 | Park Brake Switch Signal (UD7)
6 | L-BU/WH | 20 | Stop Lamp Supply Voltage | 6 | L-BU/WH | 20 | Stop Lamp Supply Voltage
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | PU | 709 | Left Park Lamp Supply Voltage | 8 | PU | 709 | Left Park Lamp Supply Voltage
9 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 9 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
10 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 10 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | PK | 839 | Ignition 1 Voltage (UD7) | 12 | PK | 839 | Ignition 1 Voltage (UD7)
13 | D-BU | 903 | Object Detection Alarm 8V Reference (UD7) | 13 | D-BU | 903 | Object Detection Alarm 8V Reference (UD7)
14 | YE | 5247 | Park Assist Alarm Signal (UD7) | 14 | YE | 5247 | Park Assist Alarm Signal (UD7)
15 | GY | 5248 | Park Assist Alarm Low Reference (UD7) | 15 | GY | 5248 | Park Assist Alarm Low Reference (UD7)
16 | -- | -- | Not Used | 16 | -- | -- | Not Used

### X402 Trunk Lid Harness to Body Harness

#### Connector Part Information

- OEM: HS015-06015
- Service: N/A
- Description: 6-Way F 090(CS) Series (WH)

#### Connector Part Information

- OEM: HS011-06016
- Service: N/A
- Description: 6-Way M 090(CS) Series (WH)

#### X402 Trunk Lid Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | OG/BK | -- | Rear Compartment Signal | 1 | OG/BK | -- | Rear Compartment Signal
2 | L-BU | -- | Trunk Latch Actuator Control | 2 | BN | -- | Trunk Latch Actuator Control
3 | PU | -- | Illumination | 3 | PU | -- | Illumination
4 | BK | -- | Ground | 4 | BK | -- | Ground
5 | L-GN | -- | Backup Lamps Control | 5 | L-GN | -- | Backup Lamps Control
6 | OG/BK | -- | Trunk Tamper Signal | 6 | L-BU | -- | Trunk Tamper Signal

### X403 Trunk Room Harness to Rear Bumper Harness (T98/UD7)

#### Connector Part Information

- OEM: MG610339
- Service: N/A
- Description: 8-Way F 070 SWP Series (NA)

#### Connector Part Information

- OEM: MG640341
- Service: N/A
- Description: 8-Way M SWP Series (BK)

#### X403 Trunk Room Harness to Rear Bumper Harness (T98/UD7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | OG | -- | Rear Fog Lamp Control (T98) | 1 | OG | -- | Rear Fog Lamp Control (T98)
2 | GY | -- | RC Sensor Signal | 2 | GY | -- | RC Sensor Signal
3 | OG/BK | -- | RM Sensor Signal | 3 | OG/BK | -- | RM Sensor Signal
4 | BU | -- | LM Sensor Signal | 4 | BU | -- | LM Sensor Signal
5 | BK | -- | Ground (T98) | 5 | BK | -- | Ground (T98)
6 | BN/WH | -- | Left Sensor Ground | 6 | BN/WH | -- | Left Sensor Ground
7 | BN | -- | Right Sensor Ground | 7 | BN | -- | Right Sensor Ground
8 | YE | -- | LC Sensor Signal | 8 | GY | -- | LC Sensor Signal

### X404 Body Harness to Fuel Pump Harness

#### Connector Part Information

- OEM: MG651110
- Service: N/A
- Description: 14-Way F WH

#### Connector Part Information

- OEM: MG641113
- Service: N/A
- Description: 14-Way M WH

#### X404 Body Harness to Fuel Pump Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | -- | Low Fuel Signal | 1 | YE | -- | Low Fuel Signal
2 | PU | -- | EVAP Canister SV Control | 2 | PU | -- | EVAP Canister SV Control
3 | GY | -- | Fuel Pump Relay Output | 3 | GY | -- | Fuel Pump Relay Output
4 | D-BU/WH | -- | Fuel Level Signal | 4 | D-BU | -- | Fuel Level Signal
5 | PU | -- | Ground | 5 | PU | -- | Ground (2.0L)
BN | -- | Ground (2.5L)
BK | -- | Ground (Diesel)
6 | PK | -- | Fuel Level Reference Voltage | 6 | PK | -- | Fuel Level Reference Voltage
7 | GY/BK | -- | 5V Reference | 7 | GY/BK | -- | 5V Reference
8 | PK/BK | -- | Ignition Voltage | 8 | PK/BK | -- | Ignition Voltage
9 | BK | -- | Ground | 9 | BK | -- | Ground
10 | BK | -- | Low Reference | 10 | BK | -- | Low Reference
11 | D-GN | -- | FTP Sensor Signal | 11 | D-GN | -- | FTP Sensor Signal
12 | -- | -- | Not Used | 12 | -- | -- | Not Used
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | -- | -- | Not Used | 14 | -- | -- | Not Used