For 1990-2009 cars

Connector 1: | Heated Seat - Driver
Connector 2: | Heated Seat - Passenger
Connector 3: | Heated Seat Switch - Driver
Connector 4: | Heated Seat Switch - Passenger

### Heated Seat - Driver

#### Connector Part Information

- OEM: KET MG 610263
- Service: N/A
- Description:

#### Heated Seat - Driver

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | RD/WH | -- | Ground
2 | D-GN | -- | Heated Seat Supply Voltage

### Heated Seat - Passenger

#### Connector Part Information

- OEM: KET MG 610263
- Service: N/A
- Description:

#### Heated Seat - Passenger

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Heated Seat Supply Voltage
2 | BK | -- | Ground

### Heated Seat Switch - Driver

#### Connector Part Information

- OEM: KET MG 651044-2
- Service: N/A
- Description: BU

#### Heated Seat Switch - Driver

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN | -- | Accessory Voltage
BN | -- | Accessory Voltage
2 | BK | -- | Ground
3 | BK (LHD) | -- | Ground
-- (RHD) | -- | Not Used
4 | L-BU (LHD) | -- | Heated Seat Supply Voltage
BN (RHD) | -- | Accessory Voltage
5 | BN (LHD) | -- | Accessory Voltage
L-BU (RHD) | -- | Heated Seat Supply Voltage
6 | -- (LHD) | -- | Not Used
BK (RHD) | -- | Ground

### Heated Seat Switch - Passenger

#### Connector Part Information

- OEM: KET MG 651044
- Service: N/A
- Description: WH

#### Heated Seat Switch - Passenger

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | GY | -- | Accessory Voltage
2 | BK | -- | Ground
3 | -- (LHD) | -- | Not Used
BK (RHD) | -- | Ground
4 | GY (LHD) | -- | Accessory Voltage
GY (LHD) | -- | Accessory Voltage
D-BU/WH (RHD) | -- | Heated Seat Supply Voltage
5 | D-BU/WH (LHD) | -- | Heated Seat Supply Voltage
GY (RHD) | -- | Accessory Voltage
GY (RHD) | -- | Accessory Voltage
6 | BK (LHD) | -- | Ground
-- (RHD) | -- | Not Used