For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Caulking Nut | 280 N·m | 207 lb ft
Centermember Bolts | 90 N·m | 66 lb ft
Centermember Front Damping Block Bolt | 80 N·m | 59 lb ft
Centermember Rear Damping Block Bolt | 80 N·m | 59 lb ft
Control Arm Bolt | 180 N·m | 133 lb ft
Control Arm Bracket Bolt | 90 N·m | 66 lb ft
Control Arm Joint Bolt | 110 N·m | 81 lb ft
Crossmember Bolts to Control Arm | 150 N·m | 110 lb ft
Crossmember Nuts to Longitudinal | 150 N·m | 110 lb ft
Front Hub Bolts | 95 N·m | 70 lb ft
Front Strut Bracket Bolts | 140 N·m | 103 lb ft
Front Strut Piston Rod Nut | 80 N·m | 59 lb ft
Front Strut Upper Nuts | 50 N·m | 37 lb ft
Impact Beam Bolt | 100 N·m | 74 lb ft
Power Steering Pipe Union Nuts to Gear Set | 30 N·m | 22 lb ft
Power Steering Return Pipe Fixing Bolt | 7 N·m | 62 lb in
Stabilizer Bar Bolt/Nuts | 50 N·m | 37 lb ft
Stabilizer Link Nuts | 50 N·m | 37 lb ft
Steering Intermediate Shaft Bolt | 25 N·m | 18 lb ft