For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Automatic Transaxle - Gasoline Engine | 7.14 ± 0.15L | 7.5 ± 0.15 qt
Automatic Transaxle - Diesel Engine | 6.94 ± 0.15L | 7.33 ± 0.15 qt
Brake Fluid and Clutch Fluid | 0.5L | 0.53 qt
Engine Coolant | 8.0L | 8.4 qt
Engine Oil - 2.0L, 2.5L Gasoline Engines | 6.4L | 6.7 qt
Engine Oil - 2.0L Diesel Engine | 6.2L | 6.6 qt
Manual Transaxle - Gasoline Engine | 1.6L | 1.78 qt
Manual Transaxle - Diesel Engine | 2.1L | 2.2 qt
Power Steering System Fluid | 1.1L | 1.2 qt