For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Parallel Link Bolt-to-Knuckle | 110 N·m | 81 lb ft
Front Parallel Link Cam Bolt-to-Crossmember | 80 N·m | 59 lb ft
Rear Brake Caliper Bolt-to-Knuckle | 45 N·m | 33 lb ft
Rear Brake Disc Screw | 4 N·m | 35 lb in
Rear Crossmember Nut/Bolt | 110 N·m | 81 lb ft
Rear Hub Nut-to-Rear Knuckle | 65 N·m | 48 lb ft
Rear Parallel Link Bolt-to-Crossmember | 110 N·m | 81 lb ft
Rear Parallel Link Bolt-to-Knuckle | 110 N·m | 81 lb ft
Rear Stabilizer Bar Bolt | 50 N·m | 37 lb ft
Rear Stabilizer Link Nut | 50 N·m | 37 lb ft
Rear Strut Lower Nut | 90 N·m | 66 lb ft
Rear Strut Upper Nut | 50 N·m | 37 lb ft
Trailing Link Bolt-to-Knuckle | 120 N·m | 89 lb ft
Trailing Link Bracket Bolt | 90 N·m | 66 lb ft
Upper Arm Nut-to-Body | 60 N·m | 44 lb ft
Upper Arm Nut-to-Rear Knuckle | 110 N·m | 81 lb ft