For 1990-2009 cars

### Roof

The roof is a one-piece painted metal unit which incorporates a single, solid headliner and 2 moldings with one on each side of the vehicle roof.

The moldings, which enclose and hide the roof rail seams, are serviceable as individual units.

The one-piece formed headliner, common to both the notchback and the hatchback, consists of a molded substrate covered with a foam-backed cloth facing. The one-piece construction requires servicing the headliner as a complete assembly.

### Power Sunroof

The sunroof is built into the roof and is made of glass. It is intended to provide light and air through the roof of the vehicle. The sunroof is powered by an electric motor and controlled by a toggle switch built into the interior courtesy lamp assembly. The sunroof is also equipped with a sunshade that opens and closes manually.

### Power Sunroof Control Switch

The power sunroof control switch is a toggle button located on the right side of the interior courtesy lamp/power sunroof control switch assembly.

#### Operating the Power Sunroof

The ignition must be ON in order to operate the power sunroof.

#### Tilting the Power Sunroof Open and Closed

To tilt open the rear end of the power sunroof, press and hold the forward portion of the toggle button until the power sunroof tilts open. To close the power sunroof from a tilted open position, press and hold the rear portion of the toggle button until the sunroof tilts closed.

#### Sliding the Power Sunroof Open and Closed

To slide open the power sunroof, press the rear portion of the toggle button until the sunroof slides. If the sunshade is closed, the power sunroof will pull the sunshade open as the sunroof slides open. To close the power sunroof from a slid-open position, press the forward portion of the toggle button until the sunroof slides closed.

### Sun Visors

The sun visors swing down in order to block out glare. They also swing to the side when they are released from the support. Each sun visor has a vanity mirror and lamp for diagnosis refer to Lighting.

### Passenger Assist Handles

There is a passenger assist handle for the right, rear out-board seat and for the front passenger seat. Passengers can use the handles to assist in keeping their balance over rough roads or during sharp turns.

### Coat Hook

The coat hooks are located on the left and right rear passenger assist handles.