For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section.
1 | NEW Fluid Pump Seal Assembly
2 | NEW Fluid Pump Seal Assembly
3 | NEW Centre Support Fluid Passage Seal Assembly
4 | Control Valve Body Assembly Tip Align the manual shift shaft position switch activator slide with the detent lever guide pin.
5 | Bolts M5 x 73 (Quantity: 6) Tighten 8 N·m (71 lb. in) in the sequence shown.