For 1990-2009 cars

#### No Overrun Braking - Manual 3-2-1

Checks | Causes
--- | ---
External Linkage | Not adjusted properly
Valve Body Assembly (60) |

• | 4-3 Sequence valve stuck

• | Checkball mispositioned

• | Spacer plate and gaskets incorrect, damaged or mispositioned

Overrun and Forward Clutch Assembly (644-651) |

• | Turbine shaft oil passages plugged or not drilled

• | Turbine shaft seal rings damaged

• | Turbine shaft sealing balls loose or missing

• | Porosity in forward or overrun clutch piston

• | Overrun piston seals cut or damaged

• | Overrun piston checkball not sealing