For 1990-2009 cars

#### Tools Required

KM6067 Radio Removal Tool

### Removal Procedure

1. Remove the navigation module. Refer to Navigation Module Replacement.
2. Remove the navigation module assembly retaining screws (1).
3. Remove the navigation module carrier from the I/P compartment.

### Installation Procedure

1. Install the navigation module carrier into the I/P compartment.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the navigation module assembly retaining screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the navigation module. Refer to Navigation Module Replacement.