For 1990-2009 cars

## Bulb Usage Chart Except HSV Maloo

Bulb | Power Rating (Watts) | Type
--- | --- | ---
Backup Lamp Bulb | 21 | Bayonet
Console Lamp Bulb | 5 | Festoon
Cabin Storage Area Lamp Bulb | 5 | Festoon
Dome Lamp Bulb | 5 | Wedge
Door Courtesy Lamp Bulb | 10 | Festoon
Front Fog Lamp Bulb | 55 | H 11
Front Indicator Bulb | 21 | Bayonet
High Beam Headlamp Bulb | 65 | H9
High Mounted Stop Lamp | LED | LED
Ignition Lock Cylinder Lamp Bulb | 1.4 | Bayonet
Instrument Panel Compartment Lamp Bulb | 5 | Festoon
Instrument Panel Courtesy Lamp Bulb - Left | 2.7 | Wedge
Instrument Panel Courtesy Lamp Bulb - Right | 2.7 | Wedge
License Lamp Bulb | 5 | Wedge
Low Beam Headlamp Bulb | 55 | H7
Park Bulb (Front) | 5 | Wedge
Rear Indicator Lamp Bulb | 21 | Bayonet
Side Indicator (Repeater) Lamp Bulb | 5 | Wedge
Stop/Tail Lamp Bulb | 5 | Bayonet
Transmission Floor Shift Control Indicator Lamp Bulb | LED | Wedge
Light Emitting Diode = LED

## Bulb Usage Chart HSV Maloo

Bulb | Power Rating (Watts) | Type
--- | --- | ---
Backup Lamp Bulb | 21 | Bayonet
Front Fog Lamp Bulb (Type A) | 55 | H 11
Front Fog Lamp Bulb (Type B) | 55 | H 3
Front Fog Lamp Bulb (Type C) | 55 | H 3
Driving Lamp Bulb | 55 | H 3
Rear Indicator Lamp Bulb (Type A) | 21 | Bayonet
Rear Indicator Lamp Bulb (Type B) | LED | LED
Side Indicator (Repeater) Lamp Bulb | 5 | Wedge
Stop/Tail Lamp Bulb (Type A) | 21/5 | Bayonet
Stop/Tail Lamp Bulb (Type B) | LED | LED
LED = Light Emitting Diode