For 1990-2009 cars

### Removal Procedure

1. Remove the trim plate panel. Refer to Console Trim Plate Replacement.
2. Remove the transmission floor shift control indicator lamp from the rear of the shift control housing by turning the lamp socket (1) counter clockwise.
3. Pull the transmission floor shift control indicator light bulb from the socket.

### Installation Procedure

1. Install a new transmission floor shift control indicator light bulb to the socket (1).
2. Install the transmission floor shift control indicator lamp to the rear of the shift control housing by turning the lamp socket clockwise.
3. Install the trim plate panel. Refer to Console Trim Plate Replacement.
4. Check the operation of the transmission floor shift control indicator light.