For 1990-2009 cars

1. Remove the power steering pump to mounting bracket retaining bolts (3).
2. Remove the power steering pump (2) from the power steering pump mounting bracket (1).
3. Remove the power steering reservoir bracket to cylinder head retaining bolt (1).
4. Remove the power steering reservoir bracket to engine front cover retaining bolt (2).
5. Remove the power steering reservoir bracket (3).
6. Remove the power steering pump bracket to cylinder head retaining bolts (4).
7. Remove the power steering pump bracket (5).