For 1990-2009 cars

## Fastener Tightening Specifications LWB SWB

Application | Specification
--- | ---
Metric | English
Bracket to I/P Centre Support Retaining Screws | 2 N·m | 18 lb in
Centre Console to End Panel Retaining Screws | 2 N·m | 18 lb in
Centre Console to Floor Retaining Bolt | 25 N·m | 18 lb ft
Centre Console to Front Floor Retaining Screws | 2 N·m | 18 lb in
Centre Console to Park Brake Assembly Retaining Bolts | 25 N·m | 18 lb ft
Coin Holder to Centre Console Retaining Screw | 2 N·m | 18 lb in
Compartment Damper to I/P Retaining Screws | 2 N·m | 18 lb in
Compartment to I/P Retaining Screws | 2 N·m | 18 lb in
Cup Holder to Centre Console Retaining Screws | 2 N·m | 18 lb in
Instrument Cluster Retaining Screws | 2 N·m | 18 lb in
Instrument Cluster Trim Assembly Screws | 2 N·m | 18 lb in
I/P Datum Pin Retaining Screws | 2 N·m | 18 lb in
I/P to Trim Pad Retaining Screws | 2 N·m | 18 lb in
Left Hand Tweeter to I/P Retaining Screws | 2 N·m | 18 lb in
Passenger Side Air Bag Module to I/P Trim Pad Retaining Nuts | 16 N·m | 12 lb ft
Storage Compartment to I/P Retaining Screws | 2 N·m | 18 lb in
Top Trim Panel to I/P Retaining Screws | 2 N·m | 18 lb in
Trim Pad - Instrument Panel (I/P) Upper Retaining Screws | 2 N·m | 18 lb in
Trim Panel to Centre Console Retaining Screws | 2 N·m | 18 lb in
Trim Panel to I/P Upper Retaining Screws | 2 N·m | 18 lb in