For 1990-2009 cars

## Fastener Tightening Specifications HSV Maloo

Application | Specification
--- | ---
Metric | English
Type B Specifications |  |
Brake Caliper Bleeder Valve Dry Torque | 17 +/-3 Nm | 12.5 lb ft
Brake Hose to Caliper (Type B) Banjo Bolt Dry Torque | 33 +/-3 Nm | 24 lb ft
Front Brake Caliper (Type B) to Knuckle Retaining Bolt | 130 Nm | 96 lb ft
Rear Brake Caliper (Type B) to Knuckle Retaining Bolt | 110 Nm | 81 lb ft

## Fastener Tightening Specifications Except HSV Maloo

Application | Specification
--- | ---
Metric | English
Brake Caliper Bleeder Valve Dry Torque | 12 Nm | 106 lb in
Brake Hose to Caliper Banjo Bolt Dry Torque | 35 Nm | 26 lb ft
Front Brake Caliper Anchor Plate to Knuckle Retaining Bolt | 60 Nm +120° | 44 lb ft +120°
Front Brake Caliper Pin Retaining Bolt | 42 Nm | 31 lb ft
Front Brake Disc Splash Shield to Steering Knuckle Retaining Bolt | 9 Nm | 71 lb in
Rear Disc Brake Backing Plate to Knuckle Retaining Bolt - Upper | 60 Nm | 44 lb ft
Rear Disc Brake Backing Plate to Knuckle Retaining Bolts - Lower | 130 Nm | 96 lb ft
Rear Brake Caliper to Knuckle Retaining Bolt | 110 Nm | 81 lb ft
Rear Brake Caliper Pin Retaining Bolt | 42 Nm | 31 lb ft