For 1990-2009 cars

Table 1: | Accelerator Pedal Position (APP) Sensor (LY7/L98)
Table 2: | Accelerator Pedal Position (APP) Sensor (LS2) (HSV Maloo)
Table 3: | A/C Refrigerant Pressure Sensor (L98)
Table 4: | A/C Refrigerant Pressure Sensor (LS2) (HSV Maloo)
Table 5: | A/C Refrigerant Pressure Sensor (LY7)
Table 6: | Air Mix Actuator
Table 7: | Ambient Light Sensor
Table 8: | Automatic Transmission Shift Lever
Table 9: | Automatic Transmission (4L60/4L65)
Table 10: | Automatic Transmission (6L80E)
Table 11: | Auxiliary Power Outlet - Console
Table 12: | Backup Lamp Switch (L98)
Table 13: | Backup Lamp Switch (LS2) (HSV Maloo)
Table 14: | Backup Lamp Switch (LY7)
Table 15: | Battery Current Sensor
Table 16: | Battery Negative
Table 17: | Battery Positive
Table 18: | Battery Remote Positive Terminal (L98)
Table 19: | Blower Motor (RHD)
Table 20: | Bluetooth Connector
Table 21: | Bluetooth Microphone
Table 22: | Bluetooth Module
Table 23: | Body Control Module (BCM) -X1
Table 24: | Body Control Module (BCM) -X2
Table 25: | Body Control Module (BCM) -X3
Table 26: | Body Control Module (BCM) -X4
Table 27: | Body Control Module (BCM) -X5
Table 28: | Body Control Module (BCM) -X6
Table 29: | Body Control Module (BCM) - X7
Table 30: | Brake Fluid Level Switch
Table 31: | Brake Pedal Position (BPP) Sensor
Table 32: | Camshaft Position (CMP) Exhaust Sensor - 1 (LY7)
Table 33: | Camshaft Position (CMP) Exhaust Sensor - 2 (LY7)
Table 34: | Camshaft Position (CMP) Exhaust Solenoid - 1 (LY7)
Table 35: | Camshaft Position (CMP) Exhaust Solenoid - 2 (LY7)
Table 36: | Camshaft Position (CMP) Intake Sensor - 1 (LY7)
Table 37: | Camshaft Position (CMP) Intake Sensor - 2 (LY7)
Table 38: | Camshaft Position (CMP) Intake Solenoid - 1
Table 39: | Camshaft Position (CMP) Intake Solenoid - 2
Table 40: | Camshaft Position (CMP) Sensor (L98)
Table 41: | Camshaft Position (CMP) Sensor (LS2) (HSV Maloo)
Table 42: | Center High Mounted Stop Lamp
Table 43: | Cigar Lighter-Front Console
Table 44: | Clutch Cruise Switch
Table 45: | Clutch Safety Switch
Table 46: | Clutch Start Switch V6
Table 47: | Clutch Start Switch V8
Table 48: | Crankshaft Position (CKP) Sensor
Table 49: | Crankshaft Position (CKP) Sensor (L98)
Table 50: | Crankshaft Position (CKP) Sensor (LS2) (HSV Maloo)
Table 51: | Cruise Control Switch (Part of the Turn Signal Multifunction Switch)
Table 52: | Data Link Connector (DLC)
Table 53: | Dome Lamp
Table 54: | Door Latch Assembly - LF
Table 55: | Door Latch Assembly - RF
Table 56: | Driving Lamp - Left (HSV Maloo)
Table 57: | Driving Lamp - Right (HSV Maloo)
Table 58: | Driving Lamp - HSVDR-1 (HSV Maloo)
Table 59: | Electronic Brake Control Module (EBCM) - (JL4)
Table 60: | Electronic Control Valve Displacement (ECVD)
Table 61: | Engine Control Module - X1 (L98)
Table 62: | Engine Control Module - X1 (LS2) (HSV Maloo)
Table 63: | Engine Control Module - X1(LY7)
Table 64: | Engine Control Module - X2 (L98)
Table 65: | Engine Control Module - X2 (LS2) (HSV Maloo)
Table 66: | Engine Control Module - X2 (LY7)
Table 67: | Engine Coolant Temperature (ECT) Sensor (L98)
Table 68: | Engine Coolant Temperature (ECT) Sensor (LS2) (HSV Maloo)
Table 69: | Engine Coolant Temperature (ECT) Sensor (LY7)
Table 70: | Engine Cooling Fan - Left
Table 71: | Engine Cooling Fan - Right
Table 72: | Engine Oil Level/Temperature Sensor (L98)
Table 73: | Engine Oil Level/Temperature Sensor (LS2) (HSV Maloo)
Table 74: | Engine Oil Level/Temperature Sensor (LY7)
Table 75: | Engine Oil Pressure (EOP) Sensor (L98)
Table 76: | Engine Oil Pressure (EOP) Sensor (LS2) (HSV Maloo)
Table 77: | Engine Oil Pressure (EOP) Sensor (LY7)
Table 78: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (L98)
Table 79: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LS2) (HSV Maloo)
Table 80: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LY7)
Table 81: | Express Down Window Module
Table 82: | Fog Lamp - Left
Table 83: | Fog Lamp - Right
Table 84: | Fuel Filler Door Latch
Table 85: | Fuel Injector - 1 (L98)
Table 86: | Fuel Injector - 1 (LS2) (HSV Maloo)
Table 87: | Fuel Injector - 1 (LY7)
Table 88: | Fuel Injector - 2 (L98)
Table 89: | Fuel Injector - 2 (LS2) (HSV Maloo)
Table 90: | Fuel Injector - 2 (LY7)
Table 91: | Fuel Injector - 3 (L98)
Table 92: | Fuel Injector - 3 (LS2) (HSV Maloo)
Table 93: | Fuel Injector - 3 (LY7)
Table 94: | Fuel Injector - 4 (L98)
Table 95: | Fuel Injector - 4 (LS2) (HSV Maloo)
Table 96: | Fuel Injector - 4 (LY7)
Table 97: | Fuel Injector - 5 (L98)
Table 98: | Fuel Injector - 5 (LS2) (HSV Maloo)
Table 99: | Fuel Injector - 5 (LY7)
Table 100: | Fuel Injector - 6 (L98)
Table 101: | Fuel Injector - 6 (LS2) (HSV Maloo)
Table 102: | Fuel Injector - 6 (LY7)
Table 103: | Fuel Injector - 7 (L98)
Table 104: | Fuel Injector - 7 (LS2) (HSV Maloo)
Table 105: | Fuel Injector - 8 (L98)
Table 106: | Fuel Injector - 8 (LS2) (HSV Maloo)
Table 107: | Fuel Level Sensor - Secondary
Table 108: | Fuel Level Sensor - Secondary (HSV Maloo)
Table 109: | Fuel Pump and Sender Assembly
Table 110: | Fuse Block - Instrument Panel
Table 111: | Fuse Block - Underhood - X1 (134)
Table 112: | Fuse Block - Underhood - X2 (132)
Table 113: | Fuse Block - Underhood - X3 (130)
Table 114: | Generator
Table 115: | Headlamp and Dimmer Panel Switch
Table 116: | Headlamp Assembly - Left
Table 117: | Headlamp Assembly - Right
Table 118: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (L98)
Table 119: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LS2) (HSV Maloo)
Table 120: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LY7)
Table 121: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (L98)
Table 122: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LS2) (HSV Maloo)
Table 123: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LY7)
Table 124: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (L98)
Table 125: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LS2) (HSV Maloo)
Table 126: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LY7)
Table 127: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (L98)
Table 128: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LS2) (HSV Maloo)
Table 129: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LY7)
Table 130: | Hood Ajar Switch
Table 131: | Horn - Left X1
Table 132: | Horn - Left X2
Table 133: | Horn - Right X1
Table 134: | Horn - Right X2
Table 135: | HVAC Control Module - X1
Table 136: | HVAC Control Module - X2
Table 137: | HVAC Control Module - X3-C1
Table 138: | Ignition Coil - 1 (L98)
Table 139: | Ignition Coil - 1 (LS2) (HSV Maloo)
Table 140: | Ignition Coil - 1 (LY7)
Table 141: | Ignition Coil - 2 (L98)
Table 142: | Ignition Coil - 2 (LS2) (HSV Maloo)
Table 143: | Ignition Coil - 2 (LY7)
Table 144: | Ignition Coil - 3 (L98)
Table 145: | Ignition Coil - 3 (LS2) (HSV Maloo)
Table 146: | Ignition Coil - 3 (LY7)
Table 147: | Ignition Coil - 4 (L98)
Table 148: | Ignition Coil - 4 (LS2) (HSV Maloo)
Table 149: | Ignition Coil - 4 (LY7)
Table 150: | Ignition Coil - 5 (L98)
Table 151: | Ignition Coil - 5 (LS2) (HSV Maloo)
Table 152: | Ignition Coil - 5 (LY7)
Table 153: | Ignition Coil - 6 (L98)
Table 154: | Ignition Coil - 6 (LS2) (HSV Maloo)
Table 155: | Ignition Coil - 6 (LY7)
Table 156: | Ignition Coil - 7 (L98)
Table 157: | Ignition Coil - 7 (LS2) (HSV Maloo)
Table 158: | Ignition Coil - 8 (L98)
Table 159: | Ignition Coil - 8 (LS2) (HSV Maloo)
Table 160: | Ignition Key Cylinder Lamp
Table 161: | Ignition Switch
Table 162: | Inflatable Restraint Front Sensor - RF
Table 163: | Inflatable Restraint Front Sensor - LF
Table 164: | Inflatable Restraint I/P Module - X1
Table 165: | Inflatable Restraint I/P Module - X2
Table 166: | Inflatable Restraint Seat Position Sensor (SPS) - Driver
Table 167: | Inflatable Restraint Sensing and Diagnostic Module - X1
Table 168: | Inflatable Restraint Sensing and Diagnostic Module - X2
Table 169: | Inflatable Restraint Steering Wheel Module - X1
Table 170: | Inflatable Restraint Steering Wheel Module - X2
Table 171: | Inflatable Restraint Steering Wheel Module Coil - X1
Table 172: | Inflatable Restraint Steering Wheel Module Coil - X1
Table 173: | Inflatable Restraint Steering Wheel Module Coil - X2
Table 174: | Inflatable Restraint Steering Wheel Module Coil - X2
Table 175: | Instrument Panel Cluster (IPC)
Table 176: | Instrument Panel Data Link Connector
Table 177: | I/P Compartment Lamp - X1
Table 178: | I/P Compartment Lamp - X2
Table 179: | I/P Compartment Lamp Switch - X1
Table 180: | I/P Compartment Lamp Switch - X2
Table 181: | Knock Sensor (KS) Bank 1 (LY7)
Table 182: | Knock Sensor (KS) Bank 2 (LY7)
Table 183: | Knock Sensor (KS) Left (L98)
Table 184: | Knock Sensor (KS) Left (LS2) (HSV Maloo)
Table 185: | Knock Sensor (KS) Right (L98)
Table 186: | Knock Sensor (KS) Right (LS2) (HSV Maloo)
Table 187: | License Lamp - Unit
Table 188: | Load Compartment Light (HSV Maloo)
Table 189: | Manifold Absolute Pressure (MAP) Sensor (L98)
Table 190: | Manifold Absolute Pressure (MAP) Sensor (LS2) (HSV Maloo)
Table 191: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LY7/L98)
Table 192: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LY7/LS2) (HSV Maloo)
Table 193: | Mode Actuator - 1
Table 194: | Mode Actuator - 2
Table 195: | Navigation Gateway Module
Table 196: | Navigation Unit - X1
Table 197: | Navigation Module - X2
Table 198: | Navigation Module - X3
Table 199: | Navigation Module - X4
Table 200: | Navigation Module - X5
Table 201: | Navigation Module - X6
Table 202: | Navigation Module - X7
Table 203: | Object Alarm Sensor - LR Corner (HSV Maloo)
Table 204: | Object Alarm Sensor - LR Middle (HSV Maloo)
Table 205: | Object Alarm Sensor - RR Corner (HSV Maloo)
Table 206: | Object Alarm Sensor - RR Middle (HSV Maloo)
Table 207: | Oil Pressure Gauge (HSV Maloo)
Table 208: | Oil Temperature Gauge (HSV Maloo)
Table 209: | Outside Rear View Mirror - Left
Table 210: | Outside Rear View Mirror - Right
Table 211: | Park Brake Switch
Table 212: | Park/Neutral Position (PNP) Switch (4L60E)
Table 213: | Radio - X1 (Type A, B, C and D Infotainment System)
Table 214: | Radio - X2
Table 215: | Radio - X4
Table 216: | Radio - X5 AM/FM Antenna
Table 217: | Rear Object Alarm Module - X1 (HSV Maloo)
Table 218: | Rear Object Alarm Module - X2 (HSV Maloo)
Table 219: | Rear Object Alarm (HSV Maloo)
Table 220: | Rear Window Defogger Grid - X1
Table 221: | Rear Window Defogger Grid - X2
Table 222: | Recirculation Actuator
Table 223: | Remote Function Actuator
Table 224: | Repeater Lamp - Left
Table 225: | Repeater Lamp - Right
Table 226: | Reverse Lockout Solenoid (L98)
Table 227: | Reverse Lockout Solenoid (LS2) (HSV Maloo)
Table 228: | Seat Adjuster Switch - Driver
Table 229: | Seat Belt Pretensioner - LF
Table 230: | Seat Belt Pretensioner - RF
Table 231: | Seat Rear Vertical Motor - Driver
Table 232: | Secondary Information Center (SIC) Module - X1
Table 233: | Speaker - Center X1 (Type B and C Infotainment System)
Table 234: | Speaker - Center X2 (Type B and C Infotainment System)
Table 235: | Speaker - LF Door (Infotainment System)
Table 236: | Speaker - LF Tweeter (Type F Infotainment System)
Table 237: | Speaker - RF Door
Table 238: | Speaker - RF Tweeter (Type F Infotainment System)
Table 239: | Starter
Table 240: | Starter
Table 241: | Steering Angle Sensor
Table 242: | Steering Angle Sensor (HSV Maloo)
Table 243: | Steering Wheel Controls Switch Assembly
Table 244: | Sunshade - Left (HSV Maloo)
Table 245: | Sunshade - Right (HSV Maloo)
Table 246: | Tail Lamp Assembly - Left
Table 247: | Tail Lamp Assembly - Right
Table 248: | Theft Deterrent Control Module
Table 249: | Theft Horn X1
Table 250: | Theft Horn X2
Table 251: | Throttle Body (L98)
Table 252: | Throttle Body (LS2) (HSV Maloo)
Table 253: | Throttle Body (LY7)
Table 254: | Transmission Control Module (TCM) - 5L40E
Table 255: | Turn Signal Multifunction Switch
Table 256: | Variable Intake Manifold (VIM) Solenoid (LY7)
Table 257: | Wheel Speed Sensor (WSS) - LF
Table 258: | Wheel Speed Sensor (WSS) - LR
Table 259: | Wheel Speed Sensor (WSS) - RF
Table 260: | Wheel Speed Sensor (WSS) - RR
Table 261: | Window/Door Lock/Outside Rear-view Mirror Switch - X1
Table 262: | Window/Door Lock/Outside Rear-view Mirror Switch - X2
Table 263: | Window Motor - LF
Table 264: | Window Motor - RF
Table 265: | Windshield Washer Fluid Pump
Table 266: | Windshield Wiper Motor
Table 267: | Windshield Wiper/Washer Switch
Table 268: | Yaw Rate and Lateral Acceleration Sensor

#### Accelerator Pedal Position (APP) Sensor (LY7/L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/YE | 1274 | 5-Volt Reference
2 | WH/BK | 1165 | 5-Volt Reference
3 | BU/WH | 116 | APP Sensor 1 Signal
4 | BN | 1271 | Low Reference
5 | PU | 1272 | Low Reference
6 | L-BU | 1162 | APP Sensor 2 Signal

#### Accelerator Pedal Position (APP) Sensor (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BN/YE | 0.5 | 5-Volt Reference
2 | WH/BK | 0.5 | 5-Volt Reference
3 | BU/WH | 0.5 | APP Sensor 1 Signal
4 | BN | 0.5 | Low Reference
5 | PU | 0.5 | Low Reference
6 | L-BU | 0.5 | APP Sensor 2 Signal

#### A/C Refrigerant Pressure Sensor (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/D-GN | 2759 | Low Reference
2 | GY | 2709 | 5-Volt Reference
3 | OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal

#### A/C Refrigerant Pressure Sensor (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BN/D-GN | 0.5 | Low Reference
2 | GY | 0.5 | 5-Volt Reference
3 | OG/BK | 0.5 | A/C Refrigerant Pressure Sensor Signal

#### A/C Refrigerant Pressure Sensor (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/GN | 2759 | Low Reference
2 | GY | 2709 | 5-Volt Reference
3 | OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal

#### Air Mix Actuator

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH | 2778 | Air Mix Actuator Power
2 | YE | 1236 | Air Mix Actuator - Control
3 | BK/RD | 719 | Low Reference
4 | BK/YE | 1646 | Air Mix Actuator Feedback
5 | BK/WH | 598 | 5-Volt Reference

#### Ambient Light Sensor

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | L-GN/BK | 1137 | DRL Ambient Light Sensor Signal
B | BK | 850 | Ground

#### Automatic Transmission Shift Lever

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PU | 1375 | Transmission Cruise Switch Reference
2 | -- | -- | Not Used
3 | BK | 850 | Ground
4 | PU/RD | 5526 | Transmission Range Select Reference
5 | -- | -- | Not Used
6 | -- | -- | Not Used
7 | -- | -- | Not Used
8 | -- | -- | Not Used

#### Automatic Transmission (4L60/4L65)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | L-GN | 1222 | Shift Solenoid A Valve Control
B | YE/BK | 1223 | Shift Solenoid B Valve Control
C | OG/BK | 1228 | PC Solenoid Valve High Control
D | L-BU/WH | 1229 | PC Solenoid Valve Low Control
E | PK | 439 | Ignition 1 Voltage
F | -- | -- | Not Used
G | -- | -- | Not Used
H | -- | -- | Not Used
I | -- | -- | Not Used
J | -- | -- | Not Used
K | OG | 1983 | Transmission Turbine Speed Switch Signal
L | YE/BK | 1227 | TFT Sensor Signal
M | TN | 2762 | Low Reference
N | PK | 1224 | Transmission Fluid Pressure Switch Signal A
O | -- | -- | Not Used
P | OG | 1226 | Transmission Fluid Pressure Switch Signal C
Q | -- | -- | Not Used
R | D-BU | 1225 | Transmission Fluid Pressure Switch Signal B
S | WH/GN | 687 | 3-2 Shift Solenoid Valve Control
T | BN/OG | 422 | TCC Solenoid Valve Control
U | BN | 418 | TCC PWM Solenoid Valve Control
V | L-BU | 1984 | Transmission Turbine Speed Switch Low Reference

#### Automatic Transmission (6L80E)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/YE | 3634 | Battery Positive Voltage
2 | BK | 450 | Ground
3 | OG/BK | 1786 | Park/Neutral Signal
4 | OG/YE | 3640 | Battery Positive Voltage
5 | BK | 450 | Ground
6 | WH/BU | 17 | Stop Lamp Switch Signal
7 | -- | -- | Not Used
8 | -- | -- | Not Used
9 | D-BU | 5985 | TCM Accessory Signal
10 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
11 | BN | 2501 | High Speed GMLAN Serial Data Bus-
12 | PK | 439 | Ignition 1 Voltage
13 | BN | 2501 | High Speed GMLAN Serial Data Bus-
14 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
15 | -- | -- | Not Used
16 | -- | -- | Not Used

#### Auxiliary Power Outlet - Console

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN/WH | 243 | Accessory Voltage
B | BK | 2050 | Ground

#### Backup Lamp Switch (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | L-GN | 5007 | Backup Lamp Switch Signal
B | BK | 450 | Ground

#### Backup Lamp Switch (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | L-GN | 0.5 | Backup Lamp Switch Signal
B | BK | 0.5 | Ground

#### Backup Lamp Switch (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-GN | 5007 | Backup Lamp Switch Signal
2 | BK | 450 | Ground

#### Battery Current Sensor

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK | 5076 | 5-Volt Reference
B | BN | 5077 | Low Reference
C | WH/GN | 5075 | Battery Current Signal

#### Battery Negative

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 50 | Ground

#### Battery Positive

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
J1 | RD | 50 | Battery Positive
J2 | RD | 1242 | Battery Positive
J3 | RD/BK | 1042 | Battery Positive

#### Battery Remote Positive Terminal (L98)

Connector Part Information | Positive Jump Start Terminal
--- | ---
Pin | Wire Color | Circuit Number | Function
1 | RD | 1 | Battery Positive Voltage

#### Blower Motor (RHD)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | GN | 442 | Battery Positive Voltage
B | OG | 5987 | HVAC Blower Motor Control Circuit

#### Bluetooth Connector

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | OG/WH | 2340 | Battery Positive Voltage
X1-2 | PK/BU | 1339 | Ignition 1 Voltage
X1-3 | L-GN | 24 | Backup Lamp Supply Voltage
X1-4 | D-GN | 5060 | Low Speed GMLAN Serial Data
X1-5 | BN | 443 | Accessory Voltage
X1-6 | BU | 7148 | Bluetooth Connector
X1-7 | OG/BK | 1406 | Remote Playback Device Left Audio Signal
X1-8 | L-BU | 1405 | Telephone Audio Signal (+)
X1-9 | WH | 700 | Mute Signal
X1-10 | BK | 1050 | Ground
X1-11 | D-BU | 658 | Cellular Telephone Voice Signal
X1-12 | L-BU/BK | 659 | Cellular Telephone Voice Low Reference
X1-13 | YE/BK | 693 | Cellular Telephone Mute Signal
X1-14 | GY | 118 | Left Front Speaker Output (-)
X1-15 | TN | 201 | Left Front Speaker Output (+)
X1-16 | -- | -- | Not Used

#### Bluetooth Microphone

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | GY/BK | 7043 | Microphone Signal
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | PK/BK | 7044 | Microphone Return

#### Bluetooth Module

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | L-BU/BK | 659 | Cellular Telephone Voice Low Reference
X1-2 | -- | -- | Not Used
X1-3 | -- | -- | Not Used
X1-4 | BU | 7148 | Blue Tooth Signal
X1-5 | BU | 7043 | Microphone Signal
X1-6 | YE/BK | 693 | Cellular Telephone Mute Signal
X1-7 | BN | 443 | Accessory Voltage
X1-8 | -- | -- | Not Used
X1-9 | D-BU | 658 | Cellular Telephone Voice Signal
X1-10 | -- | -- | Not Used
X1-11 | -- | -- | Not Used
X1-12 | PK/BK | 7044 | Microphone Return
X1-13 | -- | -- | Not Used
X1-14 | -- | -- | Not Used
X1-15 | BK | 1050 | Ground
X1-16 | OG/WH | 2340 | Battery Positive Voltage

#### Body Control Module (BCM) -X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | -- | -- | Not Used
X1-2 | WH | 1390 | Ignition Key Resistor Low Reference
X1-3 | GY | 1884 | Cruise Control Switch Signal
X1-4 | WH/BK | 1073 | Ignition Key Resistor Signal
X1-5 | L-GN | 1715 | Windshield Wiper Switch High Signal
X1-6 | -- | -- | Not Used
X1-7 | -- | -- | Not Used
X1-8 | BK/WH | 1251 | Wiper Switch Low Reference
X1-9 | L-BU | 1714 | Windshield Wiper Switch Low Signal
X1-10 | -- | -- | Not Used
X1-11 | -- | -- | Not Used
X1-12 | -- | -- | Not Used
X1-13 | -- | -- | Not Used
X1-14 | PK | 3 | Run/Crank Voltage
X1-15 | L-BU/WH | 1414 | Left Turn Signal Switch Signal
X1-16 | D-BU/WH | 1416 | Right Turn Signal Switch Signal
X1-17 | PU | 1375 | Steering Wheel Control Supply Voltage
X1-18 | PU/YE | 524 | Headlamp Dimmer Switch High Beam Signal
X1-19 | -- | -- | Not Used
X1-20 | PU/RD | 5526 | Transmission Electronic Range Select Signal
X1-21 | BN | 4 | Ignition 1 Voltage
X1-22 | -- | -- | Not Used
X1-23 | -- | -- | Not Used
X1-24 | OG | 94 | Windshield Washer Switch Signal
X1-25 | BN/RD | 1356 | Flash To Pass Switch Signal
X1-26 | -- | -- | Not Used
X1-27 | -- | -- | Not Used

#### Body Control Module (BCM) -X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-1 | OG | 1732 | Inadvertent Power Supply Voltage
X2-2 | OG/BU | 1240 | Battery Positive Voltage
X2-3 | GY | 8 | Instrument Panel Lamp Supply Voltage
X2-4 | -- | -- | Not Used
X2-5 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
X2-6 | -- | -- | Not Used
X2-7 | -- | -- | Not Used
X2-8 | BN/WH | 301 | Park Lamp Switch On Signal
X2-9 | -- | -- | Not Used
X2-10 | -- | -- | Not Used
X2-11 | L-GN/BK | 1137 | DRL Ambient Light Sensor Signal
X2-12 | WH | 103 | Headlamp Switch Headlamps On Signal
X2-13 | -- | -- | Not Used
X2-14 | -- | -- | Not Used
X2-15 | -- | -- | Not Used
X2-16 | -- | -- | Not Used
X2-17 | D-GN | 306 | Headlamp Switch Headlamps Off Signal
X2-18 | PK/BK | 1597 | Courtesy Lamps Switch Signal
X2-19 | -- | -- | Not Used
X2-20 | L-BU | 553 | Tow/Haul Switch Signal
X2-21 | BN/OG | 1571 | Traction Control Switch Signal
X2-22 | -- | -- | Not Used
X2-23 | -- | -- | Not Used
X2-24 | -- | -- | Not Used
X2-25 | PU | 328 | Interior Lamp Switch Signal

#### Body Control Module (BCM) -X3

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X3-1 | BK | 850 | Ground
X3-2 | OG/YE | 1640 | Battery Positive Voltage
X3-3 | OG/RD | 2740 | Battery Positive Voltage
X3-4 | -- | -- | Not Used
X3-5 | BK | 850 | Ground
X3-6 | -- | -- | Not Used
X3-7 | GY | 728 | Security Indicator Control
X3-8 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
X3-9 | BN | 2501 | High Speed GMLAN Serial Data Bus-
X3-10 | D-GN | 5060 | Low Speed GMLAN Serial Data
X3-11 | -- | -- | Not Used
X3-12 | -- | -- | Not Used
X3-13 | L-GN | 526 | Stop Lamp Switch Signal
X3-14 | BN/RD | 552 | Low Reference
X3-15 | GY | 598 | 5-Volt Reference
X3-16 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
X3-17 | BN | 2501 | High Speed GMLAN Serial Data Bus-
X3-18 | YE | 6817 | LED Backlight Dimming Control
X3-19 | PU/WH | 5727 | Communication Enable Relay Control
X3-20 | -- | -- | Not Used
X3-21 | OG | 192 | Fog Lamp Switch
X3-22 | -- | -- | Not Used
X3-23 | -- | -- | Not Used
X3-24 | -- | -- | Not Used
X3-25 | -- | -- | Not Used

#### Body Control Module (BCM) -X4

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X4-1 | OG/RD | 340 | Battery Positive Voltage
X4-2 | OG | 240 | Battery Positive Voltage
X4-3 | GN | 440 | Battery Positive Voltage
X4-4 | OG/PU | 2140 | Battery Positive Voltage
X4-5 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
X4-6 | -- | -- | Not Used
X4-7 | YE | 196 | Windshield Wiper Motor Park Switch Signal
X4-8 | -- | -- | Not Used
X4-9 | BK | 1650 | Ground
X4-10 | OG/BU | 2440 | Battery Positive Voltage
X4-11 | D-GN/WH | 1317 | Fog Lamp Relay - Coil - Output
X4-12 | -- | -- | Not Used
X4-13 | -- | -- | Not Used
X4-14 | -- | -- | Not Used
X4-15 | OG | 2286 | Washer Fluid Pump Relay Control
X4-16 | BN/YE | 1969 | Headlamp High Beam Relay Control
X4-17 | PK/BK | 109 | Hood Ajar Switch Signal
X4-18 | -- | -- | Not Used
X4-19 | D-BU | 5985 | TCM Accessory Signal
X4-20 | -- | -- | Not Used
X4-21 | PK | 1439 | Run/Crank Control
X4-22 | -- | -- | Not Used
X4-23 | -- | -- | Not Used
X4-24 | D-GN | 646 | Backup Lamp Relay Control
X4-25 | -- | -- | Not Used

#### Body Control Module (BCM) -X5

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X5-1 | YE/BK | 1334 | Left Rear Turn Signal Lamp Supply Voltage
X5-2 | D-GN/WH | 1335 | Right Rear Turn Signal Lamp Supply Voltage
X5-3 | -- | -- | Not Used
X5-4 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply
X5-5 | -- | -- | Not Used
X5-6 | WH/BU | 17 | Stop Lamp Switch Signal
X5-7 | -- | -- | Not Used
X5-8 | PK | 5076 | 5-Volt Reference
X5-9 | WH/GN | 5075 | Battery Current Signal
X5-10 | BN | 5077 | Low Reference
X5-11 | BN/YE | 707 | RAP Relay Coil Supply Voltage
X5-12 | -- | -- | Not Used
X5-13 | -- | -- | Not Used
X5-14 | YE | 43 | Accessory Power Relay Control
X5-15 | PU | 5531 | Hood Closed Switch Signal
X5-16 | OG/BK | 233 | Park Brake Switch Signal
X5-17 | -- | -- | Not Used
X5-18 | BN/BK | 28 | Horn Relay Control
X5-19 | -- | -- | Not Used
X5-20 | GY | 91 | Windshield Wiper Switch Signal 2
X5-21 | BN/RD | 860 | Front Windshield Wiper Switch High Signal
X5-22 | -- | -- | Not Used
X5-23 | PK/WH | 1970 | Headlamp Low Beam Relay Control
X5-24 | WH/YE | 1080 | Park Lamp Relay Control
X5-25 | -- | -- | Not Used

#### Body Control Module (BCM) -X6

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X6-1 | -- | -- | Not Used
X6-2 | L-BU | 20 | Stop Lamp Supply Voltage
X6-3 | -- | -- | Not Used
X6-4 | -- | -- | Not Used
X6-5 | -- | -- | Not Used
X6-6 | -- | -- | Not Used
X6-7 | -- | -- | Not Used
X6-8 | BN/WH | 746 | Passenger Front Door Ajar Switch Signal
X6-9 | -- | -- | Not Used
X6-10 | GY/BK | 745 | Driver Door Ajar Switch Signal
X6-11 | -- | -- | Not Used
X6-12 | -- | -- | Not Used
X6-13 | -- | -- | Not Used
X6-14 | -- | -- | Not Used
X6-15 | -- | -- | Not Used
X6-16 | -- | -- | Not Used
X6-17 | -- | -- | Not Used
X6-18 | -- | -- | Not Used
X6-19 | -- | -- | Not Used
X6-20 | PK | 781 | Driver Door Lock Switch Unlock Signal
X6-21 | -- | -- | Not Used
X6-22 | -- | -- | Not Used
X6-23 | PK/BK | 780 | Driver Door Lock Switch Lock Signal
X6-24 | -- | -- | Not Used
X6-25 | -- | -- | Not Used

#### Body Control Module (BCM) - X7

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X7-1 | -- | -- | Not Used
X7-2 | -- | -- | Not Used
X7-3 | -- | -- | Not Used
X7-4 | -- | -- | Not Used
X7-5 | -- | -- | Not Used
X7-6 | L-BU | 5921 | Driver Door / Fuel Door Unlock Control
X7-7 | BU/WH | 195 | Door Lock Relay Control
X7-8 | -- | -- | Not Used
X7-9 | WH | 194 | Door Unlock Control
X7-10 | GY/BU | 7388 | Dimmer Control Up Signal
X7-11 | BN/BK | 254 | Rear Door Lock Switch Unlock Signal
X7-12 | GY/BK | 255 | Rear Door Lock Switch Lock Signal
X7-13 | -- | -- | Not Used
X7-14 | -- | -- | Not Used
X7-15 | -- | -- | Not Used
X7-16 | -- | -- | Not Used
X7-17 | -- | -- | Not Used
X7-18 | -- | -- | Not Used
X7-19 | -- | -- | Not Used
X7-20 | -- | -- | Not Used
X7-21 | -- | -- | Not Used
X7-22 | -- | -- | Not Used
X7-23 | -- | -- | Not Used
X7-24 | GY/WH | 7389 | Dimmer Control Down Signal
X7-25 | -- | -- | Not Used
X7-26 | -- | -- | Not Used
X7-27 | -- | -- | Not Used
X7-28 | -- | -- | Not Used

#### Brake Fluid Level Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/WH | 33 | Brake Warning Indicator Control
2 | BK | 350 | Ground

#### Brake Pedal Position (BPP) Sensor

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | GY | 598 | 5-Volt Reference
B | L-GN | 526 | Stop Lamp Switch Signal
C | BN/RD | 552 | Low Reference

#### Camshaft Position (CMP) Exhaust Sensor - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BK | 632 | Low Reference
2 | D-GN | 5273 | CMP Sensor Signal - Exhaust Bank 1
3 | GY | 705 | 5-Volt Reference

#### Camshaft Position (CMP) Exhaust Sensor - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BK | 632 | Low Reference
2 | PU | 5274 | CMP Sensor Signal - Exhaust Bank 2
3 | GY | 705 | 5-Volt Reference

#### Camshaft Position (CMP) Exhaust Solenoid - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5293 | Ignition 1 Voltage
2 | L-GN | 5282 | CMP Actuator Solenoid Control - Exhaust Bank 1

#### Camshaft Position (CMP) Exhaust Solenoid - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5293 | Ignition 1 Voltage
2 | WH/BK | 5283 | CMP Actuator Solenoid Control - Exhaust Bank 2

#### Camshaft Position (CMP) Intake Sensor - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BK | 632 | Low Reference
2 | OG/BU | 5275 | CMP Sensor Signal - Intake Bank 1
3 | GY | 705 | 5-Volt Reference

#### Camshaft Position (CMP) Intake Sensor - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BK | 632 | Low Reference
2 | YE/RD | 5276 | CMP Sensor Signal - Intake Bank 2
3 | GY | 705 | 5-Volt Reference

#### Camshaft Position (CMP) Intake Solenoid - 1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5293 | Ignition 1 Voltage
2 | PU | 5284 | CMP Actuator Solenoid Control - Intake Bank 1

#### Camshaft Position (CMP) Intake Solenoid - 2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5293 | Ignition 1 Voltage
2 | OG/BK | 5272 | CMP Actuator Solenoid Control - Intake Bank 2

#### Camshaft Position (CMP) Sensor (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | OG | 631 | 5-Volt Reference
B | PK/BK | 632 | Low Reference
C | BN/WH | 633 | CMP Sensor Signal

#### Camshaft Position (CMP) Sensor (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | OG | 0.5 | 5-Volt Reference
B | PK/BK | 0.5 | Low Reference
C | BN/WH | 0.5 | CMP Sensor Signal

#### Center High Mounted Stop Lamp

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | L-BU | 20 | Stop Lamp Supply Voltage
B | BK | 1650 | Ground

#### Cigar Lighter-Front Console

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | GY | 8 | Instrument Panel Lamp Supply Voltage
X1-B | BN/YE | 143 | Accessory Voltage
X1-C | BK | 850 | Ground

#### Clutch Cruise Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/YE | 6109 | Clutch Position Sensor Reference
2 | -- | -- | Not Used
3 | YE | 6111 | Clutch Position Sensor Signal
4 | BN/YE | 6110 | Clutch Position Sensor Return

#### Clutch Safety Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/YE | 6109 | Clutch Position Sensor Reference
2 | -- | -- | Not Used
3 | YE | 6111 | Clutch Position Sensor Signal
4 | BN/YE | 6110 | Clutch Position Sensor Return

#### Clutch Start Switch V6

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/YE | 6109 | Clutch Position Sensor Reference
2 | -- | -- | Not Used
3 | YE | 6111 | Clutch Position Sensor Signal
4 | BN/YE | 6110 | Clutch Position Sensor Return

#### Clutch Start Switch V8

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/YE | 6109 | Clutch Position Sensor Reference
2 | -- | -- | Not Used
3 | YE | 6111 | Clutch Position Sensor Signal
4 | BN/YE | 6110 | Clutch Position Sensor Return

#### Crankshaft Position (CKP) Sensor

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PU | 574 | Low Reference
2 | YE/BU | 573 | CKP Sensor Signal
3 | PU/WH | 605 | 5-Volt Reference

#### Crankshaft Position (CKP) Sensor (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | D-BU/WH | 1869 | CKP Sensor Signal
B | YE/BK | 1868 | Low Reference
C | L-GN | 1867 | 5-Volt Reference

#### Crankshaft Position (CKP) Sensor (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | D-BU/WH | 0.5 | CKP Sensor Signal
B | YE/BK | 0.5 | Low Reference
C | L-GN | 0.5 | 5-Volt Reference

#### Cruise Control Switch (Part of the Turn Signal Multifunction Switch)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 850 | Ground
2 | BN/RD | 1356 | Flash To Pass Switch Signal
3 | PU/YE | 524 | Headlamp Dimmer Switch High Beam Signal
4 | BK | 850 | Ground
5 | GY | 1884 | Cruise Control Switch Signal
6 | PU | 1375 | 5-Volt Reference
7 | D-BU/WH | 1450 | Right Turn Signal Switch Signal
8 | L-BU/WH | 1414 | Left Turn Signal Switch Signal

#### Data Link Connector (DLC)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 5060 | Low Speed GMLAN Serial Data
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | BK | 850 | Ground
5 | BK | 850 | Ground
6 | BN/WH | 2500 | High Speed GMLAN Serial Data Bus+
7 | -- | -- | Not Used
8 | -- | -- | Not Used
9 | -- | -- | Not Used
10 | -- | -- | Not Used
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | BN | 2501 | High Speed GMLAN Serial Data Bus-
15 | -- | -- | Not Used
16 | OG/WH | 1840 | Battery Positive Voltage

#### Dome Lamp

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK/WH | 851 | Ground
2 | PK/BK | 1597 | Courtesy Lamp Switch on Signal
3 | PU | 328 | Interior Lamp Supply Voltagel
4 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage

#### Door Latch Assembly - LF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | BN/RD | 294 | Door Lock Actuator Unlock Control
3 | GN/WH | 295 | Door Lock Actuator Lock Control
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | BN/WH | 746 | Passenger Door Ajar Switch Signal
7 | -- | -- | Not Used
8 | BK | 2050 | Ground
9 | -- | -- | Not Used
10 | -- | -- | Not Used

#### Door Latch Assembly - RF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | GY/BK | 745 | Right Front Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | BK | 1350 | Ground
4 | PK | 781 | Driver Door Lock Switch Unlock Signal
5 | -- | -- | Not Used
6 | -- | -- | Not Used
7 | BN/RD | 694 | Driver Door Lock Actuator Unlock Control
8 | GN/WH | 295 | Door Lock Actuator Lock Control
9 | PK/BK | 780 | Driver Door Lock Switch Lock Signal
10 | -- | -- | Not Used

#### Driving Lamp - Left (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PU | 0.75 | Front Driving Lamp Relay Supply Voltage
B | BK | 0.75 | Ground

#### Driving Lamp - Right (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PU | 0.75 | Front DrivingLamp Relay Supply Voltage
B | BK | 0.75 | Ground

#### Driving Lamp - HSVDR-1 (HSV Maloo)

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BL | 0.3 | Ground
2 | RE / BL | 0.3 | Voltage Supply

#### Electronic Brake Control Module (EBCM) - (JL4)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 350 | Ground
2 | RD/BK | 142 | Battery Positive Voltage
3 | OG | 3540 | Battery Positive Voltage
4 | BK | 350 | Ground
5 | L-BU | 830 | Left Front Wheel Speed Sensor Signal
6 | GY | 7127 | Left Rear Wheel Speed Sensor Supply Voltage
7 | GY | 7128 | Right Rear Wheel Speed Sensor Supply Voltage
8 | BN | 882 | Right Rear Wheel Speed Sensor Signal
9 | GY | 7065 | Right Front Wheel Speed Sensor Supply Voltage
10 | D-GN | 872 | Right Front Wheel Speed Sensor Signal
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | BN | 2501 | High Speed GMLAN Serial Data Bus-
15 | BK/BU | 2088 | Steering Wheel Position Low Refernce
16 | BN/WH | 2086 | Yaw Rate Sensor Test Control
17 | -- | -- | Not Used
18 | D-GN | 2087 | Steering Wheel Sensor 5 Volt Reference
19 | -- | -- | Not Used
20 | PU/WH | 1699 | Combined Vehicle Sensor Signal (LAT/LONG)
21 | -- | -- | Not Used
22 | -- | -- | Not Used
23 | -- | -- | Not Used
24 | -- | -- | Not Used
25 | BN | 2501 | High Speed GMLAN Serial Data Bus-
26 | GY | 7064 | Left Front Wheel Speed Sensor Supply Voltage
27 | BN/BK | 884 | Left Rear Wheel Speed Sensor Signal
28 | L-BU | 5986 | Communication Enable Relay Supply Voltage
29 | -- | -- | Not Used
30 | -- | -- | Not Used
31 | -- | -- | Not Used
32 | -- | -- | Not Used
33 | -- | -- | Not Used
34 | -- | -- | Not Used
35 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
36 | -- | -- | Not Used
37 | L-GN/BK | 5352 | Yaw Rate Sensor Test Control
38 | -- | -- | Not Used
39 | -- | -- | Not Used
40 | -- | -- | Not Used
41 | -- | -- | Not Used
42 | -- | -- | Not Used
43 | -- | -- | Not Used
44 | -- | -- | Not Used
45 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
46 | -- | -- | Not Used

#### Electronic Control Valve Displacement (ECVD)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-BU | 7393 | A/C Compressor Low Reference
2 | D-GN | 7392 | A/C Compressor Supply Voltage

#### Engine Control Module - X1 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | OG/BK | 1876 | Park/Neutral Signal
X1-2 | -- | -- | Not Used
X1-3 | -- | -- | Not Used
X1-4 | -- | -- | Not Used
X1-5 | -- | -- | Not Used
X1-6 | -- | -- | Not Used
X1-7 | -- | -- | Not Used
X1-8 | L-GN | 5007 | Backup Lamp Switch Signal
X1-9 | WH/BU | 17 | Stop Lamp Switch Signal
X1-10 | PU/WH | 1668 | HO2S High Signal (Bank 1 Sensor 2)
X1-11 | BN/WH | 1669 | HO2S Low Signal (Bank 1 Sensor 2)
X1-12 | OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal
X1-13 | BN/D-GN | 2759 | Low Reference
X1-14 | -- | -- | Not Used
X1-15 | -- | -- | Not Used
X1-16 | PU | 1589 | Fuel Level Sensor Signal (Primary)
X1-17 | D-BU/BK | 473 | High Speed Cooling Fan Relay Control
X1-18 | D-BU | 5985 | TCM Accessory Signal
X1-19 | PK | 439 | Ignition 1 Voltage
X1-20 | OG/BK | 540 | Battery Positive Voltage
X1-21 | -- | -- | Not Used
X1-22 | -- | -- | Not Used
X1-23 | PU | 1272 | Low Reference
X1-24 | -- | -- | Not Used
X1-25 | -- | -- | Not Used
X1-26 | YE | 6111 | Sensor Clutch Position Signal
X1-27 | BN | 2501 | High Speed GMLAN Serial Data Bus-
X1-28 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
X1-29 | BU/WH | 1161 | APP Sensor 1 Signal
X1-30 | BN | 1271 | Low Reference
X1-31 | BN/YE | 452 | Low Reference
X1-32 | L-BU | 1162 | APP Sensor 2 Signal
X1-33 | -- | -- | Not Used
X1-34 | GY | 2709 | 5-Volt Reference
X1-35 | -- | -- | Not Used
X1-36 | BN/YE | 1274 | 5-Volt Reference
X1-37 | BN/RD | 472 | IAT Sensor Signal
X1-38 | BN/WH | 2760 | Low Reference
X1-39 | -- | -- | Not Used
X1-40 | -- | -- | Not Used
X1-41 | YE | 492 | MAF Sensor Signal
X1-42 | BN/YE | 6110 | Sensor Clutch Position Return
X1-43 | -- | -- | Not Used
X1-44 | -- | -- | Not Used
X1-45 | -- | -- | Not Used
X1-46 | -- | -- | Not Used
X1-47 | PK/BU | 5290 | Ignition 1 Voltage
X1-48 | -- | -- | Not Used
X1-49 | BN/WH | 1671 | HO2S Low Signal (Bank 2 Sensor 2)
X1-50 | D-GN/WH | 465 | Fuel Pump Relay Control (Primary)
X1-51 | -- | -- | Not Used
X1-52 | YE | 447 | Starter Relay Coil Control
X1-53 | -- | -- | Not Used
X1-54 | OG/YE | 6109 | Clutch Pedal Position Sensor Reference
X1-55 | -- | -- | Not Used
X1-56 | WH/BK | 1164 | 5-Volt Reference
X1-57 | -- | -- | Not Used
X1-58 | D-GN | 335 | Low Speed Cooling Fan Relay Control
X1-59 | BN | 5069 | Main Relay Control
X1-60 | -- | -- | Not Used
X1-61 | -- | -- | Not Used
X1-62 | -- | -- | Not Used
X1-63 | -- | -- | Not Used
X1-64 | OG/WH | 3223 | HO2S Heater Low Control (Bank 2 Sensor 2)
X1-65 | BN | 3122 | HO2S Heater Low Control (Bank 1 Sensor 2)
X1-66 | -- | -- | Not Used
X1-67 | -- | -- | Not Used
X1-68 | BN/WH | 419 | MIL Control
X1-69 | PU | 1670 | HO2S High Signal (Bank 2 Sensor 2)
X1-70 | L-BU | 1937 | Fuel Level Sensor Signal (Secondary)
X1-71 | -- | -- | Not Used
X1-72 | -- | -- | Not Used
X1-73 | BK | 450 | Ground

#### Engine Control Module - X1 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X1-1 | OG/BK | 0.5 | Park/Neutral Signal
X1-2 | -- | -- | --
X1-3 | -- | -- | --
X1-4 | -- | -- | --
X1-5 | -- | -- | --
X1-6 | BN/WH | 0.5 | Cruise Control Disable Clutch Switch Signal
X1-7 | -- | -- | --
X1-8 | L-GN | 0.5 | Backup Lamp Switch Signal
X1-9 | WH/BU | 0.5 | Stop Lamp Switch Signal
X1-10 | PU/WH | 0.5 | HO2S High Signal (Bank 1 Sensor 2)
X1-11 | BN/WH | 0.5 | HO2S Low Signal (Bank 1 Sensor 2)
X1-12 | OG/BK | 0.5 | A/C Refrigerant Pressure Sensor Signal
X1-13 | BN/D-GN | 0.5 | Low Reference
X1-14 | -- | -- | --
X1-15 | -- | -- | --
X1-16 | PU | 0.5 | Fuel Level Sensor Signal (Primary)
X1-17 | D-BU | 0.5 | High Speed Cooling Fan Relay Control
X1-18 | D-BU | 0.5 | TCM Accessory Signal
X1-19 | PK | 0.5 | Ignition 1 Voltage
X1-20 | OG/BK | 0.75 | Battery Positive Voltage
X1-21 | -- | -- | --
X1-22 | -- | -- | --
X1-23 | PU | 0.5 | Low Reference
X1-24 | -- | -- | --
X1-25 | -- | -- | --
X1-26 | -- | -- | --
X1-27 | BN | 0.5 | High Speed GMLAN Serial Data Bus-
X1-28 | BN/BK | 0.5 | High Speed GMLAN Serial Data Bus+
X1-29 | BU/WH | 0.5 | APP Sensor 1 Signal
X1-30 | BN | 0.5 | Low Reference
X1-31 | BN/YE | 0.5 | Low Reference
X1-32 | L-BU | 0.5 | APP Sensor 2 Signal
X1-33 | -- | -- | --
X1-34 | GY | 0.5 | 5-Volt Reference
X1-35 | -- | -- | --
X1-36 | BN/YE | 0.5 | 5-Volt Reference
X1-37 | BN/RD | 0.5 | IAT Sensor Signal
X1-38 | BN/WH | 0.5 | Low Reference
X1-39 | -- | -- | --
X1-40 | -- | -- | --
X1-41 | YE | 0.5 | MAF Sensor Signal
X1-42 | -- | -- | --
X1-43 | -- | -- | --
X1-44 | XX | XX | High Speed Cooling Fan Relay Control
X1-45 | -- | -- | --
X1-46 | -- | -- | --
X1-47 | BK | 0.75 | Ignition 1 Voltage
X1-48 | -- | -- | --
X1-49 | BN/WH | 0.5 | HO2S Low Signal (Bank 2 Sensor 2)
X1-50 | D-GN/WH | 0.5 | Fuel Pump Relay Control (Primary)
X1-51 | -- | -- | --
X1-52 | YE | 0.5 | Starter Relay Coil Control
X1-53 | -- | -- | --
X1-54 | -- | -- | --
X1-55 | -- | -- | --
X1-56 | WH/BK | 0.5 | 5-Volt Reference
X1-57 | -- | -- | --
X1-58 | D-GN | 0.5 | Low Speed Cooling Fan Relay Control
X1-59 | BN | 0.5 | Main Relay Control
X1-60 | -- | -- | --
X1-61 | -- | -- | --
X1-62 | -- | -- | --
X1-63 | -- | -- | --
X1-64 | OG/WH | 0.5 | HO2S Heater Low Control (Bank 2 Sensor 2)
X1-65 | BN | 0.5 | HO2S Heater Low Control (Bank 1 Sensor 2)
X1-66 | -- | -- | --
X1-67 | -- | -- | --
X1-68 | BN/WH | 0.5 | MIL Control
X1-69 | PU | 0.5 | HO2S High Signal (Bank 2 Sensor 2)
X1-70 | L-BU | 0.5 | Fuel Level Sensor Signal (Secondary)
X1-71 | -- | -- | --
X1-72 | -- | -- | --
X1-73 | BK | 2.0 | Ground

#### Engine Control Module - X1(LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | L-GN | 5282 | Cam Phaser Exhaust 1 Signal
X1-2 | PU | 5284 | Cam Phaser Intake 1 Signal
X1-3 | -- | -- | Not Used
X1-4 | YE/BK | 846 | Fuel Injector 6 Control
X1-5 | D-GN/WH | 428 | EVAP Canister Purge Solenoid Control
X1-6 | -- | -- | Not Used
X1-7 | OG/BU | 5275 | Intake 1 Cam Position Sensor Signal
X1-8 | -- | -- | Not Used
X1-9 | PU | 5274 | Exhaust 2 Cam Position Sensor Signal
X1-10 | OG/WH | 225 | Generator Turn On Signal
X1-11 | BN | 1174 | Oil Level Switch Signal
X1-12 | -- | -- | Not Used
X1-13 | PK | 6414 | Low Reference
X1-14 | BN | 1997 | Ether Solenoid - Feed
X1-15 | GY | 705 | 5-Volt Reference
X1-16 | -- | -- | Not Used
X1-17 | -- | -- | Not Used
X1-18 | -- | -- | Not Used
X1-19 | -- | -- | Not Used
X1-20 | -- | -- | Not Used
X1-21 | -- | -- | Not Used
X1-22 | -- | -- | Not Used
X1-23 | -- | -- | Not Used
X1-24 | YE | 581 | TAC Motor Control - 1
X1-25 | WH/BK | 5283 | Cam Phaser Exhaust 2 Signal
X1-26 | PK/BK | 1746 | Fuel Injector 3 Control
X1-27 | -- | -- | Not Used
X1-28 | BN/WH | 845 | Fuel Injector 5 Control
X1-29 | -- | -- | Not Used
X1-30 | PU/WH | 23 | Generator Field Duty Cycle Signal
X1-31 | -- | -- | Not Used
X1-32 | -- | -- | Not Used
X1-33 | YE/RD | 5276 | Intake 2 Cam Position Sensor Signal
X1-34 | D-GN | 5273 | Exhaust 1 Cam Position Sensor Signal
X1-35 | YE/BU | 573 | CKP Sensor 1 Signal
X1-36 | -- | -- | Not Used
X1-37 | -- | -- | Not Used
X1-38 | -- | -- | Not Used
X1-39 | GY | 2701 | 5-Volt Reference
X1-40 | GY | 596 | 5-Volt Reference
X1-41 | PK/BK | 632 | Low Reference
X1-42 | -- | -- | Not Used
X1-43 | BN/RD | 470 | Low Reference
X1-44 | BK | 2755 | Low Reference
X1-45 | PU/WH | 605 | 5-Volt Reference
X1-46 | PU | 574 | Low Reference
X1-47 | -- | -- | Not Used
X1-48 | BN | 582 | TAC Motor Control - 2
X1-49 | OG/BK | 5272 | Cam Phaser Intake 2 Signal
X1-50 | L-BU/BK | 844 | Fuel Injector 4 Control
X1-51 | BN/BK | 1744 | Fuel Injector 1 Control
X1-52 | L-GN/BK | 1745 | Fuel Injector 2 Control
X1-53 | -- | -- | Not Used
X1-54 | -- | -- | Not Used
X1-55 | PU | 2121 | IC 1 Control
X1-56 | L-BU | 2123 | IC 3 Control
X1-57 | GN/RD | 2125 | IC 5 Control
X1-58 | -- | -- | Not Used
X1-59 | D-BU | 496 | Knock Sensor 1 Signal
X1-60 | BN | 407 | Low Reference
X1-61 | BN/WH | 331 | Oil Pressure Sensor Signal
X1-62 | -- | -- | Not Used
X1-63 | -- | -- | Not Used
X1-64 | -- | -- | Not Used
X1-65 | -- | -- | Not Used
X1-66 | -- | -- | Not Used
X1-67 | BN/YE | 1664 | HO2S Low Signal (Bank 1 Sensor 1)
X1-68 | -- | -- | Not Used
X1-69 | -- | -- | Not Used
X1-70 | PU | 1666 | HO2S High Signal (Bank 2 Sensor 1)
X1-71 | -- | -- | Not Used
X1-72 | L-GN | 3212 | HO2S Low Signal (Bank 2 Sensor 1)
X1-73 | -- | -- | Not Used
X1-74 | -- | -- | Not Used
X1-75 | -- | -- | Not Used
X1-76 | -- | -- | Not Used
X1-77 | -- | -- | Not Used
X1-78 | PU | 6413 | Low Reference
X1-79 | OG/WH | 2122 | IC 2 Control
X1-80 | D-GN/WH | 2124 | IC 4 Control
X1-81 | L-BU/WH | 2126 | IC 6 Control
X1-82 | YE/GN | 410 | ECT Sensor Signal
X1-83 | GY | 1716 | Low Reference
X1-84 | L-BU | 1876 | Knock Sensor 2 Signal
X1-85 | GN/YE | 357 | Oil Temperature Sensor Signal
X1-86 | -- | -- | Not Used
X1-87 | -- | -- | Not Used
X1-88 | BN/BK | 2752 | Low Reference
X1-89 | PU | 486 | TP Sensor 2 Signal
X1-90 | D-GN | 485 | TP Sensor 1 Signal
X1-91 | -- | -- | Not Used
X1-92 | PU/WH | 1665 | HO2S High Signal (Bank 1 Sensor 1)
X1-93 | BN/RD | 1667 | HO2S Low Signal (Bank 2 Sensor 1)
X1-94 | -- | -- | Not Used
X1-95 | -- | -- | Not Used
X1-96 | GY/WH | 3113 | HO2S Heater Low Control (Bank 1 Sensor 1)

#### Engine Control Module - X2 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X2-1 | -- | -- | Not Used
X2-2 | L-GN | 0.5 | 5-Volt Reference
X2-3 | GY | 0.5 | 5-Volt Reference
X2-4 | -- | -- | Not Used
X2-5 | BN | 0.75 | TAC Motor Control - 2
X2-6 | YE | 0.75 | TAC Motor Control - 1
X2-7 | -- | -- | Not Used
X2-8 | D-GN/WH | 0.5 | EVAP Canister Purge Solenoid Control
X2-9 | -- | -- | Not Used
X2-10 | -- | -- | Not Used
X2-11 | L-GN | 0.75 | Reverse Lockout Solenoid Control
X2-12 | GY/WH | 0.5 | HO2S Heater Low Control (Bank 1 Sensor 1)
X2-13 | L-GN | 0.5 | HO2S Heater Low Control (Bank 2 Sensor 1)
X2-14 | -- | -- | Not Used
X2-15 | -- | -- | Not Used
X2-16 | -- | -- | Not Used
X2-17 | D-BU/WH | 0.75 | Fuel Injector 8 Control
X2-18 | BN/WH | 0.75 | Fuel Injector 5 Control
X2-19 | YE/BK | 0.75 | Fuel Injector 6 Control
X2-20 | BN/BK | 0.75 | Fuel Injector 1 Control
X2-21 | YE/D-GN | 0.5 | ECT Sensor Signal
X2-22 | BN/WH | 0.5 | Low Reference
X2-23 | D-GN/YE | 0.5 | Oil Temperature Sensor Signal
X2-24 | BN/RD | 0.5 | Low Reference
X2-25 | -- | -- | Not Used
X2-26 | D-BU | 0.5 | Knock Sensor 1 Signal
X2-27 | GY | 0.5 | Low Reference
X2-28 | -- | -- | Not Used
X2-29 | L-BU | 0.5 | Knock Sensor 2 Signal
X2-30 | TN | 0.5 | Low Reference
X2-31 | -- | -- | Not Used
X2-32 | PU/WH | 0.5 | Generator Field Duty Cycle Signal
X2-33 | BN | 0.5 | Oil Level Switch Signal
X2-34 | BK | 0.5 | Low Reference
X2-35 | BN/BK | 0.5 | Low Reference
X2-36 | -- | -- | Not Used
X2-37 | L-GN/BK | 0.75 | Fuel Injector 2 Control
X2-38 | PK/BK | 0.75 | Fuel Injector 3 Control
X2-39 | L-BU/BK | 0.75 | Fuel Injector 4 Control
X2-40 | OG/BK | 0.75 | Fuel Injector 7 Control
X2-41 | GY | 0.5 | 5-Volt Reference
X2-42 | -- | -- | Not Used
X2-43 | GY | 0.5 | 5-Volt Reference
X2-44 | OG | 0.5 | 5-Volt Reference
X2-45 | -- | -- | Not Used
X2-46 | -- | -- | Not Used
X2-47 | -- | -- | Not Used
X2-48 | -- | -- | Not Used
X2-49 | -- | -- | Not Used
X2-50 | BN/WH | 0.5 | Oil Pressure Sensor Signal
X2-51 | -- | -- | Not Used
X2-52 | -- | -- | Not Used
X2-53 | OG/BK | 0.5 | Low Reference
X2-54 | -- | -- | Not Used
X2-55 | -- | -- | Not Used
X2-56 | BN/YE | 0.5 | HO2S Low Signal (Bank 1 Sensor 1)
X2-57 | PU/WH | 0.5 | HO2S High Signal (Bank 1 Sensor 1)
X2-58 | L-GN | 0.5 | MAP Sensor Signal
X2-59 | PU | 0.5 | HO2S High Signal (Bank 2 Sensor 1)
X2-60 | BN/RD | 0.5 | HO2S Low Signal (Bank 2 Sensor 1)
X2-61 | OG/WH | 0.5 | Generator Turn On Signal
X2-62 | -- | -- | Not Used
X2-63 | PU | 0.5 | TP Sensor 2 Signal
X2-64 | BN/WH | 0.5 | CMP Sensor Signal
X2-65 | D-GN | 0.5 | TP Sensor 1 Signal
X2-66 | PK/BK | 0.5 | Low Reference
X2-67 | -- | -- | Not Used
X2-68 | D-BU/WH | 0.5 | CKP Sensor Signal
X2-69 | YE/BK | 0.5 | Low Reference
X2-70 | PU | 0.5 | IC 1 Control
X2-71 | PU/WH | 0.5 | IC 8 Control
X2-72 | OG | 0.5 | IC 7 Control
X2-73 | OG/WH | 0.5 | IC 2 Control
X2-74 | L-BU/WH | 0.5 | IC 6 Control
X2-75 | D-GN/RD | 0.5 | IC 5 Control
X2-76 | D-GN/WH | 0.5 | IC 4 Control
X2-77 | L-BU | 0.5 | IC 3 Control
X2-78 | BN | 0.5 | Low Reference
X2-79 | BN/WH | 0.5 | Low Reference
X2-80 | -- | -- | Not Used

#### Engine Control Module - X2 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X2-1 | -- | -- | --
X2-2 | L-GN | 0.5 | 12-Volt Reference
X2-3 | GY | 0.5 | 5-Volt Reference
X2-4 | -- | -- | --
X2-5 | BN | 0.75 | TAC Motor Control - 2
X2-6 | YE | 0.75 | TAC Motor Control - 1
X2-7 | -- | -- | --
X2-8 | D-GN/WH | 0.75 | EVAP Canister Purge Solenoid Control
X2-9 | -- | -- | --
X2-10 | -- | -- | --
X2-11 | L-GN | 0.75 | Reverse Lockout Solenoid Control
X2-12 | GY/WH | 0.5 | HO2S Heater Low Control (Bank 1 Sensor 1)
X2-13 | L-GN | 0.5 | HO2S Heater Low Control (Bank 2 Sensor 1)
X2-14 | -- | -- | --
X2-15 | -- | -- | --
X2-16 | -- | -- | --
X2-17 | D-BU/WH | 0.75 | Fuel Injector 8 Control
X2-18 | BN/WH | 0.75 | Fuel Injector 5 Control
X2-19 | YE/BK | 0.75 | Fuel Injector 6 Control
X2-20 | BN/BK | 0.75 | Fuel Injector 1 Control
X2-21 | YE/D-GN | 0.5 | ECT Sensor Signal
X2-22 | BN/WH | 0.5 | Low Reference
X2-23 | D-GN/YE | 0.5 | Oil Temperature Sensor Signal
X2-24 | BN/RD | 0.5 | Low Reference
X2-25 | -- | -- | --
X2-26 | D-BU | 0.5 | Knock Sensor 1 Signal
X2-27 | GY | 0.5 | Low Reference
X2-28 | -- | -- | --
X2-29 | L-BU | 0.5 | Knock Sensor 2 Signal
X2-30 | TN | 0.5 | Low Reference
X2-31 | -- | -- | --
X2-32 | PU/WH | 0.5 | Generator Field Duty Cycle Signal
X2-33 | BN | 0.5 | Oil Level Switch Signal
X2-34 | BK | 0.5 | Low Reference
X2-35 | BN/BK | 0.5 | Low Reference
X2-36 | -- | -- | --
X2-37 | L-GN/BK | 0.75 | Fuel Injector 2 Control
X2-38 | PK/BK | 0.75 | Fuel Injector 3 Control
X2-39 | L-BU/BK | 0.75 | Fuel Injector 4 Control
X2-40 | OG/BK | 0.75 | Fuel Injector 7 Control
X2-41 | GY | 0.5 | 5-Volt Reference
X2-42 | -- | -- | --
X2-43 | GY | 0.5 | 5-Volt Reference
X2-44 | OG | 0.35 | 12-Volt Reference
X2-45 | -- | -- | --
X2-46 | -- | -- | --
X2-47 | -- | -- | --
X2-48 | -- | -- | --
X2-49 | -- | -- | --
X2-50 | BN/WH | 0.5 | Oil Pressure Sensor Signal
X2-51 | -- | -- | --
X2-52 | -- | -- | --
X2-53 | OG/BK | 0.5 | Low Reference
X2-54 | -- | -- | --
X2-55 | -- | -- | --
X2-56 | BN/YE | 0.5 | HO2S Low Signal (Bank 1 Sensor 1)
X2-57 | PU/WH | 0.5 | HO2S High Signal (Bank 1 Sensor 1)
X2-58 | L-GN | 0.5 | MAP Sensor Signal
X2-59 | PU | 0.5 | HO2S High Signal (Bank 2 Sensor 1)
X2-60 | BN/RD | 0.5 | HO2S Low Signal (Bank 2 Sensor 1)
X2-61 | OG/WH | 0.5 | Generator Turn On Signal
X2-62 | -- | -- | --
X2-63 | PU | 0.5 | TP Sensor 2 Signal
X2-64 | BN/WH | 0.5 | CMP Sensor Signal
X2-65 | D-GN | 0.5 | TP Sensor 1 Signal
X2-66 | PK/BK | 0.5 | Low Reference
X2-67 | -- | -- | --
X2-68 | D-BU/WH | 0.5 | CKP Sensor Signal
X2-69 | YE/BK | 0.5 | Low Reference
X2-70 | PU | 0.5 | IC 1 Control
X2-71 | PU/WH | 0.5 | IC 8 Control
X2-72 | OG | 0.5 | IC 7 Control
X2-73 | OG/WH | 0.5 | IC 2 Control
X2-74 | L-BU/WH | 0.5 | IC 6 Control
X2-75 | D-GN/RD | 0.5 | IC 5 Control
X2-76 | D-GN/WH | 0.5 | IC 4 Control
X2-77 | L-BU | 0.5 | IC 3 Control
X2-78 | BN | 0.5 | Low Reference
X2-79 | BN/WH | 0.5 | Low Reference
X2-80 | -- | -- | --

#### Engine Control Module - X2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-1 | BK | 450 | Ground
X2-2 | BK | 450 | Ground
X2-3 | PK/BU | 5290 | Ignition 1 Voltage
X2-4 | BK | 450 | Ground
X2-5 | PK/BK | 5290 | Ignition 1 Voltage
X2-6 | PK/BU | 5290 | Ignition 1 Voltage
X2-7 | GY/WH | 3122 | HO2S Heater Low Control (Bank 1 Sensor 2)
X2-8 | -- | -- | Not Used
X2-9 | BN/YE | 452 | Low Reference
X2-10 | D-GN/WH | 465 | Fuel Pump Relay Control (Primary)
X2-11 | BN/GN | 2759 | Low Reference
X2-12 | -- | -- | Not Used
X2-13 | YE | 492 | MAF Sensor Signal
X2-14 | -- | -- | Not Used
X2-15 | BU/WH | 1161 | APP Sensor 1 Signal
X2-16 | YE | 6111 | Sensor Clutch Position Signal
X2-17 | OG/BK | 1786 | Park/Neutral/Clutch Safety Switch Signal
X2-18 | L-GN | 5007 | Backup Lamp Switch Signal
X2-19 | -- | -- | Not Used
X2-20 | OG/WH | 3223 | HO2S Heater Low Control (Bank 2 Sensor 2)
X2-21 | BN/WH | 419 | MIL Control
X2-22 | BN/WH | 2760 | Low Reference
X2-23 | BN/GN | 3121 | HO2S Low Signal (Bank 1 Sensor 2)
X2-24 | BN/RD | 3221 | HO2S Low Signal (Bank 2 Sensor 2)
X2-25 | L-BU | 1162 | APP Sensor 2 Signal
X2-26 | L-BU | 1937 | Fuel Level Sensor Signal (1)
X2-27 | -- | -- | Not Used
X2-28 | -- | -- | Not Used
X2-29 | -- | -- | Not Used
X2-30 | -- | -- | Not Used
X2-31 | -- | -- | Not Used
X2-32 | -- | -- | Not Used
X2-33 | -- | -- | Not Used
X2-34 | BN | 1271 | Low Reference
X2-35 | GY | 2709 | 5-Volt Reference
X2-36 | PU | 1589 | Fuel Level Sensor Signal (2)
X2-37 | -- | -- | Not Used
X2-38 | PU | 3120 | HO2S High Signal (Bank 1 Sensor 2)
X2-39 | OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal
X2-40 | -- | -- | Not Used
X2-41 | D-BU | 5985 | Ignition Switch Wake Up Signal
X2-42 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
X2-43 | -- | -- | Not Used
X2-44 | -- | -- | Not Used
X2-45 | BU/BK | 473 | High Speed Cooling Fan Relay Control
X2-46 | D-GN | 335 | Low Speed Cooling Fan Relay Control
X2-47 | PU | 1272 | Low Reference
X2-48 | BN/YE | 1274 | 5-Volt Reference
X2-49 | WH/BK | 1164 | 5-Volt Reference
X2-50 | BN/RD | 472 | IAT Sensor Signal
X2-51 | PU | 3220 | HO2S High Signal (Bank 2 Sensor 2)
X2-52 | WH/BU | 17 | Stop Lamp Switch Signal
X2-53 | -- | -- | Not Used
X2-54 | PK | 439 | Ignition 1 Voltage
X2-55 | BN | 2501 | High Speed GMLAN Serial Data Bus-
X2-56 | OG/BK | 540 | Battery Positive Voltage
X2-57 | YE | 447 | Starter Relay Coil Control
X2-58 | BN | 5069 | Main Relay Control

#### Engine Coolant Temperature (ECT) Sensor (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN/WH | 2761 | Low Reference
B | YE/D-GN | 410 | ECT Sensor Signal

#### Engine Coolant Temperature (ECT) Sensor (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN/WH | 0.5 | Low Reference
B | YE/D-GN | 0.5 | ECT Sensor Signal

#### Engine Coolant Temperature (ECT) Sensor (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | YE/GN | 410 | ECT Sensor Signal
2 | BK | 2755 | Low Reference

#### Engine Cooling Fan - Left

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 250 | Ground
B | BU | 409 | Left Cooling Fan Motor Supply Voltage

#### Engine Cooling Fan - Right

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | GY | 532 | Right Cooling Fan Motor Low Reference
B | WH | 504 | Right Cooling Fan Motor Supply Voltage

#### Engine Oil Level/Temperature Sensor (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN | 1174 | Oil Level Switch Signal
B | D-GN/YE | 357 | Oil Temperature Sensor Signal
C | BN/RD | 470 | Low Reference

#### Engine Oil Level/Temperature Sensor (LS2) (HSV Maloo)

Connector Part Information | GT 150 Sealed 4.5
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN | 0.5 | Oil Level Switch Signal
B | YE | 0.5 | Oil Temperature Sensor Signal
C | BN/RD | 0.5 | Low Reference

#### Engine Oil Level/Temperature Sensor (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN | 1174 | Oil Level Switch Signal
B | GN/YE | 357 | Oil Temperature Sensor Signal
C | BK | 2755 | Low Reference

#### Engine Oil Pressure (EOP) Sensor (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 2755 | Low Reference
2 | GY | 2705 | 5-Volt Reference
3 | BN/WH | 331 | Oil Pressure Sensor Signal

#### Engine Oil Pressure (EOP) Sensor (LS2) (HSV Maloo)

Connector Part Information | GT 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BK | 0.5 | Low Reference
2 | GY | 0.5 | 5-Volt Reference
3 | BN/WH | 0.5 | Oil Pressure Sensor Signal

#### Engine Oil Pressure (EOP) Sensor (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/RD | 470 | Low Reference
2 | GY | 596 | 5-Volt Reference
3 | BN/WH | 331 | Oil Pressure Sensor Signal

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BK | 5293 | Ignition 1 Voltage
2 | D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.75 | Ignition 1 Voltage
B | D-GN/WH | 0.75 | EVAP Canister Purge Solenoid Control

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5293 | Ignition 1 Voltage
B | D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

#### Express Down Window Module

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BU/WH | 666 | Power Window Motor Right Front Up Control
2 | BN/OG | 165 | Power Window Motor Left Front Down Control
3 | L-BU | 166 | Power Window Master Switch Right Front Up Signal
4 | -- | -- | Not Used
5 | BK | 1350 | Ground
6 | BN | 1300 | Power Window Master Switch Left Front Up Signal
7 | -- | -- | Not Used
8 | D-GN/BK | 1001 | RAP Supply Voltage
9 | GN/BK | 167 | Power Window Master Switch Right Front Down Signal
10 | BN | 667 | Power Window Motor Right Front Down Control
11 | D-BU | 164 | Power Window Motor Left Front Up Control
12 | GY/BU | 1136 | Power Window Motor Left Front Down Control

#### Fog Lamp - Left

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PU | 34 | Front Fog Lamp Relay Supply Voltage
B | BK | 350 | Ground

#### Fog Lamp - Right

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PU | 34 | Front Fog Lamp Relay Supply Voltage
B | BK | 350 | Ground

#### Fuel Filler Door Latch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | GN/WH | 295 | Door Lock Actuator Lock Control
2 | BN/RD | 694 | Driver Door Lock Actuator Unlock Control

#### Fuel Injector - 1 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5291 | Ignition 1 Voltage
B | BN/BK | 1744 | Fuel Injector 1 Control

#### Fuel Injector - 1 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.75 | Ignition 1 Voltage
B | BN/BK | 0.75 | Fuel Injector 1 Control

#### Fuel Injector - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5291 | Ignition 1 Voltage
B | BN/BK | 1744 | Fuel Injector 1 Control

#### Fuel Injector - 2 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK | 5292 | Ignition 1 Voltage
B | L-GN/BK | 1745 | Fuel Injector 2 Control

#### Fuel Injector - 2 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK | 0.75 | Ignition 1 Voltage
B | L-GN/BK | 0.75 | Fuel Injector 2 Control

#### Fuel Injector - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK | 5292 | Ignition 1 Voltage
B | L-GN/BK | 1745 | Fuel Injector 2 Control

#### Fuel Injector - 3 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5291 | Ignition 1 Voltage
B | PK/BK | 1746 | Fuel Injector 3 Control

#### Fuel Injector - 3 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.75 | Ignition 1 Voltage
B | PK/BK | 0.75 | Fuel Injector 3 Control

#### Fuel Injector - 3 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5291 | Ignition 1 Voltage
B | PK/BK | 1746 | Fuel Injector 3 Control

#### Fuel Injector - 4 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK | 5292 | Ignition 1 Voltage
B | L-BU/BK | 844 | Fuel Injector 4 Control

#### Fuel Injector - 4 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK | 0.75 | Ignition 1 Voltage
B | L-BU/BK | 0.75 | Fuel Injector 4 Control

#### Fuel Injector - 4 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK | 5292 | Ignition 1 Voltage
B | L-BU/BK | 844 | Fuel Injector 4 Control

#### Fuel Injector - 5 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5291 | Ignition 1 Voltage
B | BN/WH | 845 | Fuel Injector 5 Control

#### Fuel Injector - 5 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.75 | Ignition 1 Voltage
B | BN/WH | 0.75 | Fuel Injector 5 Control

#### Fuel Injector - 5 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5291 | Ignition 1 Voltage
B | BN/WH | 845 | Fuel Injector 5 Control

#### Fuel Injector - 6 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK | 5292 | Ignition 1 Voltage
B | YE/BK | 846 | Fuel Injector 6 Control

#### Fuel Injector - 6 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK | 0.75 | Ignition 1 Voltage
B | YE/BK | 0.75 | Fuel Injector 6 Control

#### Fuel Injector - 6 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK | 5292 | Ignition 1 Voltage
B | YE/BK | 846 | Fuel Injec tor 6 Control

#### Fuel Injector - 7 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5291 | Ignition 1 Voltage
B | OG/BK | 877 | Fuel Injector 7 Control

#### Fuel Injector - 7 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.75 | Ignition 1 Voltage
B | OG/BK | 0.75 | Fuel Injector 7 Control

#### Fuel Injector - 8 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK | 5292 | Ignition 1 Voltage
B | D-BU/WH | 878 | Fuel Injector 8 Control

#### Fuel Injector - 8 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK | 0.75 | Ignition 1 Voltage
B | D-BU/WH | 0.75 | Fuel Injector 8 Control

#### Fuel Level Sensor - Secondary

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | L-BU | 1937 | Fuel Level Signal Signal (Secondary)
3 | BN/YE | 452 | Low Reference
4 | -- | -- | Not Used
5 | -- | -- | Not Used

#### Fuel Level Sensor - Secondary (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
Z-1 | BN/YE | 0.3 | Fuel Level Signal (Secondary)
Z-2 | L-BU | 0.5 | Low Reference
Z-3 | -- | -- | --
Z-4 | -- | -- | --
Z-5 | -- | -- | --

#### Fuel Pump and Sender Assembly

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/YE | 452 | Low Reference
2 | PU | 1589 | Fuel Level Sensor Signal [- Primary]
3 | -- | -- | Not Used
4 | BK | 1350 | Ground
5 | GY | 120 | Fuel Pump Supply Voltage

#### Fuse Block - Instrument Panel

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
B1-A | RD | 242 | Battery Positive Voltage
B1-B | OG/BU | 1540 | Battery Positive Voltage
B2-A | D-GN | 801 | RAP Supply Voltage
B2-B | D-GN | 1001 | RAP Supply Voltage
B3-A | RD | 242 | Battery Positive Voltage
B3-B | OG | 1140 | Battery Positive Voltage
F1-B | OG/YE | 1340 | Battery Positive Voltage
F2-A | RD | 242 | Battery Positive Voltage
F2-B | -- | -- | Not Used
F3-B | OG/RD | 3240 | Battery Positive Voltage
F4-B | OG/YE | 1640 | Battery Positive Voltage
F5-B | OG | 240 | Battery Positive Voltage
F6-A | RD/BK | 642 | Battery Positive Voltage
F6-B | OG/GN | 440 | Battery Positive Voltage
F7-B | -- | -- | Spare Fuse
F8-B | OG/RD | 340 | Battery Positive Voltage
F9-B | OG/RD | 2740 | Battery Positive Voltage
F10-A | RD/YE | 642 | Battery Positive Voltage
F10-B | OG/PU | 2140 | Battery Positive Voltage
F11-B | OG/BU | 1240 | Battery Positive Voltage
F12-B | OG/BK | 1040 | Battery Positive Voltage
F13-B | BN/YE | 143 | Accessory Voltage
F14-A | YE | 643 | Accessory Voltage
F14-B | BN/WH | 243 | Accessory Voltage
F15-B | BN/BU | 343 | Accessory Voltage
F16-B | BN | 443 | Accessory Voltage
F17-A | -- | -- | Not Used
F17-B | -- | -- | Not Used
F23-A | YE | 6817 | LED Backlight Dimming Control
F23-B | PU/WH | 7005 | I/P Dimming Control
F24-A | D-GN | 801 | RAP Supply Voltage
F24-B | D-GN | 1301 | RAP Supply Voltage
R1-30 | RD | 242 | Battery Positive Voltage
R1-85 | BN/YE | 707 | RAP Relay Control
R1-86 | BK | 850 | Ground
R1-87 | D-GN | 801 | RAP Supply Voltage
R2-30 | GN/WH | 295 | Door Lock Actuator Lock Control
R2-85 | BK | 1450 | Ground
R2-86 | L-BU | 195 | Door Lock Relay Control
R2-87 | OG/RD | 3240 | Battery Positive Voltage
R2-87A | BK | 1450 | Ground
R3-30 | BN/RD | 294 | Door Lock Actuator Unlock Control
R3-85 | WH | 194 | Door Unlock Control
R3-86 | OG/RD | 3240 | Battery Positive Voltage
R3-87 | OG/RD | 3240 | Battery Positive Voltage
R3-87A | BK | 1450 | Ground
R5-30 | -- | -- | Not Used
R5-85 | -- | -- | Not Used
R5-86 | -- | -- | Not Used
R5-87 | -- | -- | Not Used
R6-30 | BN/RD | 694 | Driver Door Lock Actuator Unlock Control
R6-85 | L-BU | 5921 | Driver Door/Fuel Door Unlock Control
R6-86 | OG/RD | 3240 | Battery Positive Voltage
R6-87 | OG/RD | 3240 | Battery Positive Voltage
R6-87A | BK | 1450 | Ground
R8-30 | RD/BK | 642 | Battery Positive Voltage
R8-85 | YE | 43 | Accessory Voltage
R8-86 | BK | 1450 | Ground
R8-87 | YE | 643 | Accessory Voltage
R12-30 | GY | 120 | Fuel Pump Supply Voltage
R12-85 | D-GN/WH | 465 | Fuel Pump Relay Control
R12-86 | BK | 1450 | Ground
R12-87 | OG/GN | 2840 | Battery Positive Voltage

#### Fuse Block - Underhood - X1 (134)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/D-BU | 5294 | Ignition 1 Voltage
2 | -- | -- | Not Used
3 | D-GN | 335 | Low Speed Cooling Fan Relay Control
4 | -- | -- | Not Used
5 | PK | 439 | Ignition 1 Voltage
6 | -- | -- | Not Used
7 | YE | 447 | Starter Relay Coil Control
8 | PU | 293 | Rear Defog Element Supply Voltage
9 | PU | 6 | Starter Solenoid Crank Voltage
10 | -- | -- | Not Used
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | -- | -- | Not Used
15 | -- | -- | Not Used
16 | -- | -- | Not Used
17 | -- | -- | Not Used
18 | -- | -- | Not Used
19 | -- | -- | Not Used
20 | OG | 3540 | Battery Positive Voltage
21 | -- | -- | Not Used
22 | YE | 712 | Left Headlamp Low Beam Supply Voltage
23 | D-BU/BK | 473 | High Speed Cooling Fan Relay Control
24 | D-BU | 5985 | TCM Accessory Signal
25 | PK/D-BU | 5293 | Ignition 1 Voltage
26 | -- | -- | Not Used
27 | -- | -- | Not Used
28 | -- | -- | Not Used
29 | -- | -- | Not Used
30 | -- | -- | Not Used
31 | OG/YE | 3640 | Battery Positive Voltage
32 | BK | 350 | Ground
33 | -- | -- | Not Used
34 | WH/D-BU | 17 | Stop Lamp Switch Signal
35 | -- | -- | Not Used
36 | D-BU | 5985 | TCM Accessory Signal
37 | -- | -- | Not Used
38 | -- | -- | Not Used
39 | -- | -- | Not Used
40 | -- | -- | Not Used
41 | PK/D-BU | 5290 | Ignition 1 Voltage
42 | -- | -- | Not Used
43 | -- | -- | Not Used
44 | -- | -- | Not Used
45 | BK | 350 | Ground
46 | BK | 350 | Ground
47 | PK | 5292 | Ignition 1 Voltage
48 | -- | -- | Not Used
49 | BN | 5069 | Main Relay Control
50 | -- | -- | Not Used
51 | PK/BU | 5291 | Ignition 1 Voltage
52 | -- | -- | Not Used
53 | -- | -- | Not Used
54 | -- | -- | Not Used

#### Fuse Block - Underhood - X2 (132)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | -- | -- | Not Used
5 | D-GN | 442 | Battery Positive Voltage
6 | RD/BK | 642 | Battery Positive Voltage
7 | -- | 842 | Spare Battery Positive Voltage
8 | PU | 293 | Rear Defog Element Supply Voltage
9 | -- | 542 | Spare Battery Positive Voltage
10 | -- | -- | Not Used
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | L-BU | 5986 | Communication Enable Relay Supply Voltage
14 | -- | -- | Not Used
15 | WH/YE | 1080 | Park Lamp Relay Control
16 | -- | -- | Not Used
17 | PK/BU | 339 | Ignition 1 Voltage
18 | PU | 34 | Fog Lamps Supply Voltage
19 | -- | -- | Not Used
20 | -- | -- | Not Used
21 | -- | -- | Not Used
22 | -- | -- | Not Used
23 | PU | 709 | Left Park Lamp Supply Voltage
24 | WH/D-BU | 193 | Rear Defog Relay Control
25 | PK/WH | 1970 | Headlamp Low Beam Relay Control
26 | BN/RD | 860 | Front Windshield Wiper Switch High Signal
27 | D-GN/WH | 317 | Fog Lamps Relay Control
28 | BN/YE | 1969 | Headlamp High Beam Relay Control
29 | BN/BK | 28 | Horn Relay Control
30 | -- | -- | Not Used
31 | OG | 2268 | Washer Fluid Pump Relay Control
32 | PK | 1439 | Run Crank Control
33 | -- | -- | Not Used
34 | -- | -- | Not Used
35 | -- | -- | Not Used
36 | -- | -- | Not Used
37 | -- | -- | Not Used
38 | -- | -- | Not Used
39 | -- | -- | Not Used
40 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
41 | L-GN | 24 | Backup Lamp Supply Voltage
42 | -- | -- | Not Used
43 | WH/BU | 17 | Stop Lamp Switch Signal
44 | -- | -- | Not Used
45 | D-BU | 5985 | TCM Accessory Signal
46 | -- | -- | Not Used
47 | -- | -- | Not Used
48 | -- | -- | Not Used
49 | -- | -- | Not Used
50 | -- | -- | Not Used
51 | -- | -- | Not Used
52 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
53 | -- | -- | Not Used
54 | PU/WH | 5727 | Communication Enable Relay Control
55 | D-GN | 646 | Reverse Relay Control
56 | GY | 91 | Windshield Wiper Switch Signal 2
57 | -- | -- | Not Used
58 | -- | -- | Not Used
59 | OG/GN | 2240 | Battery Positive Voltage
60 | D-GN | 1149 | Theft Deterrent Horn Fuse Supply Voltage
61 | -- | -- | Not Used
62 | -- | -- | Not Used
63 | -- | -- | Not Used
64 | -- | -- | Not Used
65 | BN/WH | 309 | Lamp Supply Voltage
66 | -- | -- | Not Used
67 | -- | -- | Not Used
68 | PK/BU | 1339 | Ignition 1 Voltage
69 | PU | 5531 | Hood Closed Switch Signal
70 | PK/BK | 109 | Hood Ajar Switch Signal
71 | -- | -- | Not Used
72 | -- | -- | Not Used
73 | -- | -- | Not Used
74 | BN/WH | 74 | Windshield Wiper Motor High Speed
75 | -- | -- | Not Used
76 | -- | -- | Not Used
77 | -- | -- | Not Used
78 | RD/BU | 2640 | Battery Positive Voltage
79 | -- | -- | Not Used
80 | RD | 242 | Battery Positive Voltage
81 | -- | -- | Not Used
82 | -- | -- | Not Used
83 | D-GN | 96 | Windshield Wiper Motor Low Speed
84 | -- | -- | Not Used

#### Fuse Block - Underhood - X3 (130)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH | 504 | Cooling Fan Low Reference
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | BK | 250 | Ground
5 | -- | -- | Not Used
6 | OG | 228 | Windshield Washer Pump Control
7 | -- | -- | Not Used
8 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
9 | PK/BK | 109 | Hood Ajar Switch Signal
10 | PU | 709 | Left Park Lamp Supply Voltage
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
15 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
16 | -- | -- | Not Used
17 | -- | -- | Not Used
18 | BN/WH | 309 | Right Park Lamp Supply Voltage
19 | -- | -- | Not Used
20 | PU | 5531 | Hood Closed Switch Signal
21 | BN/BK | 312 | Right Headlamp Low Beam Supply Voltage
22 | YE | 712 | Left Headlamp Low Beam Supply Voltage
23 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
24 | -- | -- | Not Used
25 | D-GN | 1329 | Horn Fuse Supply Voltage
26 | -- | -- | Not Used
27 | -- | -- | Not Used
28 | -- | -- | Not Used
29 | GY | 532 | Cooling Fan Low Reference
30 | -- | -- | Not Used
31 | -- | -- | Not Used
32 | BU | 409 | Cooling Fan Motor Supply Voltage

#### Generator

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/WH | 225 | Generator Turn On Signal
2 | PU/WH | 23 | Generator Field Duty Cycle Signal

#### Headlamp and Dimmer Panel Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH | 103 | Headlamp Switch Headlamps On Signal
2 | -- | -- | Not Used
3 | D-GN | 306 | Headlamp Switch Headlamps Off Signal/Automatic Headlamp Low Control
4 | BK | 850 | Ground
5 | BN/WH | 301 | Park Lamp Switch Signal
6 | OG | 192 | Front Fog Lamp Switch Signal
7 | GY/WH | 7389 | Dimmer Control Down Signal
8 | YE | 6817 | LED Backlight Dimming Control
9 | -- | -- | Not Used
10 | PK/BU | 1339 | Ignition 1 Voltage
11 | -- | -- | Not Used
12 | GY/BU | 7388 | Dimmer Control Up Signal

#### Headlamp Assembly - Left

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 250 | Ground
2 | BK | 250 | Ground
3 | BK | 250 | Ground
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | PU | 709 | Left Park Lamp Supply Voltage
7 | YE | 712 | Left Headlamp Low Beam Supply Voltage
8 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
9 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
10 | -- | -- | Not Used

#### Headlamp Assembly - Right

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 250 | Ground
2 | BK | 250 | Ground
3 | BK | 250 | Ground
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | BN/WH | 309 | Right Park Lamp Supply Voltage
7 | BN/BK | 312 | Right Headlamp Low Beam Supply Voltage
8 | L-GN/WH | 0.5 | Right Headlamp High Beam Supply Voltage
9 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
10 | -- | -- | Not Used

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN/YE | 1664 | HO2S Low Signal (Bank 1 Sensor 1)
B | PU/WH | 1665 | HO2S High Signal (Bank 1 Sensor 1)
C | GY/WH | 3113 | HO2S Heater Low Control (Bank 1 Sensor 1)
D | PK/BU | 5293 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN/RD | 0.5 | HO2S Low Signal (Bank 1 Sensor 1)
B | PU/WH | 0.5 | HO2S High Signal (Bank 1 Sensor 1)
C | GY/WH | 0.5 | HO2S Heater Low Control (Bank 1 Sensor 1)
D | PK/BK | 0.5 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5293 | Ignition 1 Voltage
2 | GY/WH | 3113 | HO2S Heater Low Control (Bank 1 Sensor 1)
3 | BN/YE | 1664 | HO2S Low Signal (Bank 1 Sensor 1)
4 | PU/WH | 1665 | HO2S High Signal (Bank 1 Sensor 1)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN/WH | 1669 | HO2S Low Signal (Bank 1 Sensor 2)
B | PU/WH | 1668 | HO2S High Signal (Bank 1 Sensor 2)
C | BN | 3122 | HO2S Heater Low Control (Bank 1 Sensor 2)
D | PK/D-BU | 5294 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN/WH | 0.5 | HO2S Low Signal (Bank 1 Sensor 2)
B | PU/WH | 0.5 | HO2S High Signal (Bank 1 Sensor 2)
C | BN | 0.5 | HO2S Heater Low Control (Bank 1 Sensor 2)
D | PK/D-BU | 0.75 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/D-BU | 5294 | Ignition 1 Voltage
2 | BN | 3122 | HO2S Heater Low Control (Bank 1 Sensor 2)
3 | BN/GN | 3121 | HO2S Low Signal (Bank 1 Sensor 2)
4 | PU | 3120 | HO2S High Signal (Bank 1 Sensor 2)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN/RD | 1667 | HO2S Low Signal (Bank 2 Sensor 1)
B | PU | 1666 | HO2S High Signal (Bank 2 Sensor 1)
C | L-GN | 3212 | HO2S Heater Low Control (Bank 2 Sensor 1)
D | PK/BU | 5293 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LS2) (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN/RD | 0.5 | HO2S Low Signal (Bank 2 Sensor 1)
B | PU | 0.5 | HO2S High Signal (Bank 2 Sensor 1)
C | L-GN | 0.5 | HO2S Heater Low Control (Bank 2 Sensor 1)
D | PK/BK | 0.5 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5293 | Ignition 1 Voltage
2 | L-GN | 3212 | HO2S Low Signal (Bank 2 Sensor 1)
3 | L-GN | 1667 | HO2S Heater Low Control (Bank 2 Sensor 1)
4 | PU | 1666 | HO2S High Signal (Bank 2 Sensor 1)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN/WH | 1671 | HO2S Low Signal (Bank 2 Sensor 2)
B | PU | 1670 | HO2S High Signal (Bank 2 Sensor 2)
C | OG/WH | 3223 | HO2S Heater Low Control (Bank 2 Sensor 2)
D | PK/D-BU | 5294 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN/WH | 0.5 | HO2S Low Signal (Bank 2 Sensor 2)
B | PU | 0.5 | HO2S High Signal (Bank 2 Sensor 2)
C | OG/WH | 0.5 | HO2S Heater Low Control (Bank 2 Sensor 2)
D | PK/D-BU | 0.75 | Battery 1 Voltage

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/D-BU | 5294 | Battery 1 Voltage
2 | OG/WH | 3223 | HO2S Heater Low Control (Bank 2 Sensor 2)
3 | BN/RD | 3221 | HO2S Low Signal (Bank 2 Sensor 2)
4 | PU | 3220 | HO2S High Signal (Bank 2 Sensor 2)

#### Hood Ajar Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BK | 109 | Hood Ajar Switch Signal
B | PU | 5531 | Hood Closed Switch Signal
C | BK | 250 | Ground

#### Horn - Left X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | D-GN | 1329 | Content Left Horn Control

#### Horn - Left X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-A | BK | 250 | Ground

#### Horn - Right X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | D-GN | 1329 | Content Right Horn Control

#### Horn - Right X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-A | BK | 250 | Ground

#### HVAC Control Module - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | OG | 5987 | HVAC Blower Motor Control Circuit
X1-2 | BK | 1450 | Ground

#### HVAC Control Module - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-1 | -- | -- | Not Used
X2-2 | -- | -- | Not Used
X2-3 | -- | -- | Not Used
X2-4 | -- | -- | Not Used
X2-5 | -- | -- | Not Used
X2-6 | WH/BU | 193 | Rear Defog Relay Control
X2-7 | -- | -- | Not Used
X2-8 | -- | -- | Not Used
X2-9 | -- | -- | Not Used
X2-10 | D-GN | 5060 | Low Speed GMLAN Serial Data
X2-11 | -- | -- | Not Used
X2-12 | D-BU | 7393 | AC Compressor Low Reference
X2-13 | D-GN | 7392 | AC Compressor Supply Voltage
X2-14 | OG/GN | 2240 | Battery Positive Voltage

#### HVAC Control Module - X3-C1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X3C1-1 | BK | 119 | Mode Actuator 1 - Control
X3C1-2 | BN | 2273 | Mode Actuator 1 - Power
X3C1-3 | GY | 2275 | Mode Actuator 1 - Feedback
X3C1-4 | RD | 1199 | Mode Actuator 2 - Feedback
X3C1-5 | BK/YE | 1646 | Air Mix Actuator - Feedback
X3C1-6 | WH/RD | 1838 | Recirculation Actuator - Feedback
X3C1-7 | BK | 732 | Evaporator Temperature Sensor Signal
X3C1-8 | BK | 731 | Evaporator Temperature Sensor Low Reference
X3C1-9 | BU/BK | 718 | Low Reference
X3C1-10 | BK/RD | 719 | Low Reference
X3C1-11 | L-GN | 2210 | Mode Actuator 2 - Power
X3C1-12 | OG | 1791 | Mode Actuator 2 - Control
X3C1-13 | WH | 2778 | Air Mix Actuator - Power
X3C1-14 | YE | 1236 | Air Mix Actuator - Control
X3C1-15 | WH/BK | 2274 | Recirculation Actuator - Power
X3C1-16 | WH/BU | 1614 | Recirculation Actuator - Control
X3C1-17 | GN | 474 | 5-Volt Reference
X3C1-18 | PK | 1236 | 5-Volt Reference
X3C1-19 | BK/WH | 598 | 5-Volt Reference
X3C1-20 | WH/GN | 597 | 5-Volt Reference
X3C1-21 | BU | 1791 | Low Reference
X3C1-22 | L-BU | 720 | Low Reference

#### Ignition Coil - 1 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2450 | Ground
B | BN | 2129 | Low Reference
C | PU | 2121 | IC 1 Control
D | PK/BK | 5291 | Ignition 1 Voltage

#### Ignition Coil - 1 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.85 | Ground
B | BN | 0.85 | Low Reference
C | PU | 0.8 | IC 1 Control
D | PK/BK | 0.85 | Ignition 1 Voltage

#### Ignition Coil - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2550 | Ground
B | PU | 6413 | Low Reference
C | PU | 2121 | IC 1 Control
D | PK/BU | 5291 | Ignition 1 Voltage

#### Ignition Coil - 2 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | BN/WH | 2130 | Low Reference
C | OG/WH | 2122 | IC 2 Control
D | PK/BK | 5292 | Ignition 1 Voltage

#### Ignition Coil - 2 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.85 | Ground
B | BN/WH | 0.85 | Low Reference
C | OG/WH | 0.5 | IC 2 Control
D | PK/BK | 0.85 | Ignition 1 Voltage

#### Ignition Coil - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | PK | 6413 | Low Reference
C | OG/WH | 2122 | IC 2 Control
D | PK | 5292 | Ignition 1 Voltage

#### Ignition Coil - 3 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2450 | Ground
B | BN | 2129 | Low Reference
C | L-BU | 2123 | IC 3 Control
D | PK/BK | 5291 | Ignition 1 Voltage

#### Ignition Coil - 3 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.85 | Ground
B | BN | 0.85 | Low Reference
C | L-BU | 0.8 | IC 3 Control
D | PK/BK | 0.85 | Ignition 1 Voltage

#### Ignition Coil - 3 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2550 | Ground
B | PU | 6413 | Low Reference
C | L-BU | 2123 | IC 3 Control
D | PK/BU | 5291 | Ignition 1 Voltage

#### Ignition Coil - 4 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | BN/WH | 2130 | Low Reference
C | D-GN/WH | 2124 | IC 4 Control
D | PK/BK | 5292 | Ignition 1 Voltage

#### Ignition Coil - 4 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.85 | Ground
B | BN/WH | 0.85 | Low Reference
C | D-GN/WH | 0.5 | IC 4 Control
D | PK/BK | 0.85 | Ignition 1 Voltage

#### Ignition Coil - 4 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | PK | 6414 | Low Reference
C | D-GN/WH | 2124 | IC 4 Control
D | PK | 5292 | Ignition 1 Voltage

#### Ignition Coil - 5 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2450 | Ground
B | BN | 2129 | Low Reference
C | D-GN | 2125 | IC 5 Control
D | PK/BK | 5291 | Ignition 1 Voltage

#### Ignition Coil - 5 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.85 | Ground
B | BN | 0.85 | Low Reference
C | D-GN | 0.8 | IC 5 Control
D | PK/BK | 0.85 | Ignition 1 Voltage

#### Ignition Coil - 5 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2550 | Ground
B | PU | 6413 | Low Reference
C | GN/RD | 2125 | IC 5 Control
D | PK/BU | 0.75 | Ignition 1 Voltage

#### Ignition Coil - 6 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | BN/WH | 2130 | Low Reference
C | L-BU/WH | 2126 | IC 6 Control
D | PK/BK | 5292 | Ignition 1 Voltage

#### Ignition Coil - 6 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.85 | Ground
B | BN/WH | 0.85 | Low Reference
C | L-BU/WH | 0.5 | Left Front Door Open Switch Signal
D | PK/BK | 0.85 | Ignition 1 Voltage

#### Ignition Coil - 6 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | PK | 6414 | Low Reference
C | L-BU/WH | 2126 | IC 6 Control
D | PK | 5292 | Ignition 1 Voltage

#### Ignition Coil - 7 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2450 | Ground
B | BN | 2129 | Low Reference
C | OG | 2127 | IC 7 Control
D | PK/BK | 5291 | Ignition 1 Voltage

#### Ignition Coil - 7 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.85 | Ground
B | BN | 0.85 | Low Reference
C | OG | 0.8 | IC 7 Control
D | PK/BK | 0.85 | Ignition 1 Voltage

#### Ignition Coil - 8 (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | BN/WH | 2130 | Low Reference
C | PU/WH | 2128 | IC 8 Control
D | PK/BK | 5292 | Ignition 1 Voltage

#### Ignition Coil - 8 (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.85 | Ground
B | BN/WH | 0.85 | Low Reference
C | PU/WH | 0.5 | IC 8 Control
D | PK/BK | 0.85 | Ignition 1 Voltage

#### Ignition Key Cylinder Lamp

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
B | BK | 850 | Ground

#### Ignition Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK | 3 | Run/Crank Voltage
2 | OG/BK | 1040 | Battery Positive Voltage
3 | BN | 4 | Accessory Voltage
4 | WH | 390 | Ignition Key Resistor Low Reference
5 | -- | -- | Not Used
6 | WH/BK | 1073 | Ignition Key Resistor Signal

#### Inflatable Restraint Front Sensor - RF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | YE | 354 | Discriminating Sensor - Signal
2 | BN/YE | 5045 | Discriminating Sensor - Low Reference

#### Inflatable Restraint Front Sensor - LF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 1409 | Discriminating Sensor - Signal
2 | GY | 5600 | Discriminating Sensor - Low Reference

#### Inflatable Restraint I/P Module - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | BU | 3024 | I/P Module - Stage 1 - Low Control
X1-2 | YE | 3025 | I/P Module - Stage 1 - High Control

#### Inflatable Restraint I/P Module - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-1 | PU | 3026 | I/P Module - Stage 2 - Low Control
X2-2 | D-GN | 3027 | I/P Module - Stage 2 - High Control

#### Inflatable Restraint Seat Position Sensor (SPS) - Driver

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | PK/BU | 5055 | Seat Position Sensor - Right Front - Signal
B | PU/WH | 1363 | Seat Belt Switch - Right Front - Low Reference

#### Inflatable Restraint Sensing and Diagnostic Module - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | BN | 3020 | Steering Wheel Module - Stage1 - Low Control
X1-2 | BN/RD | 3021 | Steering Wheel Module - Stage1 - High Control
X1-3 | WH | 3023 | Steering Wheel Module - Stage2 - High Control
X1-4 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control
X1-5 | -- | -- | Not Used
X1-6 | -- | -- | Not Used
X1-7 | -- | -- | Not Used
X1-8 | -- | -- | Not Used
X1-9 | -- | -- | Not Used
X1-10 | -- | -- | Not Used
X1-11 | -- | -- | Not Used
X1-12 | -- | -- | Not Used
X1-13 | -- | -- | Not Used
X1-14 | -- | -- | Not Used
X1-15 | -- | -- | Not Used
X1-16 | -- | -- | Not Used
X1-17 | -- | -- | Not Used
X1-18 | -- | -- | Not Used
X1-19 | GY | 5600 | Discriminating Sensor - Low Reference
X1-20 | D-GN | 1409 | Discriminating Sensor - Signal
X1-21 | PK/BU | 339 | Ignition 1 Voltage
X1-22 | OG/YE | 1340 | Battery Positive Voltage
X1-23 | -- | -- | Not Used
X1-24 | BK/WH | 1751 | Ground

#### Inflatable Restraint Sensing and Diagnostic Module - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-1 | -- | -- | Not Used
X2-2 | -- | -- | Not Used
X2-3 | -- | -- | Not Used
X2-4 | -- | -- | Not Used
X2-5 | -- | -- | Not Used
X2-6 | -- | -- | Not Used
X2-7 | PU | 3026 | I/P Module - Stage 2 - Low Control
X2-8 | D-GN | 3027 | I/P Module - Stage 2 - High Control
X2-9 | YE | 3025 | I/P Module - Stage 1 - High Control
X2-10 | BU | 3024 | I/P Module - Stage 1 - Low Control
X2-11 | -- | -- | Not Used
X2-12 | -- | -- | Not Used
X2-13 | -- | -- | Not Used
X2-14 | -- | -- | Not Used
X2-15 | BK/WH | 2118 | Seat Belt Pretensioner - High Control
X2-16 | OG/BK | 2119 | Seat Belt Pretensioner - Low Control
X2-17 | OG | 2117 | Seat Belt Pretensioner - Low Control
X2-18 | L-GN | 2116 | Seat Belt Pretensioner - High Control
X2-19 | -- | -- | Not Used
X2-20 | -- | -- | Not Used
X2-21 | -- | -- | Not Used
X2-22 | -- | -- | Not Used
X2-23 | YE | 354 | Discriminating Sensor - Signal
X2-24 | BN/YE | 5045 | Discriminating Sensor - Low Reference
X2-25 | -- | -- | Not Used
X2-26 | -- | -- | Not Used
X2-27 | -- | -- | Not Used
X2-28 | -- | -- | Not Used
X2-29 | -- | -- | Not Used
X2-30 | -- | -- | Not Used
X2-31 | -- | -- | Not Used
X2-32 | -- | -- | Not Used
X2-33 | -- | -- | Not Used
X2-34 | -- | -- | Not Used
X2-35 | L-GN | 5055 | Seat Position Sensor - Right Front - Signal
X2-36 | BK/WH | 238 | Seat Belt Switch - Right Front
X2-37 | -- | -- | Not Used
X2-38 | D-BU | 1363 | Seat Belt Switch - Right Front - Low Reference
X2-39 | -- | -- | Not Used
X2-40 | D-GN | 5060 | Low Speed GMLAN Serial Data

#### Inflatable Restraint Steering Wheel Module - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | BN | 3020 | Steering Wheel Module - Stage1 - Low Control
X1-2 | TN | 3021 | Steering Wheel Module - Stage1 - High Control

#### Inflatable Restraint Steering Wheel Module - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-1 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control
X2-2 | WH | 3023 | Steering Wheel Module - Stage2 - High Control

#### Inflatable Restraint Steering Wheel Module Coil - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | GY/BU | 7367 | Steering Wheel Resistor Ladder Right Signal #2
X1-B | BN/GN | 7364 | Steering Wheel Resistor Ladder Right Signal #1
X1-C | BN | 7312 | Steering Wheel Resistor Ladder Left Signal #1
X1-D | L-BU | 7313 | Steering Wheel Resistor Ladder Left Signal #2
X1-E | BN/WH | 897 | DIC Switch Low Reference
X1-F | OG/BK | 5201 | Steering Wheel Controls Signal
X1-G | BK | 850 | Ground
X1-H | PU/WH | 7005 | I/P Dimming Control
X1-I | -- | -- | Not Used
X1-J | BN/BK | 28 | Horn Relay Control
X1-K | -- | -- | Not Used

#### Inflatable Restraint Steering Wheel Module Coil - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | GY/BU | 7367 | Steering Wheel Resistor Ladder Right Signal #2
X1-B | YE | 7364 | Steering Wheel Resistor Ladder Right Signal #1
X1-C | BN | 7312 | Steering Wheel Resistor Ladder Left Signal #1
X1-D | L-BU | 7313 | Steering Wheel Resistor Ladder Left Signal #2
X1-E | GN | 897 | DIC Switch Low Reference
X1-F | OG/BK | 5201 | Steering Wheel Controls Signal
X1-G | BK | 850 | Ground
X1-H | PU | 7005 | I/P Dimming Control
X1-J | BK/WH | 28 | Horn Relay Control
X1-K | -- | -- | Not Used

#### Inflatable Restraint Steering Wheel Module Coil - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A-1 | TN | 3021 | Steering Wheel Module - Stage1 - High Control
A-2 | BN | 3020 | Steering Wheel Module - Stage1 - Low Control
B-1 | WH | 3023 | Steering Wheel Module - Stage2 - High Control
B-2 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control

#### Inflatable Restraint Steering Wheel Module Coil - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A-1 | BN/RD | 3021 | Steering Wheel Module - Stage1 - High Control
A-2 | BN | 3020 | Steering Wheel Module - Stage1 - Low Control
B-1 | WH | 3023 | Steering Wheel Module - Stage2 - High Control
B-2 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control

#### Instrument Panel Cluster (IPC)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/WH | 1840 | Battery Positive Voltage
2 | GY | 728 | Security Indicator Control
3 | BU | 7148 | Bluetooth Signal
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | BN | 7312 | Steering Wheel Resistor Ladder Left Signal #1
7 | GY/BU | 7367 | Steering Wheel Resistor Ladder Right SIgnal #2
8 | BN/GN | 7364 | Steering Wheel Resistor Ladder Right Signal #1
9 | BK | 850 | Ground
10 | PK | 3 | Ignition 1 Voltage
11 | BN/WH | 419 | MIL Control
12 | OG/BK | 5201 | Steering Wheel Controls Signal
13 | BN/WH | 33 | Brake Warning Indicator Control
14 | -- | -- | Not Used
15 | D-GN | 5060 | Low Speed GMLAN Serial Data
16 | -- | -- | Not Used
17 | L-BU | 7313 | Steering Wheel Resistor Ladder Left Signal #2
18 | BN/WH | 897 | DIC Switch Low Reference

#### Instrument Panel Data Link Connector

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 5060 | Low Speed GMLAN Serial Data
2 | D-GN | 5060 | Low Speed GMLAN Serial Data
3 | D-GN | 5060 | Low Speed GMLAN Serial Data
4 | D-GN | 5060 | Low Speed GMLAN Serial Data
5 | D-GN | 5060 | Low Speed GMLAN Serial Data
6 | D-GN | 5060 | Low Speed GMLAN Serial Data
7 | -- | -- | Not Used
8 | D-GN | 5060 | Low Speed GMLAN Serial Data
9 | -- | -- | Not Used
10 | -- | -- | Not Used
11 | D-GN | 5060 | Low Speed GMLAN Serial Data
12 | D-GN | 5060 | Low Speed GMLAN Serial Data

#### I/P Compartment Lamp - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | OG | 1732 | Glovebox Courtesy Lamp Supply Voltage

#### I/P Compartment Lamp - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-A | PU | 175 | Glove Box Lamp Control

#### I/P Compartment Lamp Switch - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circui Number | Function
X1-A | PU | 175 | Glove Box Lamp Control

#### I/P Compartment Lamp Switch - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-A | BK | 1450 | Ground

#### Knock Sensor (KS) Bank 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-BU | 496 | Knock Sensor 1 Signal
2 | GY | 1716 | Low Reference Knock Sensor Signal Return

#### Knock Sensor (KS) Bank 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-BU | 1876 | Knock Sensor 2 Signal
2 | BN | 407 | Low Reference Knock Sensor Signal Return

#### Knock Sensor (KS) Left (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-BU | 496 | Knock Sensor 1 Signal
2 | GY | 1716 | Low Reference Knock Sensor Signal Return

#### Knock Sensor (KS) Left (LS2) (HSV Maloo)

Connector Part Information | GT 150 Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | D-BU | 0.5 | Knock Sensor 1 Signal
2 | GY | 0.5 | Low Reference Knock Sensor Signal Return

#### Knock Sensor (KS) Right (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-BU | 1876 | Knock Sensor 2 Signal
2 | TN | 407 | Low Reference Knock Sensor S ignal Return

#### Knock Sensor (KS) Right (LS2) (HSV Maloo)

Connector Part Information | GT 150 Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | L-BU | 0.5 | Knock Sensor 2 Signal
2 | TN | 0.5 | Low Reference Knock Sensor Signal Return

#### License Lamp - Unit

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/WH | 309 | Lamp Supply Voltage
2 | BK | 1850 | Ground

#### Load Compartment Light (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OR | 1732 | Courtesy Lamps Supply Voltage
2 | BK | 0737 | Ground

#### Manifold Absolute Pressure (MAP) Sensor (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | GY | 2704 | 5-Volt Reference
2 | OG/BK | 469 | Low Reference
3 | L-GN | 432 | MAP Sensor Signal

#### Manifold Absolute Pressure (MAP) Sensor (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | OG/BK | 0.5 | Low Reference
B | L-GN | 0.5 | MAP Sensor Signal
C | GY | 0.5 | 5-Volt Reference

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LY7/L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | YE | 492 | MAF Sensor Signal
B | PK | 439 | Ignition 1 Voltage
C | BK | 450 | Ground
D | BN/RD | 472 | IAT Sensor Signal
E | BN/WH | 2760 | Low Reference

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LY7/LS2) (HSV Maloo)

Connector Part Information | GT 150 Sealed 4.0
--- | ---
Pin | Wire Colour | Wire Size | Function
A | YE | 0.5 | MAF Sensor Signal
B | PK | 0.5 | Ignition 1 Voltage
C | BK | 0.5 | Ground
D | BN/RD | 0.5 | IAT Sensor Signal
E | BN/WH | 0.5 | Low Reference

#### Mode Actuator - 1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN | 2273 | Mode Actuator 1 - Power
2 | BK | 119 | Mode Actuator 1 - Control
3 | BU | 1791 | Low Reference
4 | GY | 2275 | Mode Actuator 1 - Feedback
5 | GN | 474 | 5-Volt Reference

#### Mode Actuator - 2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-GN | 2210 | Mode Actuator 2 - Power
2 | OG | 1791 | Mode Actuator 2 - Control
3 | L-BU | 720 | Low Reference
4 | RD | 1199 | Mode Actuator 2 - Feedback
5 | PK | 1236 | 5-Volt Reference

#### Navigation Gateway Module

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BN | 0.3 | Navigation Display Serial Data High
2 | OG | 0.3 | Navigation Display Serial Data High
3 | OG | 0.85 | Mute Signal
4 | -- | -- | Not Used
5 | L-GN | 0.5 | Low Speed GMLAN Serial Data
6 | OG/WH | 0.85 | Battery Positive Voltage
7 | YE | 0.3 | Navigation Display Serial Data Low
8 | YE | 0.3 | Backlight Lamps Control
9 | -- | -- | Not Used
10 | -- | -- | Not Used
11 | -- | -- | Not Used
12 | BK/WH | 0.5 | Ground

#### Navigation Unit - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X1-A1 | -- | -- | Not Used
X1-A2 | -- | -- | Not Used
X1-A3 | -- | -- | Not Used
X1-A4 | OG/WH | 0.85 | Battery Positive Voltage
X1-A6 | YE | 0.3 | Backlight Lamps Control
X1-A7 | OG | 0.3 | Navigation Control Signal
X1-A8 | BK/WH | 0.85 | Ground

#### Navigation Module - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X2-A1 | -- | -- | Not Used
X2-A2 | -- | -- | Not Used
X2-A3 | -- | -- | Not Used
X2-A4 | -- | -- | Not Used
X2-A5 | PK/BK | 0.3 | Navigation Mono Audio Signal (+)
X2-A6 | OG/BK | 0.3 | Navigation Mono Audio Signal (-)
X2-A7 | -- | -- | Not Used
X2-A8 | -- | -- | Not Used

#### Navigation Module - X3

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X3-C1 | -- | -- | Not Used
X3-C2 | -- | -- | Not Used
X3-C3 | -- | -- | Not Used
X3-C4 | -- | -- | Not Used
X3-C4 | -- | -- | Not Used
X3-C5 | -- | -- | Not Used
X3-C6 | -- | -- | Not Used
X3-C7 | BN | 0.3 | Navigation Display Serial Data High
X3-C8 | YE | 0.3 | Navigation Display Serial Data Low
X3-C9 | -- | -- | Not Used
X3-C10 | -- | -- | Not Used
X3-C11 | -- | -- | Not Used
X3-C12 | -- | -- | Not Used
X3-C13 | -- | -- | Not Used
X3-C14 | -- | -- | Not Used
X3-C15 | -- | -- | Not Used
X3-C16 | -- | -- | Not Used
X3-C17 | -- | -- | Not Used
X3-C18 | -- | -- | Not Used
X3-C19 | -- | -- | Not Used
X3-C20 | -- | -- | Not Used

#### Navigation Module - X4

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X4-A1 | -- | -- | Not Used
X4-A2 | -- | -- | Not Used
X4-A3 | -- | -- | Not Used
X4-A4 | OG | 0.85 | Mute Signal
X4-A5 | -- | -- | Not Used
X4-A6 | -- | -- | Not Used
X4-A7 | -- | -- | Not Used
X4-A8 | -- | -- | Not Used
X4-A9 | -- | -- | Not Used
X4-A10 | -- | -- | Not Used

#### Navigation Module - X5

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X5-A | OG | 0.5 | Antenna Signal
X5-B | GY | 0.5 | Drain Wire

#### Navigation Module - X6

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X6-1 | RD | 0.3 | Video Connector - R
X6-2 | GN | 0.3 | Video Connector - G
X6-3 | WH | 0.3 | Video Connector - B
X6-4 | BK | 0.3 | Ground
X6-5 | YE | 0.3 | Video Connector - Sync
X6-6 | BK | 0.3 | Drain Wire

#### Navigation Module - X7

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X7-1 | WH | 0.3 | Video Connector - B
X7-2 | -- | -- | Not Used
X7-3 | RD | 0.3 | Video Connector - R
X7-4 | -- | -- | Not Used
X7-5 | -- | -- | Not Used
X7-6 | -- | -- | Not Used
X7-7 | -- | -- | Not Used
X7-8 | -- | -- | Not Used
X7-9 | -- | -- | Not Used
X7-10 | BK | 0.3 | Ground
X7-11 | GN | 0.3 | Video Connector - G
X7-12 | -- | -- | Not Used
X7-13 | YE | 0.3 | Video Connector - Sync
X7-14 | -- | -- | Not Used
X7-15 | -- | -- | Not Used
X7-16 | -- | -- | Not Used
X7-17 | -- | -- | Not Used
X7-18 | -- | -- | Not Used

#### Object Alarm Sensor - LR Corner (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | RD | 0.5 | Object Sensor Supply Voltage
2 | BK | 0.5 | Object Sensor Low Reference
3 | YE | 0.5 | LR Corner Object Sensor Signal

#### Object Alarm Sensor - LR Middle (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | RD | 0.5 | Object Sensor Supply Voltage
2 | BK | 0.5 | Object Sensor Low Reference
3 | OG | 0.5 | LR Middle Object Sensor Signal

#### Object Alarm Sensor - RR Corner (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | RD | 0.5 | Object Sensor Supply Voltage
2 | BK | 0.5 | Object Sensor Low Reference
3 | PU | 0.5 | RR Corner Object Sensor Signal

#### Object Alarm Sensor - RR Middle (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | RD | 0.5 | Object Sensor Supply Voltage
2 | BK | 0.5 | Object Sensor Low Reference
3 | D-GN | 0.5 | RR Middle Object Sensor Signal

#### Oil Pressure Gauge (HSV Maloo)

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Wire Size | Function
3 | YE | 0.3 | Low Speed GMLAN Serial Data
2 | BU | 0.3 | Ground
1 | BU / RE | 0.3 | Battery Positive Voltage
4 | YE | 0.3 | Low Speed GMLAN Serial Data
5 | BU | 0.3 | Ground
6 | BU / RE | 0.3 | Battery Positive Voltage

#### Oil Temperature Gauge (HSV Maloo)

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | YE | 0.3 | Low Speed GMLAN Serial Data
2 | BU | 0.3 | Ground
3 | BU / RE | 0.3 | Battery Positive Voltage
4 | YE | 0.3 | Low Speed GMLAN Serial Data
5 | BU | 0.3 | Ground
6 | BU / RE | 0.3 | Battery Positive Voltage

#### Outside Rear View Mirror - Left

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH/BU | 7391 | Left Mirror Motor Up/Left Control
2 | WH/BK | 81 | Left Mirror Motor Right Control
3 | -- | -- | Not Used
4 | L-GN/BK | 89 | Left Mirror Motor Down Control
5 | -- | -- | Not Used
6 | -- | -- | Not Used

#### Outside Rear View Mirror - Right

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH/BU | 7391 | Right Mirror Motor Up/Left Control
2 | OG/WH | 881 | Right Mirror Motor Right Control
3 | -- | -- | Not Used
4 | PU/WH | 889 | Right Mirror Motor Down Control
5 | -- | -- | Not Used
6 | -- | -- | Not Used

#### Park Brake Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
B | OG/BK | 233 | Park Brake Switch Signal

#### Park/Neutral Position (PNP) Switch (4L60E)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | OG/BK | 1786 | Park Neutral Signal
4 | YE | 772 | Transmission Range Switch Signal B
5 | BN/YE | 771 | Transmission Range Switch Signal A
6 | GY | 773 | Transmission Range Switch Signal C
7 | BK | 450 | Ground
8 | WH | 776 | Transmission Range Switch Signal P

#### Radio - X1 (Type A, B, C and D Infotainment System)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | -- | -- | Not Used
X1-2 | D-GN | 117 | Right Front Speaker Output (-)
X1-3 | GY | 118 | Left Front Speaker Output (-)
X1-4 | -- | -- | Not Used
X1-5 | -- | -- | Not Used
X1-6 | L-GN | 200 | Right Front Speaker Output (+)
X1-7 | BN | 201 | Left Front Speaker Output (+)
X1-8 | -- | -- | Not Used

#### Radio - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-9 | -- | -- | Not Used
X2-10 | OG/BU | 4340 | Battery Positive Voltage
X2-11 | -- | -- | Not Used
X2-12 | BK | 1050 | Ground
X2-13 | -- | -- | Not Used
X2-14 | OG/BU | 4340 | Battery Positive Voltage
X2-15 | OG/BU | 4340 | Battery Positive Voltage
X2-16 | BK | 1050 | Ground

#### Radio - X4

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X4-1 | L-BU | 1405 | Telephone Audio Signal (-)
X4-2 | -- | -- | Not Used
X4-3 | -- | -- | Not Used
X4-4 | -- | -- | Not Used
X4-5 | WH | 700 | Telephone Audio Signal Mute
X4-6 | D-GN | 5060 | Low Speed GMLAN Serial Data
X4-7 | OG/BK | 1405 | Telephone Audio Signal (+)
X4-8 | -- | -- | Not Used
X4-9 | -- | -- | Not Used
X4-10 | -- | -- | Not Used
X4-11 | -- | -- | Not Used
X4-12 | -- | -- | Not used

#### Radio - X5 AM/FM Antenna

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
C | GY | 6001 | Radio Antenna Post
S | Bare | 6015 | Radio Antenna Shield

#### Rear Object Alarm Module - X1 (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X1-1 | OG/PU | 0.85 | Battery Positive Voltage
X1-2 | YE | 0.3 | Object Detection Alarm Signal A
X1-3 | -- | -- | --
X1-4 | -- | -- | --
X1-5 | GY | 0.3 | Object Detection Alarm Signal B
X1-6 | D-GN | 0.3 | Low Speed GMLAN Serial Data
X1-7 | BK | 0.5 | Ground
X1-8 | -- | -- | --
X1-9 | -- | -- | --
X1-10 | -- | -- | --
X1-11 | -- | -- | --
X1-12 | -- | -- | --

#### Rear Object Alarm Module - X2 (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
X2-1 | PU | 0.3 | RR Corner Object Sensor Signal
X2-2 | D-GN | 0.3 | RR Middle Object Sensor Signal
X2-3 | OG | 0.3 | LR Middle Object Sensor Signal
X2-4 | D-BU | 0.3 | Object Sensor Supply Voltage
X2-5 | YE | 0.3 | LR Corner Object Sensor Signal
X2-6 | -- | -- | --
X2-7 | -- | -- | --
X2-8 | GY | 0.3 | Object Sensor Low Reference

#### Rear Object Alarm (HSV Maloo)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | YE | 0.3 | Object Detection Alarm Signal A
2 | GY | 0.3 | Object Detection Alarm Signal B

#### Rear Window Defogger Grid - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | PU | 293 | Rear Defog Element Supply Voltage

#### Rear Window Defogger Grid - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-A | BK | 1650 | Ground

#### Recirculation Actuator

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH/BU | 1614 | Recirculation Actuator - Control
2 | WH/BK | 2274 | Recirculation Actuator - Power
3 | BU/BK | 718 | Low Reference
4 | WH/RD | 1838 | Recirculation Actuator - Feedback
5 | WH/GN | 597 | 5-Volt Reference

#### Remote Function Actuator

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/WH | 1840 | Battery Positive Voltage
2 | D-GN | 5060 | Low Speed GMLAN Serial Data
3 | -- | -- | Not Used
4 | BK | 1650 | Ground

#### Repeater Lamp - Left

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 2050 | Ground
2 | YE/BK | 1334 | Left Rear Turn Signal Lamp Supply Voltage

#### Repeater Lamp - Right

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 1850 | Ground
2 | D-GN/WH | 1335 | Right Rear Turn Signal Lamp Supply Voltage

#### Reverse Lockout Solenoid (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | L-GN | 1652 | Reverse Lockout Solenoid Control
B | PK/BK | 5705 | Reverse Lockout Solenoid Battery Power

#### Reverse Lockout Solenoid (LS2) (HSV Maloo)

Connector Part Information | Metri-Pack 150 Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | L-GN | 07.5 | Reverse Lockout Solenoid Control
B | PK/BK | 0.75 | RAP [X] Fuse Supply Voltage

#### Seat Adjuster Switch - Driver

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | BN | -- | --
X1-2 | D-BU | -- | --
X1-3 | GN/YE | -- | --
X1-4 | D-BU/RD | -- | --
X1-5 | -- | -- | --
X1-6 | BK | -- | --
X1-7 | RD | -- | --
X1-8 | -- | -- | --

#### Seat Belt Pretensioner - LF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-GN | 2116 | Seat Belt Pretensioner - Passenger - High Control
2 | OG | 2117 | Seat Belt Pretensioner - Passenger - Low Control

#### Seat Belt Pretensioner - RF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK/WH | 2118 | Seat Belt Pretensioner - Driver - High Control
2 | OG/BK | 2119 | Seat Belt Pretensioner - Driver - Low Control

#### Seat Rear Vertical Motor - Driver

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1 | YE | 282 | Driver Seat Rear Vertical Motor Up Control
X2 | L-BU | 283 | Driver Seat Rear Vertical Motor Down Control

#### Secondary Information Center (SIC) Module - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 5060 | Low Speed GMLAN Serial Data
2 | -- | -- | --
3 | -- | -- | --
4 | RD/WH | 1840 | Battery Positive Voltage
5 | -- | -- | --
6 | -- | -- | --
7 | -- | -- | --
8 | BK | 1450 | Ground

#### Speaker - Center X1 (Type B and C Infotainment System)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | GY | 201 | Left Front Speaker Output (+)
X1-B | BN | 118 | Left Front Speaker Output (-)

#### Speaker - Center X2 (Type B and C Infotainment System)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-A | D-GN | 117 | Right Front Speaker Output (-)
X2-B | L-GN | 200 | Right Front Speaker Output (+)

#### Speaker - LF Door (Infotainment System)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | GY | 118 | Left Front Speaker Output (-)
2 | BN | 201 | Left Front Speaker Output (+)

#### Speaker - LF Tweeter (Type F Infotainment System)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | GY | 118 | Left Front Speaker Output (-)
2 | BN | 201 | Left Front Speaker Output (+)

#### Speaker - RF Door

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 117 | Right Front Speaker Output (-)
2 | L-GN | 200 | Right Front Speaker Output (+)

#### Speaker - RF Tweeter (Type F Infotainment System)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 117 | Right Front Speaker Output (-)
2 | L-GN | 200 | Right Front Speaker Output (+)

#### Starter

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | PU | 6 | Starter Solenoid Crank Voltage

#### Starter

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-A | RD | 1 | Battery Voltage

#### Steering Angle Sensor

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PU | 2501 | High Speed GMLAN Serial Data Bus-
2 | D-BU | 2501 | High Speed GMLAN Serial Data Bus-
3 | GY | 2500 | High Speed GMLAN Serial Data Bus+
4 | BN | 2500 | High Speed GMLAN Serial Data Bus+
5 | L-GN | 5986 | Communication Enable Relay Supply Voltage
6 | OG | 2688 | Steering Wheel Position Sensor Low Reference

#### Steering Angle Sensor (HSV Maloo)

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BN | 0.35 | High Speed GMLAN Serial Data Bus-
2 | BN | 0.35 | High Speed GMLAN Serial Data Bus-
3 | BN/BK | 0.35 | High Speed GMLAN Serial Data Bus+
4 | BN/BK | 0.35 | High Speed GMLAN Serial Data Bus+
5 | L-BU | 0.5 | Communication Enable Relay Supply Voltage
6 | BK/BU | 0.5 | Steering Wheel Position Sensor Low Reference

#### Steering Wheel Controls Switch Assembly

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | GY/BU | 7367 | Steering Wheel Resistor Ladder Right Signal #2
X1-2 | YE | 7364 | Steering Wheel Resistor Ladder Right Signal #1
X1-3 | BN | 7312 | Steering Wheel Resistor Ladder Left Signal #1
X1-4 | L-BU | 7313 | Steering Wheel Resistor Ladder Left Signal #2
X1-5 | GN | 897 | Steering Wheel Controls Low Reference
X1-6 | OG/BK | 5201 | Steering Wheel Controls Signal
X1-7 | BK | 850 | Ground
X1-8 | PU | 7005 | I/P Dimming Control

#### Sunshade - Left (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BK/WH | 0.5 | Ground
2 | OG | 0.5 | Courtesy Lamps Supply Voltage

#### Sunshade - Right (HSV Maloo)

Connector Part Information | Metri-Pack 150 Series
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BK/WH | 0.5 | Ground
2 | OG | 0.5 | Courtesy Lamps Supply Voltage

#### Tail Lamp Assembly - Left

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK/WH | 1851 | Ground
2 | BK | 1850 | Ground
3 | PU | 709 | Left Park Lamp Supply Voltage
4 | L-BU | 20 | Stop Lamp Switch Signal
5 | L-GN | 24 | Backup Lamp Supply Voltage
6 | YE/BK | 1334 | Left Rear Turn Signal Lamp Supply Voltage

#### Tail Lamp Assembly - Right

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK/WH | 1851 | Ground
2 | BK | 1850 | Ground
3 | BN/WH | 309 | Right Park Lamp Supply Voltage
4 | L-BU | 20 | Stop Lamp Switch Signal
5 | L-GN | 24 | Backup Lamp Supply Voltage
6 | D-GN/WH | 1335 | Right Rear Turn Signal Lamp Supply Voltage

#### Theft Deterrent Control Module

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/BK | 1040 | Battery Positive Voltage
2 | BN | 4 | Ignition 1 Voltage
3 | BK | 850 | Ground
4 | -- | -- | Not Used
5 | D-GN | 5060 | Low Speed GMLAN Serial Data

#### Theft Horn X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-A | D-GN | 1149 | Content Theft Horn Control

#### Theft Horn X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-A | BK | 1250 | Ground

#### Throttle Body (L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN | 582 | TAC Motor Control - 2
B | YE | 581 | TAC Motor Control - 1
C | BN/BK | 2752 | Low Reference
D | D-GN | 485 | TP Sensor 1 Signal
E | GY | 2701 | 5-Volt Reference
F | PU | 486 | TP Sensor 2 Signal

#### Throttle Body (LS2) (HSV Maloo)

Connector Part Information | GT 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN | 0.75 | TAC Motor Control - 2
B | YE | 0.75 | TAC Motor Control - 1
C | BN/BK | 0.5 | Low Reference
D | D-GN | 0.5 | TP Sensor 1 Signal
E | GY | 0.5 | 5-Volt Reference
F | PU | 0.5 | TP Sensor 2 Signal

#### Throttle Body (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN | 582 | TAC Motor Control - 2
B | YE | 581 | TAC Motor Control - 1
C | BN/BK | 2752 | Low Reference
D | D-GN | 485 | TP Sensor 1 Signal
E | GY | 2701 | 5-Volt Reference
F | PU | 486 | TP Sensor 2 Signal

#### Transmission Control Module (TCM) - 5L40E

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-GN/BK | 822 | VSS Low Signal
2 | OG/BK | 1786 | Park/Neutral Signal
3 | PU/WH | 821 | VSS High Signal
4 | BN | 418 | TCC PWM Solenoid Valve Control
5 | D-BU | 5985 | TCM Accessory Signal
6 | BK | 450 | Ground
7 | -- | -- | Not Used
8 | OG | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control
9 | PK | 439 | Ignition 1 Voltage
10 | OG | 1983 | Transmission Turbine Speed Switch Signal
11 | L-BU | 1984 | Transmission Turbine Speed Switch Low Reference
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | -- | -- | Not Used
15 | YE/BK | 1227 | TFT Sensor Signal
16 | -- | -- | Not Used
17 | -- | -- | Not Used
18 | YE/BK | 1223 | Shift Solenoid B Valve Control
19 | WH | 898 | Shift Solenoid C Valve Control
20 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
21 | BN | 2501 | High Speed GMLAN Serial Data Bus-
22 | -- | -- | Not Used
23 | -- | -- | Not Used
24 | YE | 772 | Transmission Range Switch Signal B
25 | GY | 773 | Transmission Range Switch Signal C
26 | BN/WH | 2762 | Low Reference
27 | OG/YE | 3640 | Battery Positive Voltage
28 | -- | -- | Not Used
29 | L-BU/WH | 1229 | PC Solenoid Valve Low Control
30 | L-GN | 1222 | Shift Solenoid A Valve Control
31 | -- | -- | Not Used
32 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
33 | BN | 2501 | High Speed GMLAN Serial Data Bus-
34 | -- | -- | Not Used
35 | -- | -- | Not Used
36 | BN/YE | 771 | Transmission Range Switch Signal A
37 | WH | 776 | Transmission Range Switch Signal P
38 | WH/BU | 17 | Stop Lamp Switch Signal
39 | -- | -- | Not Used
40 | -- | -- | Not Used
41 | -- | -- | Not Used
42 | -- | -- | Not Used

#### Turn Signal Multifunction Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 1850 | Ground
2 | BN/RD | 1356 | Flash To Pass Switch Signal
3 | PU/YE | 524 | Headlamp Dimmer Switch High Beam Signal
4 | BK | 850 | Ground
5 | GY | 1884 | Cruise Control Switch Signal
6 | PU | 1317 | Steering Wheel Control Supply Voltage
7 | D-BU/WH | 1415 | Right Front Turn Signal Switch Signal
8 | L-BU/WH | 1414 | Left Front Turn Signal Switch Signal

#### Variable Intake Manifold (VIM) Solenoid (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PU/BU | 5293 | Ignition 1 Voltage
2 | BN | 1997 | 1997 Ether Solenoid - Feed

#### Wheel Speed Sensor (WSS) - LF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN | 830 | Wheel Speed Sensor Signal Left Front
2 | BK | 7064 | Wheel Speed Sensor Supply Voltage Left Front

#### Wheel Speed Sensor (WSS) - LR

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/BK | 884 | Wheel Speed Sensor Signal Left Rear
2 | GY | 7127 | Wheel Speed Sensor Supply Voltage Left Rear

#### Wheel Speed Sensor (WSS) - RF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN | 872 | Wheel Speed Sensor Signal Right Front
2 | BK | 7065 | Wheel Speed Sensor Supply Voltage Right Front

#### Wheel Speed Sensor (WSS) - RR

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN | 882 | Wheel Speed Sensor Signal Right Rear
2 | GY | 7128 | Wheel Speed Sensor Supply Voltage Right Rear

#### Window/Door Lock/Outside Rear-view Mirror Switch - X1

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X1-1 | -- | -- | Not Used
X1-2 | -- | -- | Not Used
X1-3 | -- | -- | Not Used
X1-4 | -- | -- | Not Used
X1-5 | -- | -- | Not Used
X1-6 | -- | -- | Not Used
X1-7 | -- | -- | Not Used
X1-8 | -- | -- | Not Used
X1-9 | -- | -- | Not Used
X1-10 | D-GN | 1001 | RAP [X] Fuse Supply Voltage
X1-11 | BK | 1307 | Power Window Master Switch Lockout Control
X1-12 | -- | -- | Not Used
X1-13 | -- | -- | Not Used

#### Window/Door Lock/Outside Rear-view Mirror Switch - X2

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
X2-1 | D-GN | 1301 | RAP [X] Fuse Supply Voltage
X2-2 | BN | 1300 | Power Window Master Switch Left Front Up Signal
X2-3 | GY/BU | 1136 | Power Window Master Switch Left Front Down Signal
X2-4 | BK | 2050 | Ground
X2-5 | BN/BK | 254 | Power Door Unlock Fuse Supply Voltage
X2-6 | WH/BK | 81 | Left Mirror Switch Right Signal
X2-7 | L-GN/BK | 89 | Left Mirror Motor Down Control
X2-8 | WH/BU | 7391 | Mirror Motor up/left Control
X2-9 | L-BU | 166 | Power Window Master Switch Right Front Up Signal
X2-10 | GN/BK | 167 | Power Window Master Switch Right Front Down Signal
X2-11 | YE | 6817 | LED Backlight Dimming Control
X2-12 | PU/WH | 889 | Right Mirror Motor Down Control
X2-13 | OG/WH | 881 | Right Mirror Motor Right Control
X2-14 | BK | 2050 | Ground
X2-15 | GY/BK | 255 | Power Door Lock Fuse Supply Voltage
X2-16 | BN/BU | 343 | Switch Voltage

#### Window Motor - LF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN/OG | 165 | Power Window Motor Left Front Down Control
B | D-BU | 164 | Power Window Motor Left Front Up Control

#### Window Motor - RF

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BN | 667 | Power Window Motor Right Front Down Control
B | BU/WH | 666 | Power Window Motor Right Front Up Control

#### Windshield Washer Fluid Pump

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG | 228 | Windshield Washer Pump Control
2 | BK | 250 | Ground

#### Windshield Wiper Motor

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | YE | 196 | Windshield Wiper Motor Park Switch Signal
2 | BK | 250 | Ground
3 | BN/WH | 92 | Windshield Wiper Motor High Speed
4 | D-GN | 95 | Windshield Wiper Motor Low Speed

#### Windshield Wiper/Washer Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | L-GN | 1715 | Windshield Wiper Switch High Signal
5 | -- | -- | Not Used
6 | OG | 94 | Windshield Wa sher Switch Signal
7 | L-BU | 1714 | Windshield Wiper Switch Low Signal
8 | BK/WH | 2151 | Ground

#### Yaw Rate and Lateral Acceleration Sensor

Connector Part Information |
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 2087 | 5-V Reference
2 | L-GN/BK | 5352 | Yaw Rate Sensor Test Control
3 | L-BU | 5986 | Communication Enable Relay Supply Voltage
4 | BN/WH | 2086 | Yaw Rate Signal
5 | PU/WH | 1699 | Combined Vehicle Inertial Sensor Signal (Lat/Long Rate)
6 | BK/BU | 2088 | Low Reference