For 1990-2009 cars

#### Tools Required

J 41479 Crankshaft Rear Oil Seal Installer

### Removal Procedure

1. Remove the engine flywheel. Refer to Engine Flywheel Replacement.
2. Gently pry the crankshaft rear oil seal (1) from the rear cover (2).

### Installation Procedure

1. Install the crankshaft rear seal. Refer to Crankshaft Rear Oil Seal Installation.
2. Install the engine flywheel. Refer to Engine Flywheel Replacement.