For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the General Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Suspension General Diagnosis .
2 | Verify the vehicle leans or sways in corners. Does the vehicle operate normally? | System OK | Go to Step 3
3 | Inspect the following components for wear or damage:

• | The front coil springs

• | The rear coil springs

Are the components worn or damaged?

Go to Step 7

Go to Step 4

4 | Inspect the stabiliser bar links for wear or damage. Are the stabiliser bar links worn or damaged? | Go to Step 8 | Go to Step 5
5 | Inspect the stabiliser bar insulators for wear or damage. Are the stabiliser bar insulators worn or damaged? | Go to Step 9 | Go to Step 6
6 | Inspect the stabiliser bars for wear or damage. Are the stabiliser bars worn or damaged? | Go to Step 10 | Go to Strategy Based Diagnosis .
7 | Replace the springs. Refer to the appropriate procedure:

• | Front Coil Springs Replacement for Front.

• | Coil Spring Replacement for Rear.

Did you complete the repair?

Go to Step 11

--

8 | Replace the stabiliser bar link(s). Refer to Stabilizer Shaft Link Replacement for Front or Stabilizer Shaft Link Replacement for Rear. Did you complete the repair? | Go to Step 11 | --
9 | Replace the stabiliser bar Insulators. Refer to Stabilizer Shaft Insulator Replacement for Front or Stabilizer Shaft Insulator Replacement for Rear . Did you complete the repair? | Go to Step 11 | --
10 | Replace the stabiliser bar. Refer to Stabilizer Shaft Replacement for Front or Stabilizer Shaft Replacement for Rear. Did you complete the repair? | Go to Step 11 | --
11 | Operate the vehicle in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3