For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 44 N·m | 32 lb ft
Bearing Lock Plate Bolt | 11 N·m | 97 lb in
Drain Plug | 37 N·m | 27 lb ft
Drive Flange Nut | 57 N·m | 42 lb ft
Fill Plug | 37 N·m | 27 lb ft
Front Case to Middle Case Bolts | 40 N·m | 29 lb ft
Middle Case to Rear Case Bolts | 40 N·m | 30 lb ft
Oil Through Bolts | 8 N·m | 71 lb in
Rear Case to Housing Extension Bolts | 29 N·m | 21 lb ft
Reverse Idler Shaft Bolt | 28 N·m | 20 lb ft
Service Hole Plug | 39 N·m | 29 lb ft
Shift Control Assembly Bolt | 18 N·m | 13 lb ft
Shift Control Lever Bracket Bolts | 21 N·m | 15 lb ft
Shift Fork Bolts | 19 N·m | 14 lb ft
Shift and Select Lever Bolt | 33 N·m | 24 lb ft
Shift Shaft Detent Plug | 24 N·m | 18 lb ft
Speed Sensor Bolt | 8 N·m | 71 lb in
Transmission Bolt | 50 N·m | 37 lb ft
Transmission Mount Bolt | 60 N·m | 44 lb ft