For 1990-2009 cars

Figure 1: |

#### Engine Grounds (LY7)

(1) | Ground Engine Block -- G107
(2) | Ground Engine Block -- G109
(3) | Ground Engine -- G106

Figure 2: |

#### Engine Grounds (L98)

(1) | Ground Engine -- G112
(2) | Ground Engine -- G110

Figure 3: |

#### Battery Wiring (LY7)

(1) | Fuse Block Underhood -- X124
(2) | ABS Bracket Ground -- G103
(3) | Engine Block Ground -- G108
(4) | Starter -- M15
(5) | Jumpstart Positive Stud -- G104
(6) | Dash Panel Grommet / Stud
(7) | Generator Connector -- G8-X2

Figure 4: |

#### Battery Wiring (L98)

(1) | Fuse Block - Underhood -- X124
(2) | ABS Bracket Ground -- G103
(3) | Engine Block Ground -- G111
(4) | Starter -- M15
(5) | Jumpstart Positive Stud -- G104
(6) | Dash Panel Grommet / Stud
(7) | Generator Connector -- G8-X2

Figure 5: |

#### Battery Wiring

(1) | Ground Chassis Fender -- G104 (Jumpstart Negative post)
(2) | Ground Chassis Rail Right -- G101

Figure 6: |

#### Body Wiring

(1) | Inflatable Restraint Sensing and Diagnostic Module -- A65-X2
(2) | Inflatable Restraint Sensing and Diagnostic Module -- A65-X1
(3) | SDM Bracket Ground -- G308

Figure 7: |

#### Instrument Panel Wiring

(1) | Body Front Wiring Connector 5 -- X207
(2) | Body Front Wiring Connector 4 -- X204
(3) | Body Front Wiring Connector 3 -- X200
(4) | Right Hand Body Wiring Connector 1 -- X201
(5) | Right Cockpit Endplate Ground -- G201
(6) | Right Hand Body Wiring Connector 3 -- X254
(7) | Right Hand Body Wiring Connector 2 -- X253