For 1990-2009 cars

### Point-to-Point Measurements

Location | Description | Length
--- | --- | ---
A | Upper Top Door Hinge Hole to Upper Door Striker Hole | 1085 mm (42.72 in)
B | Hinge Pillar Datum Hole to Upper Door Striker Hole | 1174 mm (46.22 in)
C | Lower Bottom Door Hinge Hole to Upper Door Striker Hole | 1088 mm (42.83 in)
D | Hinge Pillar Datum Hole to Upper Door Hinge Hole | 88 mm (3.46 in)
E | Lower Door Striker Hole to Lower Body Side Extension Datum Hole | 1732 mm (68.20 in)
All dimensions are measured from a zero line, a centre line and a common datum. All dimensions are symmetrical unless otherwise specified.

### Dimensions - Underbody

Location | Description | Length | Width | Height
--- | --- | --- | --- | ---
1 | Zero Line 18 mm Hole | 1535 mm (60.43 in) | 810 mm (31.89 in) | 128 mm (5.04 in)
A | 20 mm Hole | 805 mm (31.69 in) | 886 mm (34.88 in) | 328 mm (12.91 in)
B | 10 mm Bumper Mounting | 1136 mm (44.72 in) | 0 | 0
C | 16 mm Hole | 2140 mm (84.25 in) | 1024 mm (40.31 in) | 200 mm (7.87 in)
D | 25.1 mm x 39.7 mm Gage Hole | 2910 mm (114.57 in) | 1024 mm (40.31 in) | 198 mm (7.80 in)
E | 25.1 mm x 39.7 mm Gage Hole | 3114 mm (122.60 in) | 1048 mm (41.26 in) | 432 mm (17.01 in)
F | 18 mm Hole | 3335 mm (131.30 in) | 1048 mm (41.26 in) | 432 mm (17.01 in)
All dimensions are measured from a zero line, a centre line and a common datum. All dimensions are symmetrical unless otherwise specified.