For 1990-2009 cars

#### Tools Required

• | J 45004 Fuel Tank Drain Hose

• | J 42960-2 Fuel Flapper Door Holder

Caution: Never drain or store fuel in an open container. Always use an approved fuel storage container in order to reduce the chance of fire or explosion.

Notice: Do not run the fuel pump unless the fuel pump is submerged in fuel in order to prevent damage to the fuel pump.

1. Remove the fuel filler cap.
2. Install the J 42960-2 into the fuel fill pipe in order to hold the door open.
3. Insert the J 45004 into the fuel tank until the hose reaches the bottom of the fuel tank.
4. Use an air operated pump device in order to drain as much fuel through the fuel fill pipe as possible.