For 1990-2009 cars

## Clutch Rattle RHD

Cause | Action
--- | ---
DEFINITION: A rattle noise coming from the clutch components with the clutch disengaged or engaged. Review the Symptoms - Clutch .
Idle rattle clutch engaged | Replace the engine flywheel, due to faulty damper springs. Refer to the following procedures:

• | Engine Flywheel Replacement .

• | Clutch Assembly Replacement .

Clutch is incorrectly installed | Replace the clutch assembly. Refer to Clutch Assembly Replacement .
Clutch disc splines and transmission input shaft splines worn |

1. Inspect the clutch disc hub to transmission input shaft splines for excessive clearance.
2. Replace the clutch assembly if the clutch splines are worn. Refer to Clutch Assembly Replacement .
3. Replace the transmission input shaft. Refer to Transmission Disassemble for 3.6L Engines or Transmission Disassemble for 6.0L Engines.