For 1990-2009 cars

Description | Specifications
--- | ---
Steel Wheels
Rim Width Code | 7J
Diameter Code | 16
Maximum Permissible Radial Runout All Steel Wheels | 0.7 mm
Offset | 43 mm (positive)

### Alloy Wheel Specifications - Except HSV Maloo

Description | Specifications
--- | ---
Alloy Wheels
Rim Width Code | 8J
Diameter Code | 18, 19
Maximum Permissible Radial Runout All Models | 0.4 mm
Offset
18" x 8", 19" x 8" | 48 mm (positive)

### Alloy Wheel Specifications - HSV Maloo

Description | Specifications
--- | ---
Alloy Wheels
Rim Width Code | 8J | 9.5J
Diameter Code | 19 | 20
Maximum Permissible Radial Runout All Models | 0.4 mm
Offset
19" x 8" , 20" x 8" | 48 mm (positive)
19" x 9.5", 20" x 9.5" | 57 mm (positive)

### Inflation Pressure Specifications - Except HSV Maloo

Model | Engine | Wheel | Tire Designation | Recommended Cold Inflation
--- | --- | --- | --- | ---
Up to 2 Passengers | Up to Max. Load
Front | Rear | Front | Rear
Ute | V6 | 7J x 16 steel | 225/60 R16 102H | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 270 kPa | 39 PSI
SV6 | V6 | 8J x 18 alloy | 245/45 R18 96V | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 270 kPa | 39 PSI
SS | V8 | 8J x 18 alloy | 245/45 R18 96V | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 270 kPa | 39 PSI
SS-V | V8 | 8J x 19 alloy | 245/40 R19 94W | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 270 kPa | 39 PSI
Temporary use spare | 17 x 4 | T155/80 R17 111M | 420
For speeds above 160 km/h | 250 kPa | 36 PSI | 250 kPa | 36 PSI | 270 kPa | 39 PSI | 300 kPa | 43 PSI

### Inflation Pressure Specifications - HSV Maloo

Model | Engine | Wheel | Tyre Designation | Recommended Cold Inflation kPa
--- | --- | --- | --- | ---
Up to 3 Passengers | Up to Max. Load
Front | Rear | Front | Rear
Maloo | V8 | 8.0J x 19 alloy | 245/40 ZR19 98Y | 250 | 250 | 250 | 270
Maloo | V8 | 9.5J x 19 alloy | 275/35 ZR19 96Y | 250 | 250 | 250 | 270
Maloo Spare | V8 | 8.0J x 19 alloy | 245/40 ZR19 98Y | 300
Maloo | V8 | 8.0J x 20 alloy | 245/35 ZR20 95Y | 250 | 250 | 250 | 270
Maloo | V8 | 9.5J x 20 alloy | 275/30 ZR20 97Y | 250 | 250 | 250 | 270
Maloo Spare | V8 | 8.0J x 20 alloy | 245/35 ZR20 95Y | 300