For 1990-2009 cars

### Removal Procedure

1. Remove the seats. Refer to Front Seat Replacement - Bucket .
2. Remove the door sill plate trim. Refer to Door Sill Plate Replacement .
3. Remove the centre pillar lower trim. Refer to Center Pillar Lower Trim Panel Replacement .
4. Remove the centre pillar upper trim. Refer to Center Pillar Upper Trim Panel Replacement .
5. Remove the child restraint anchor. Refer to Child Restraint Tether Anchor Replacement .
6. Remove the front floor console. Refer to Front Floor Console Replacement .
7. Lift the rear window shelf trim panel lower access flaps (1).
8. From the passenger side, holding the access flap upward, remove the rear window shelf trim panel to body retaining screws (1).
9. From the drivers side, holding the access flap upward, remove the rear window shelf trim panel to body retaining screws (1).

Important: The rear window shelf trim panel retainers are a single use item and must be discarded after use.

Important: Pull on the rear window shelf trim panel to disengage the retainers.

10. Remove the rear window shelf trim panel (1).

Discard the retainers.

### Installation Procedure

Important: Push on the rear window shelf trim panel to engage the NEW retainers.

1. Install the rear window shelf trim panel (1).

Notice: Refer to Fastener Notice in the Preface section.

2. From the drivers side, holding the access flap upward, install the rear window shelf trim panel to body retaining screws (1).

Tighten
Tighten the retaining screws to 2.0 N·m (18 lb in).

Notice: Refer to Fastener Notice in the Preface section.

3. From the passenger side, holding the access flap upward, install the rear window shelf trim panel to body retaining screws (1).

Tighten
Tighten the retaining screws to 2.0 N·m (18 lb in).

4. Install the front floor console. Refer to Front Floor Console Replacement .
5. Install the child restraint anchor. Refer to Child Restraint Tether Anchor Replacement .
6. Install the centre pillar upper trim. Refer to Center Pillar Upper Trim Panel Replacement .
7. Install the centre pillar lower trim. Refer to Center Pillar Lower Trim Panel Replacement .
8. Install the door sill plate trim. Refer to Door Sill Plate Replacement .
9. Install the seats. Refer to Front Seat Replacement - Bucket .