For 1990-2009 cars

Component | Application | Specification
--- | --- | ---
Brake Fluid | Type Capacity | DOT 4 or Super DOT 4 0.9 Litres (0.791 quarts)
Brake Booster | Make Type Size | Mando Corporation Tandem Vacuum Suspended 203 mm (8 in) or 229 mm (9 in)
Master Cylinder | Type Bore Size Nominal Stroke | Fore/aft split 26 mm (1.023 in) 37 mm (1.456 in)
Brake Pedal Travel | Maximum Specification with 445 Nm (100 lbs) of force applied to the pedal with the ignition OFF and the booster power reserve depleted. | 90 mm (3.54 in)