For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Seat Belt Lower Anchor to Body Retaining Bolt | 43 N·m | 32 lb ft
Seat Belt Retractor to Pillar Retaining Bolts | 43 N·m | 32 lb ft
Seat Upper Guide to Body Retaining Bolt (Adjustable D-ring) | 43 N·m | 32 lb ft
Seat Intermediate Guide to Pillar Retaining Screws | 3 N·m | 27 lb in
Seat Belt Height Adjuster to Pillar Retaining Bolts | 30 N·m | 22 lb ft