For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Bolt M5 x 73 (Qty: 6) Important: Do not remove all the bolts in the control valve body assembly. Remove only the bolts indicated.

#### Special Tool

DT-48285 Valve Body Torx Plus Socket (if applicable)

2 | Control Valve Body Assembly Notice: Use care when handling the control valve body assembly. If dropped, damage to the control solenoid valve body assembly internal components, including the transmission control module (TCM), may result.
3 | Important: Do not reuse the seals. Replace with NEW seals. Reusing old seals may cause transmission damage. Fluid Pump Seal Assembly
4 | Important: Do not reuse the seals. Replace with NEW seals. Reusing old seals may cause transmission damage. Fluid Pump Seal Assembly
5 | Important: Do not reuse the seals. Replace with NEW seals. Reusing old seals may cause transmission damage. Center Support Fluid Passage Seal Assembly