For 1990-2009 cars

Application | Specification | Specification
--- | --- | ---
Metric | Imperial
Defrost Mode Actuator to HVAC Module Assembly Retaining Screws | 1 N·m | 9 lb in
Air Mix Actuator to HVAC Module Assembly Retaining Screws | 1 N·m | 9 lb in
Face/Floor Mode Actuator to HVAC Module Assembly Retaining Screws | 1 N·m | 9 lb in
HVAC Control Module to HVAC Module Assembly Retaining Screws | 2 N·m | 18 lb in
Recirculation Actuator to Air Inlet Assembly Retaining Screws | 1 N·m | 9 lb in