For 1990-2009 cars

## Engine Controls Connector End Views w/o Throttle Actuator Control

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position (CKP) Sensor
Table 3: | Engine Coolant Temperature (ECT) Sensor
Table 4: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Table 5: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve
Table 6: | Exhaust Gas Recirculation (EGR) Valve
Table 7: | Fuel Injector 1
Table 8: | Fuel Injector 2
Table 9: | Fuel Injector 3
Table 10: | Fuel Injector 4
Table 11: | Fuel Pump
Table 12: | Heated Oxygen Sensor 1 (HO2S1)
Table 13: | Heated Oxygen Sensor 2 (HO2S2)
Table 14: | Heated Oxygen Sensor 2 (HO2S2) (Mexico,Japan)
Table 15: | Idle Air Control (IAC) Valve
Table 16: | Ignition Coil (IC) Module
Table 17: | Intake Air Temperature (IAT) Sensor
Table 18: | Intake Manifold Tuning Valve Solenoid
Table 19: | Knock Sensor (KS)
Table 20: | Manifold Absolute Pressure (MAP) Sensor
Table 21: | Rough Road Sensor
Table 22: | Throttle Position (TP) Sensor

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | KET MG 640541

• | 3-Way F ITC (Injector Connector) Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 1846 | Ignition 1 Voltage
2 | BK/WH | 251 | Ground
3 | PU (BN/WH) | 633 | Camshaft Position (CMP) Sensor Signal

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way JR Power Timer 3P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
2 | YE/BK | 1868 | Low Reference
3 | BK/WH | 51 | Ground

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | PED 12040753

• | 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK (BK/YE) | 808 | Low Reference
B | L-GN (YE) | 410 | Engine Coolant Temperature (ECT) Sensor Signal

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | PED 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 1846 | Ignition 1 Voltage
2 | WH | 428 | Evaporative Emission (EVAP) Canister Purge Solenoid Control

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

Connector Part Information |

• | PED 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 1846 | Ignition 1 Voltage
2 | L-BU/PU | 428 | Evaporative Emission (EVAP) Canister Vent Solenoid Control

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | PED 12186139

• | 5-Way F Metri-Pack 150 Series Sealed, Pull To Seat (L-GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 435 | Exhaust Gas Recirulation (EGR) Solenoid Low Control
2 | OG/BK | 469 | Low Reference
3 | WH/BK | 1456 | Exhaust Gas Recirulation (EGR) Valve Position Signal
4 | L-BU/BK | 1688 | 5-Volt Reference
5 | GY | 120 | Fuel Pump Supply Voltage

#### Fuel Injector 1

Connector Part Information |

• | PED 15326181

• | 2-Way F Micro-Pack 064 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE/BU (BK) | 1744 | Fuel Injector 1 Control
B | PK | 139 | Ignition 1 Voltage

#### Fuel Injector 2

Connector Part Information |

• | PED 15326181

• | 2-Way F Micro-Pack 064 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN/WH (L-GN/BK) | 1745 | Fuel Injector 2 Control
B | PK | 139 | Ignition 1 Voltage

#### Fuel Injector 3

Connector Part Information |

• | PED 15326181

• | 2-Way F Micro-Pack 064 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-GN/BK (PK/BK) | 1746 | Fuel Injector 3 Control
B | PK | 139 | Ignition 1 Voltage

#### Fuel Injector 4

Connector Part Information |

• | PED 15326181

• | 2-Way F Micro-Pack 064 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-GN/WH (L-BU/BK) | 844 | Fuel Injector 4 Control
B | PK | 139 | Ignition 1 Voltage

#### Fuel Pump

Connector Part Information |

• | AMP 936039

• | 6-Way Fuel Pump 6POS CONN'R ASS'Y

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU | 1936 | Fuel Level Sensor Signal
2 | BK | 1250 | Ground
3 | GY | 120 | Fuel Pump Supply Voltage
4 | BK | 1250 | Ground
5 | PU | 172 | Low Fuel Indicator Control
6 | PU/BK | 632 | Low Reference

#### Heated Oxygen Sensor 1 (HO2S1)

Connector Part Information |

• | PED 12162144

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/RD | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
2 | PK/BK | 1846 | Ignition 1 Voltage
3 | GY | 1653 | Heated Oxygen Sensor (HO2S) 1 Signal
4 | BN/WH | 1669 | Heated Oxygen Sensor (HO2S) 1 Heater Control

#### Heated Oxygen Sensor 2 (HO2S2)

Connector Part Information |

• | AMP 174257-2

• | 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
2 | PK/BK | 1846 | Ignition 1 Voltage
3 | L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference
4 | BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control

#### Heated Oxygen Sensor 2 (HO2S2) (Mexico,Japan)

Connector Part Information |

• | AMP 174257-2

• | 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 1846 | Ignition 1 Voltage
2 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
3 | BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
4 | L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | PED 12040754

• | 4-Way F Black Metri-Pack 150 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH | 444 | Idle Air Control (IAC) Coil B Low Control
B | PU/WH | 1749 | Idle Air Control (IAC) Coil B High Control
C | YE/WH | 1748 | Idle Air Control (IAC) Coil A Low Control
D | BN | 1747 | Idle Air Control (IAC) Coil A High Control

#### Ignition Coil (IC) Module

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-BU | 406 | Ignition Coil (IC) Timing Control (1 and 4)
B | PK | 739 | Ignition 1 Voltage
C | D-GN/WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | AMP 85202-1

• | 2-Way JR Power Timer 2P Hsg Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 808 | Low Reference
2 | GY (BN) | 472 | Intake Air Temperature (IAT) Sensor Signal

#### Intake Manifold Tuning Valve Solenoid

Connector Part Information |

• | AMP 174352-2

• | 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
2 | PK/D-BU | 539 | Ignition 1 Voltage

#### Knock Sensor (KS)

Connector Part Information |

• | AMP 368215-1

• | 3-Way JPT 3P Ass'y for Knock Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE/BK | 496 | Knock Sensor (KS) Signal
2 | D-BU/WH | 808 | Low Reference
3 | BK/WH | 51 | Ground

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | AMP 174359-2

• | 3-Way F 070 Series Econoseal Mark-2 Cap 3P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU/BK | 1688 | 5-Volt Reference
2 | D-BU/WH (L-GN) | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
3 | OG/BK | 469 | Low Reference

#### Rough Road Sensor

Connector Part Information |

• | PED 12162185

• | 3-Way Metri-Pack 150.2 Series Sealed, Pull To Seat (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GY | 605 | 5-Volt Reference
B | D-GN | 602 | Rough Road Sensor Signal
C | PU/WH | 632 | Low Reference

#### Throttle Position (TP) Sensor

Connector Part Information |

• | PED 12065287

• | 3-Way F Metri-Pack 150 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-GN/WH (D-GN/YE) | 416 | 5-Volt Reference
B | BK | 808 | Low Reference
C | GY (D-BU) | 417 | Throttle Position (TP) Sensor Signal