For 1990-2009 cars

Table 1: | Ashtray Lamp
Table 2: | Back Up Lamp - Left
Table 3: | Back Up Lamp - Right
Table 4: | Center High Mounted Stop Lamp (CHMSL) Hatchback
Table 5: | Battery Saver
Table 6: | Center High Mounted Stop Lamp (CHMSL) Notchback
Table 7: | Daytime Running Lamp (DRL) Module (North America)
Table 8: | Daytime Running Lamp (DRL) Relay (North America)
Table 9: | Daytime Running Lamp (DRL) Module (Scandinavia)
Table 10: | Daytime Running Lamp (DRL) Relay 1 (Scandinavia)
Table 11: | Daytime Running Lamp (DRL) Relay 2 (Scandinavia)
Table 12: | Dome Lamp w/Dimmer
Table 13: | Dome Lamp w/o Dimmer
Table 14: | Door Ajar Switch - Left Front
Table 15: | Door Ajar Switch - Left Rear
Table 16: | Door Ajar Switch - Right Front
Table 17: | Door Ajar Switch - Right Rear
Table 18: | Fog Lamp - Left Front
Table 19: | Fog Lamp - Right Front
Table 20: | Fog Lamp - Left Rear
Table 21: | Fog Lamp - Right Rear
Table 22: | Hazard Switch
Table 23: | Headlamp - High Beam - Left
Table 24: | Headlamp - High Beam - Right
Table 25: | Headlamp - Low Beam - Left
Table 26: | Headlamp - Low Beam - Right
Table 27: | Headlamp Leveling Switch
Table 28: | Headlamp Switch
Table 29: | I/P Compartment Lamp
Table 30: | I/P Compartment Lamp Switch
Table 31: | I/P Dimmer Switch
Table 32: | Ignition Key Cylinder Lamp
Table 33: | Lamp Control Module
Table 34: | License Plate Lamp - Left
Table 35: | License Plate Lamp - Right
Table 36: | Park/Turn Signal Lamp - Left Front (North America)
Table 37: | Park/Turn Signal Lamp - Left Front (Except North America)
Table 38: | Park/Turn Signal Lamp - Right Front (North America)
Table 39: | Park/Turn Signal Lamp - Right Front (Except North America)
Table 40: | Reading/Dome Lamp Switch w/Sunroof
Table 41: | Reading Lamps w/oSunroof
Table 42: | Rear Compartment Lamp
Table 43: | Rear Fog Lamp Relay
Table 44: | Backup Lamp Switch (M/T)
Table 45: | Shift Indicator Lamp
Table 46: | Side Marker Lamp - Left Rear
Table 47: | Side Marker Lamp - Right Rear
Table 48: | Stop Lamp Switch
Table 49: | Tail/Stop Lamp - Left Rear Inner (Hatchback)
Table 50: | Tail/Stop Lamp - Right Rear Inner (Hatchback)
Table 51: | Tail/Stop Lamp - Left Rear Outer (Hatchback)
Table 52: | Tail/Stop Lamp - Right Rear Outer (Hatchback)
Table 53: | Turn Signal Lamp - Left Front (Except North America)
Table 54: | Turn Signal Lamp - Left Rear
Table 55: | Turn Signal Lamp - Right Front (Except North America)
Table 56: | Turn Signal Lamp - Right Rear
Table 57: | Turn Signal Multifunction Switch
Table 58: | Turn Signal Repeater Lamp - Left
Table 59: | Turn Signal Repeater Lamp - Right
Table 60: | Turn Signal/Hazard Flasher Module

#### Ashtray Lamp

Connector Part Information | 2-Way F (BK)
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BN/WH | 309 | Ashtray Lamp Supply Voltage
2 | D-GN | 44 | Ground

#### Back Up Lamp - Left

Connector Part Information |

• | OEM: 0001338

• | 2-Way F CE-F22.2 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH | 24 | Backup Lamps Supply Voltage
B | BK/WH | 750 | Ground

#### Back Up Lamp - Right

Connector Part Information |

• | OEM: 0001338

• | 2-Way F CE-F22.2 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH | 24 | Backup Lamps Supply Voltage
B | BK/WH | 750 | Ground

#### Center High Mounted Stop Lamp (CHMSL) Hatchback

Connector Part Information |

• | KET MG 610392

• | 2-Way F SDL Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 750 | Ground
2 | L-BU | 20 | Stop Lamp Switch Signal

#### Battery Saver

Connector Part Information |

• | KET MG 651050

• | 8-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | WH | 1080 | Light Switch Signal
3 | WH | 1080 | Illumination Relay Control
4 | OG | 1540 | Ignition 1 Voltage
5 | BK | 1050 | Ground
6 | PU | 128 | Door Ajar Signal
7 | L-GN | 80 | Key in Ignition Signal
8 | -- | -- | Not Used

#### Center High Mounted Stop Lamp (CHMSL) Notchback

Connector Part Information |

• | KET MG 630679

• | 2-Way F SDL Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 20 | Stop Lamp Switch Signal
2 | BK | 1250 | Ground

#### Daytime Running Lamp (DRL) Module (North America)

Connector Part Information |

• | PED 12064998

• | 8-Way F Connector (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | OG | 140 | Battery Voltage
B | L-GN | 11 | Headlamp High Beam Supply Voltage
C | PU | 12 | Headlamp Low Beam Supply Voltage
D | PU/WH | 33 | Brake Warning Indicator Control
E | BK | 1050 | Ground
F | BN | 141 | Ignition 3 Voltage
G | WH | 629 | Daytime Running Lamp (DRL) Indicator Control
H | -- | -- | Not Used

#### Daytime Running Lamp (DRL) Relay (North America)

Connector Part Information |

• | AK 838033

• | 9-Way F Relay (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | BN/WH | 309 | Right Park Lamp Supply Voltage
85 | BK | 250 | Ground
86 | L-GN | 11 | Headlamp High Beam Supply Voltage
87 | PU | 12 | Headlamp Low Beam Supply Voltage

#### Daytime Running Lamp (DRL) Module (Scandinavia)

Connector Part Information |

• | F8-4

• | 8-Way M Connector (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 140 | Battery Voltage
2 | BN/WH | 309 | Park Lamp Signal
3 | D-BU | 2641 | Daytime Running Lamp (DRL) Relay Control
4 | PU | 12 | Headlamp Low Beam Supply Voltage
5 | BK | 1050 | Ground
6 | PK | 239 | Ignition Voltage
7 | BN/WH | 309 | Park Lamp Signal
8 | PU/WH | 231 | Oil Pressure Signal

#### Daytime Running Lamp (DRL) Relay 1 (Scandinavia)

Connector Part Information |

• | AK 838033

• | 9-Way F Relay

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | D-BU | 2641 | Daytime Running Lamp (DRL) Relay Control
85 | OG | 140 | Battery Positive Voltage
86 | WH | 1080 | Park Lamp Relay Control
87 | OG | 140 | Battery Positive Voltage

#### Daytime Running Lamp (DRL) Relay 2 (Scandinavia)

Connector Part Information |

• | AK 36409

• | 9-Way F Relay

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | L-BU/BK | 2346 | Flash to Pass Signal
85 | BN | 141 | Battery Positive Voltage
86 | GY/BK | 1798 | Headlamp Relay Control
87 | L-BU | 1346 | Headlamp Relay Supply Voltage/Headlamp Control

#### Dome Lamp w/Dimmer

Connector Part Information |

• | KET MG 610398

• | 6-Way F SDL Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | PK | 839 | Ignition 1 Voltage
4 | BK | 850 | Ground
5 | PU | 156 | Courtesy Lamp Control
6 | D-GN/WH | 900 | Key Cylinder Lamp Control

#### Dome Lamp w/o Dimmer

Connector Part Information |

• | KET MG 610396

• | 4-Way F SDL Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | 850 | Ground
3 | PU | 156 | Courtesy Lamp Control
4 | OG | 640 | Battery Positive Voltage

#### Door Ajar Switch - Left Front

Connector Part Information |

• | KET MG 630063

• | 2-Way 250 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 156 | Courtesy Lamp Control

#### Door Ajar Switch - Left Rear

Connector Part Information |

• | KET MG 630063

• | 2-Way 250 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 156 | Courtesy Lamp Control

#### Door Ajar Switch - Right Front

Connector Part Information |

• | KET MG 630063

• | 2-Way 250 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 156 | Courtesy Lamp Control

#### Door Ajar Switch - Right Rear

Connector Part Information |

• | KET MG 630063

• | 2-Way 250 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 156 | Courtesy Lamp Control

#### Fog Lamp - Left Front

Connector Part Information |

• | PED 12020599

• | 2-Way F Metri-Pack 280 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 34 | Front Fog Lamp Supply Voltage
B | BK | 50 | Ground

#### Fog Lamp - Right Front

Connector Part Information |

• | PED 12020599

• | 2-Way F Metri-Pack 280 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 34 | Front Fog Lamp Supply Voltage
B | BK | 150 | Ground

#### Fog Lamp - Left Rear

Connector Part Information |

• | 12092379

• | 3-Way F Lamp Socket Wedge Base W3 (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH | 122 | Rear Fog Lamp Supply Voltage
B | -- | -- | Not Used
G | BK/WH | 70 | Ground

#### Fog Lamp - Right Rear

Connector Part Information |

• | 12092379

• | 3-Way F Lamp Socket Wedge Base W3 (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH | 122 | Rear Fog Lamp Supply Voltage
B | -- | -- | Not Used
G | BK/WH | 70 | Ground

#### Hazard Switch

Connector Part Information |

• | KET MG 651056

• | 10-Way F 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch
3 | BN/WH | 309 | Right Park Lamp Supply Voltage
4 | BN | 27 | Hazard Flasher Signal (Optional)
5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
6 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
7 | L-BU | 1508 | Turn Signal Switch Signal
8 | OG | 1040 | Battery Positive Voltage
9 | PK | 16 | Turn Signal Flasher Signal
10 | PK | 339 | Ignition 1 Voltage

#### Headlamp - High Beam - Left

Connector Part Information |

• | 12033701

• | 2-Way F Metri-Pack 480 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD | 711 | Left Headlamp High Beam Supply Voltage
B | BK/WH | 1250 | Ground

#### Headlamp - High Beam - Right

Connector Part Information |

• | 12033701

• | 2-Way F Metri-Pack 480 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD | 311 | Right Headlamp High Beam Supply Voltage
B | BK/WH | 1250 | Ground

#### Headlamp - Low Beam - Left

Connector Part Information |

• | 12033701

• | 2-Way F Metri-Pack 480 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-GN | 712 | Left Headlamp Low Beam Supply Voltage
B | BK/WH | 250 | Ground

#### Headlamp - Low Beam - Right

Connector Part Information |

• | 12033701

• | 2-Way F Metri-Pack 480 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 312 | Right Headlamp Low Beam Supply Voltage
B | BK/WH | 250 | Ground

#### Headlamp Leveling Switch

Connector Part Information |

• | MOLEX 5557-06R

• | 6-Way F Mini Fit Conn. Rec. Housing (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage
2 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage
3 | PU | 12 | Headlamp Low Beam Supply Voltage
4 | D-GN | 44 | Instrument Panel Lamps Dimming Control
5 | -- | -- | Not Used
6 | BK | 250 | Ground

#### Headlamp Switch

Connector Part Information |

• | MOLEX 5559-06P

• | 6-Way Mini Fit Conn. Crimp Pin Housing (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage (w/o North America DRL)
PU | 12 | Headlamp Low Beam Supply Voltage (w/North America DRL)
2 | GY/BK | 1798 | Headlamp Relay Control
3 | BK | 250 | Ground
4 | -- | -- | Not Used
5 | YE | 317 | Front Fog Relay Coil Supply Voltage
6 | WH | 1080 | Park Lamp Relay Control

#### I/P Compartment Lamp

Connector Part Information |

• | AK 36277

• | 2-Way F SWP Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 175 | I/P Compartment Lamp Signal
2 | BK | 1050 | Ground

#### I/P Compartment Lamp Switch

Connector Part Information |

• | F2-14

• | 2-Way F SWP Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 1540 | Battery Positive Voltage (w/Rear Fog Lamps) (w/Lamp Driver Control Module)
2 | PU | 175 | I/P Compartment Lamp Signal

#### I/P Dimmer Switch

Connector Part Information |

• | KET MG 610045

• | 3-Way F 250 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch
2 | BK | 250 | Ground
3 | BN/WH | 309 | Right Park Lamp Supply Voltage

#### Ignition Key Cylinder Lamp

Connector Part Information |

• | KET MG 610207

• | 2-Way F 118 (PA) Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
2 | D-GN/WH | 900 | Key Cylinder Lamp Control

#### Lamp Control Module

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | WH | 1080 | Park Lamp Relay Control
3 | WH | 1080 | Park Lamp Relay Control
4 | OG | 1540 | Battery Positive Voltage
5 | BK | 1050 | Ground
6 | PU | 126 | Left Front Door Open Switch Signal
7 | L-GN | 80 | Key in Ignition Switch Signal
8 | -- | -- | Not Used

#### License Plate Lamp - Left

Connector Part Information |

• | 12110053

• | 2-Way F Lamp Socket Wedge Base W2 (L-GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK (North America) | 709 | Left Park Lamp Supply Voltage
PU
B | WH (North America) | 550 | Ground
BK | 1250 | Ground

#### License Plate Lamp - Right

Connector Part Information |

• | 12110053

• | 2-Way F Lamp Socket Wedge Base W2 (L-GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK (North America) | 709 | Left Park Lamp Supply Voltage
PU
B | WH (North America) | 550 | Ground
BK | 1250 | Ground

#### Park/Turn Signal Lamp - Left Front (North America)

Connector Part Information |

• | KET MG 610327

• | 3-Way F SWP Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | PU | 709 | Left Park Lamp Supply Voltage
3 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

#### Park/Turn Signal Lamp - Left Front (Except North America)

Connector Part Information |

• | KET MG 610327

• | 3-Way F SWP Series (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 709 | Left Park Lamp Supply Voltage
2 | BK | 50 | Ground
3 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

#### Park/Turn Signal Lamp - Right Front (North America)

Connector Part Information |

• | KET MG 610327

• | 3-Way F SWP Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 150 | Ground
2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | L-BU | 15 | Right Turn Signal Lamps Supply Voltage

#### Park/Turn Signal Lamp - Right Front (Except North America)

Connector Part Information |

• | KET MG 610327

• | 3-Way F SWP Series (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage
2 | BK | 150 | Ground
3 | L-BU | 15 | Right Turn Signal Lamps Supply Voltage

#### Reading/Dome Lamp Switch w/Sunroof

Connector Part Information |

• | KET MG 610402

• | 8-Way F SDL Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 850 | Ground
2 | -- | -- | Not Used
3 | OG | 640 | Battery Positive Voltage
4 | D-GN/WH | 133 | Sunroof Limit Switch Low Reference
5 | BN | 641 | Ignition 3 Voltage
6 | PU | 132 | Sunroof Limit Switch Soft Stop Signal
7-8 | -- | -- | Not Used

#### Reading Lamps w/oSunroof

Connector Part Information |

• | KET MG 610392

• | 2-Way F SDL Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
2 | BK | 850 | Ground

#### Rear Compartment Lamp

Connector Part Information |

• | KET MG 610043

• | 2-Way F Connector (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
2 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal

#### Rear Fog Lamp Relay

Connector Part Information |

• | AK 36907

• | 9-Way F Connector (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | PU | 1977 | Outside Moisture Sensor Signal 1
3 | -- | -- | Not Used
4 | OG | 1540 | Battery Positive Voltage (w/Rear Fog Lamps) (w/Lamp Driver Control Module)
5 | YE | 317 | Front Fog Relay Coil Supply Voltage
6 | RD | 122 | Rear Fog Lamp Supply Voltage
7 | L-BU | 1346 | Headlamp Relay Supply Voltage
8 | BK | 250 | Ground
9 | -- | -- | Not Used

#### Backup Lamp Switch (M/T)

Connector Part Information |

• | PED 12052641

• | 2-Way F Metri-Pack 150 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 839 | Ignition 1 Voltage
2 | L-GN | 24 | Backup Lamp Supply Voltage

#### Shift Indicator Lamp

Connector Part Information |

• | 94797519

• | 2-Way F (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 44 | Instrument Panel Lamps Dimming Control
2 | BN/WH | 309 | Right Park Lamp Supply Voltage

#### Side Marker Lamp - Left Rear

Connector Part Information |

• | 12110053

• | 2-Way F Lamp Socket Wedge Base W2 (L-GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 709 | Left Park Lamp Supply Voltage
B | BK | 550 | Ground

#### Side Marker Lamp - Right Rear

Connector Part Information |

• | 12110053

• | 2-Way F Lamp Socket Wedge Base W2 (L-GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH | 309 | Right Park Lamp Supply Voltage
B | BK | 550 | Ground

#### Stop Lamp Switch

Connector Part Information |

• | KET MG 610267

• | 4-Way F 250 D/L Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 239 | Ignition 1 Voltage
2 | OG/BK | 540 | Battery Positive Voltage
3 | D-GN | 286 | Automatic Transmission Shift Lock Solenoid Supply Voltage
4 | L-BU | 20 | Stop Lamp Supply Voltage

#### Tail/Stop Lamp - Left Rear Inner (Hatchback)

Connector Part Information |

• | 12160394

• | 3-Way F Lamp Socket Wedge Base W3 Right Angle (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD | 20 | Stop Lamp Supply Voltage
B | WH/D-GN | 709 | Left Park Lamp Supply Voltage
G | BK | 450 | Ground

#### Tail/Stop Lamp - Right Rear Inner (Hatchback)

Connector Part Information |

• | 12160394

• | 3-Way F Lamp Socket Wedge Base W3 Right Angle (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD | 20 | Stop Lamp Supply Voltage
B | WH/D-GN | 309 | Right Park Lamp Supply Voltage
G | BK | 450 | Ground

#### Tail/Stop Lamp - Left Rear Outer (Hatchback)

Connector Part Information |

• | 12092379

• | 3-Way F Lamp Socket Wedge Base W3 (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD | 20 | Stop Lamp Supply Voltage
B | WH/BK | 709 | Left Park Lamp Supply Voltage
G | BK | 250 | Ground

#### Tail/Stop Lamp - Right Rear Outer (Hatchback)

Connector Part Information |

• | 12092379

• | 3-Way F Lamp Socket Wedge Base W3 (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD | 20 | Stop Lamp Supply Voltage
B | WH/BK | 309 | Left Park Lamp Supply Voltage
G | BK | 450 | Ground

#### Turn Signal Lamp - Left Front (Except North America)

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

#### Turn Signal Lamp - Left Rear

Connector Part Information |

• | 15354859

• | 2-Way F Lamp Socket BB W-3 (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE | 14 | Left Turn Signal Lamps Supply Voltage
G | BK | 50 | Ground

#### Turn Signal Lamp - Right Front (Except North America)

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 150 | Ground
2 | L-BU | 15 | Right Turn Signal Lamps Supply Voltage

#### Turn Signal Lamp - Right Rear

Connector Part Information |

• | 15354859

• | 2-Way F Lamp Socket BB W-3 (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE | 14 | Left Turn Signal Lamps Supply Voltage
G | BK | 50 | Ground

#### Turn Signal Multifunction Switch

Connector Part Information |

• | KET MG 610203

• | 7-Way F 118 (PA) Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
2 | PK | 16 | Turn Signal Flasher Signal
3 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
4 | L-GN | 11 | Headlamp High Beam Supply Voltage
5 | PU | 12 | Headlamp Low Beam Supply Voltage
6 | L-BU | 1346 | Headlamp Relay Supply Voltage
L-BU/BK | 2346 | Flash to Pass Signal (Except North America)
7 | OG | 140 | Battery Positive Voltage

#### Turn Signal Repeater Lamp - Left

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage (North America)
BK | 50 | Ground
2 | BK | 1150 | Ground (North America)
PU | 709 | Left Park Lamps Supply Voltage

#### Turn Signal Repeater Lamp - Right

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 15 | Right Turn Signal Lamps Supply Voltage (North America)
BK | 150 | Ground
2 | BK | 150 | Ground (North America)
BN/WH | 309 | Right Park Lamps Supply Voltage

#### Turn Signal/Hazard Flasher Module

Connector Part Information |

• | AK 36906

• | 9-Way Relay Connector (GN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | L-BU | 1508 | Turn Signal Switch Signal
3-5 | -- | -- | Not Used
6 | PK | 16 | Turn Signal Flasher Signal
7 | -- | -- | Not Used
8 | BK | 250 | Ground
9 | -- | -- | Not Used