For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
CHMSL Mounting Nuts | 4 N·m | 35 lb in
Daytime Running Lamp Bolts | 2 N·m | 18 lb in
Door Jamb Switch Screw | 4 N·m | 35 lb in
Front Fog Lamp Nuts | 4 N·m | 35 lb in
Headlamp Assembly Bolts and Nuts | 4 N·m | 35 lb in
License Plate Lamp Screws | 4 N·m | 35 lb in
Map Lamp Screws | 1.5 N·m | 13 lb in
Rear Combination Lamp Assembly Screws - Four Door | 4 N·m | 35 lb in
Rear Combination Lamp Assembly Screws - Five Door/Wagon | 3 N·m | 27 lb in
Rear Combination Lamp Assembly Nuts | 3 N·m | 27 lb in