For 1990-2009 cars

Table 1: | Struts Seem Weak
Table 2: | Struts are Noisy
Table 3: | Leaks

### Strut Dampener

A strut dampener is basically a shock absorber. However, strut dampeners are easier to extend and retract by hand than are shock absorbers.

#### Struts Seem Weak

Checks | Actions
--- | ---
Inspect the tire pressures. | Adjust the tire pressures to the specifications on the tire placard.
Inspect the load conditions under which the vehicle is normally driven. | Consult with the owner to confirm the owner's understanding of normal load conditions.
Test the compression and rebound effectiveness of the strut dampener. |

• | Quickly push down and then lift up on the corner of the bumper nearest the strut dampener being tested.

• | Compare the compression and rebound with those of a similar vehicle that has an acceptable ride quality.

• | Replace the strut dampener, if needed.

#### Struts are Noisy

Checks | Actions
--- | ---
Inspect the mountings for looseness or damage. | Tighten the strut dampener. Replace the strut dampener, if needed.
Test the compression and rebound effectiveness of the strut dampener. |

• | Quickly push down and then lift up on the corner of the bumper nearest the strut dampener being tested.

• | Compare the compression and rebound with those of a similar vehicle that has an acceptable ride quality.

• | Replace the strut dampener, if needed.

#### Leaks

Checks | Actions
--- | ---
Inspect for a slight trace of fluid. | The strut dampener is OK.
Inspect the seal cover on the fully extended strut. | Replace the strut dampener.
Inspect for an excessive amount of fluid on the strut dampener. | Replace the strut dampener.