For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rain sensor cover.
3. Disconnect the electrical connector.
4. Remove the rain sensor.

### Installation Procedure

1. Install the rain sensor.
2. Connect the electrical connector.
3. Install the rain sensor cover.
4. Connect the negative battery cable.