For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Hose Inlet Bolt and Ring Seals - Rear | 32 N·m | 24 lb ft
Brake Hose Inlet Fitting-to-Caliper Bolt - Front | 40 N·m | 30 lb ft
Caliper Bleeder Valve - Front | 8 N·m | 71 lb in
Caliper Mounting Bolts - Rear | 56 N·m | 41 lb ft
Caliper-to-Steering Knuckle Mounting Bolts - Front | 95 N·m | 70 lb ft
Hub Bolts - Rear | 65 N·m | 48 lb ft
Lower Caliper Mounting Bolt - Rear | 27 N·m | 20 lb ft
Parking Brake Shoe Hold-Down Spring Assembly Screw - Rear | 4 N·m | 35 lb in
Retaining Frame-to-Caliper Housing Bolts - Front | 27 N·m | 20 lb ft
Rotor Detent Screw - Rear | 4 N·m | 35 lb in
Rotor-to-Front Wheel Hub Detent Screw - Front | 4 N·m | 35 lb in
Splash Shield-to-Steering Knuckle Screws - Front | 4 N·m | 35 lb in