For 1990-2009 cars

Figure 1: |

#### Camshaft Position (CMP) and Crankshaft Position (CKP) Sensors, EVAP (L95, LXT)

(1) | Camshaft Position (CMP) Sensor
(2) | Crankshaft Position (CKP) Sensor
(3) | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

Figure 2: |

#### Crankshaft Position (CKP) Sensors, EVAP, Ignition Coils (L79, LDA, L34)

(1) | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve
(2) | Crankshaft Position (CKP) Sensor
(3) | Ignition Coil Modules

Figure 3: |

#### Diesel Engine (1 of 2)

(1) | Oil Separator
(2) | EGR Solenoid Valve
(3) | CMP
(4) | EGR Valve
(5) | Throttle Plate Actuator
(6) | Starter Motor
(7) | Oil Pan
(8) | A/C Compressor
(9) | Generator
(10) | Fuel Injection Pump
(11) | Power Steering Pump
(12) | MAP Sensor
(13) | Fuel Injector

Figure 4: |

#### Diesel Engine (2 of 2)

(1) | EGR Valve
(2) | Wastegate Solenoid
(3) | Oil Pressure Sensor

Figure 5: |

#### Engine Control Module (ECM), Engine Coolant Temperature (ECT), Camshaft Position (CMP) and Rough Road Sensors (L79, LDA, L34)

(1) | Engine Control Module (ECM)
(2) | Engine Coolant Temperature (ECT) Sensor
(3) | Camshaft Position (CMP) Sensor
(4) | Rough Road Sensor

Figure 6: |

#### Engine Coolant Temperature (ECT), Ignition Coils, Engine Control Module (ECM) (L95, LXT)

(1) | Engine Coolant Temperature (ECT)
(2) | Ignition Coils/Modules
(3) | Engine Control Module (ECM)

Figure 7: |

#### Exhaust Gas Recirculation (EGR) Valve, Knock Sensor (KS) (L95, LXT)

(1) | Exhaust Gas Recirculation (EGR) Valve (Euro Emissions)
(2) | Knock Sensor (KS)
(3) | Exhaust Gas Recirculation (EGR) Valve (ECE 83 Emissions)

Figure 8: |

#### Exhaust Gas Recirculation (EGR) Valve, Knock Sensor (KS) (L79, LDA)

(1) | Exhaust Gas Recirculation (EGR) Valve (Euro Emissions)
(2) | Knock Sensor (KS)
(3) | Exhaust Gas Recirculation (EGR) Valve (ECE 83 Emissions)

Figure 9: |

#### Exhaust Gas Recirculation (EGR) Valve, Knock Sensor (KS) (L34)

(1) | Exhaust Gas Recirculation (EGR) Valve
(2) | Knock Sensor (KS)

Figure 10: |

#### Fuel Injectors, Heated Oxygen Sensor (HO2S) 1, Heated Oxygen Sensor (HO2S) 2, Idle Air Control (IAC) Valve, Intake Air Temperature (IAT) Sensor (L79, LDA)

(1) | Fuel Injector 1
(2) | Fuel Injector 2
(3) | Fuel Injector 3
(4) | Fuel Injector 4
(5) | Heated Oxygen Sensor (HO2S) 1 (MR-140), Oxygen Sensor (HV-240)
(6) | Heated Oxygen Sensor (HO2S) 2 (MR-140)
(7) | Idle Air Control (IAC) Valve
(8) | Intake Air Temperature (IAT) Sensor

Figure 11: |

#### Fuel Injectors, Heated Oxygen Sensor (HO2S) 1, Heated Oxygen Sensor (HO2S) 2, Intake Air Temperature (IAT) Sensor (L95, LXT)

(1) | Fuel Injector 1
(2) | Fuel Injector 2
(3) | Fuel Injector 3
(4) | Fuel Injector 4
(5) | Heated Oxygen Sensor (HO2S) 1/Oxygen Sensor (O2S) (ECE 83 Emissions)
(6) | Heated Oxygen Sensor (HO2S) 2
(7) | Intake Air Temperature (IAT) Sensor

Figure 12: |

#### Fuel Injectors, Heated Oxygen Sensor (HO2S) 1, Heated Oxygen Sensor (HO2S) 2, Idle Air Control (IAC) Valve, Intake Air Temperature (IAT) Sensor (L34)

(1) | Fuel Injector 1
(2) | Fuel Injector 2
(3) | Fuel Injector 3
(4) | Fuel Injector 4
(5) | Heated Oxygen Sensor (HO2S) 1
(6) | Heated Oxygen Sensor (HO2S) 2
(7) | Idle Air Control (IAC) Valve
(8) | Intake Air Temperature (IAT) Sensor

Figure 13: |

#### Fuel Vapor Recovery System (L34)

(1) | Fuel Tube
(2) | Fuel Filler Cap
(3) | Fuel Tank
(4) | Service Port
(5) | Fuel Pipe to Fuel Rail
(6) | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve
(7) | Vacuum Hose to Intake Manifold
(8) | Evaporative Emissions (EVAP) Canister
(9) | Evaporative Emissions Canister Vent Solenoid Valve

Figure 14: |

#### Manifold Absolute Pressure (MAP), Oil Pressure, Throttle Position (TP) Sensors (L79, LDA, L34)

(1) | Manifold Absolute Pressure (MAP) Sensor
(2) | Engine Oil Pressure Switch
(3) | Throttle Position (TP) Sensor
(4) | Idle Air Control (IAC)

Figure 15: |

#### TCM Harness RHD (M98)

(1) | Park/Neutral Position (PNP) Switch
(2) | Output Speed Sensor (OSS)
(3) | X207
(4) | Input Speed Sensor (ISS)
(5) | Automatic Transaxle

Figure 16: |

#### TCM Harness LHD (M98)

(1) | Park/Neutral Position (PNP) Switch
(2) | Output Speed Sensor (OSS)
(3) | Transmission Control Module (TCM)
(4) | X207
(5) | Input Speed Sensor (ISS)
(6) | Automatic Transaxle

Figure 17: |

#### Throttle Body, Manifold Absolute Pressure (MAP), Oil Pressure (L95, LXT)

(1) | Throttle Body
(2) | Manifold Absolute Pressure (MAP) Sensor
(3) | Oil Pressure Switch

Figure 18: |

#### Transmission Control Module (TCM) (MLQ)

(1) | Transmission Control Module (TCM) Aisin

Figure 19: |

#### Transmission Electronic Components (MLQ)

(1) | Transmission Control Module (TCM) Harness Connector
(2) | Input Speed Sensor (ISS) Connector
(3) | Transaxle Harness
(4) | Solenoid Connectors
(5) | Park/Neutral Position (PNP) Switch
(6) | Output Shaft Speed (OSS) Sensor (Vehicle Speed Sensor (VSS))
(7) | Output Shaft Speed (OSS) Connector
(8) | TCM

Figure 20: |

#### Transmission Control Module (TCM) (MFA)

(1) | Transmission Control Module (TCM) ZF 4HP16
(2) | Key Interlock Module

Figure 21: |

#### Transaxle Housing (MFA)

(1) | Transaxle Housing
(2) | Breather Pipe
(3) | Sleeve Protector
(4) | Type Plate
(5) | Axle Shaft Seal
(6) | Sealing Sleeve
(7) | Sealing Sleeve
(8) | Cable Terminal
(9) | Output Speed Sensor
(10) | Bolt
(11) | Washer
(12) | Bushing
(13) | Shaft Seal
(14) | Park/Neutral Position Switch
(15) | Bolt
(16) | Shim
(17) | Shim