For 1990-2009 cars

Range | Park/Neutral | Reverse | D | 3 | 2 | 1
--- | --- | --- | --- | --- | --- | ---
Gear | N | R | 1st | 2nd | 3rd | 4th | ³1st | ¹2nd | 3rd | ²1st | 2nd | 1st
Solenoid Valve 1 | ON | ON/OFF | ON/OFF | ON/OFF | ON/OFF | ON/OFF | ON/OFF | ON/OFF | ON/OFF | ON/OFF | ON/OFF | ON/OFF
Solenoid Valve 2 | ON | ON | ON | OFF | OFF | OFF | ON | OFF | OFF | ON | OFF | ON
Line Pressure Control Solenoid Valve (PCS) 3 | OFF | OFF | OFF | ON | ON/OFF | ON/OFF | OFF | ON | ON/OFF | OFF | ON | OFF
Line Pressure Control Solenoid Valve (PCS) 4 | ON | OFF | ON | ON | ON | OFF | ON | ON | ON | ON | ON | ON
Line Pressure Control Solenoid Valve (PCS) 5 | OFF | OFF | ON | ON | OFF | OFF | ON | ON | OFF | ON | ON | ON
Line Pressure Control Solenoid Valve (PCS) 6 | ON | OFF | ON | ON | ON | OFF | ON | ON | ON | ON | ON | ON
Brake B | A | A | A | -- | A | -- | A | -- | A | A | -- | A
Brake C | -- | -- | -- | -- | -- | H | -- | -- | -- | -- | -- | --
Brake D | -- | H | -- | -- | -- | -- | -- | -- | -- | -- | -- | --
Brake E | -- | -- | -- | A | A | A | -- | A | A | -- | A | --
Brake F | -- | -- | H | H | -- | -- | H | H | -- | H | H | H
Lock-up Clutch | -- | -- | -- | -- | -- | A | -- | -- | -- | -- | -- | --
A = Applied H = Holding ON = The solenoid is energized OFF = The solenoid is not energized ¹Manual Second-Third gear is only available above approximately 100 km/h (62 mph).

²Manual First-Second gear is only available above approximately 60 km/h (37 mph).

³Manual First-Third gear is also possible at high vehicle speed as a safety feature.