For 1990-2009 cars

Table 1: | Fuse Block - Underhood Label Usage
Table 2: | Fuse Block - Underhood Auxiliary Label Usage
Table 3: | Fuse Block - I/P Label Usage

### Fuse Block - Underhood Label

#### Fuse Block - Underhood Label Usage

No. | Device | Rating | Description
--- | --- | --- | ---
EF1 | BATT PWR Fuse | 30A | Battery Main, F13-F16, F21-F24
EF2 | ABS Fuse | 60A | EBCM, Oil Feeding Connector
EF3 | HVAC BLWR Fuse | 30A | Blower Relay
EF4 | IGN 2 Fuse | 30A | Ignition Switch - 2
EF5 | IGN 1 Fuse | 30A | Ignition Switch - 1
EF6 | COOL FAN LOW Fuse | 20A | Cooling Fan Low Relay
EF7 | DEFOG Fuse | 30A | Defog Relay
EF8 | COOL FAN HI Fuse | 30A | Cooling Fan HI Relay (Gasoline)
40A | Cooling Fan HI Dummy Plug (Diesel)
EF9 | PWR WINDOW Fuse | 20A | Power Window Switch
EF10 | IGN COIL Fuse | 15A | Fuel Connector, ECM, MR-140, LEGR, EI System
EF11 | ECM Fuse | 10A | ECM, Main Relay, Sirius D4
EF12 | HEADLAMPS Fuse | 25A | Headlamp, ILLUM Relay
EF13 | STOP LAMPS Fuse | 15A | Brake Switch
EF14 | DRIVER'S PWR WNOW Fuse | 20A | Power Window Switch
EF15 | HI BEAM Fuse | 15A | Headlamp HI
EF16 | HORN Fuse | 15A | Horn Relay, Siren, Hood Contact Switch
EF17 | A/C Fuse | 10A | A/C Comp Relay
EF18 | FUEL PUMP Fuse | 15A | Fuel Pump
EF19 | IP FUSE BLOCK Fuse | 15A | Cluster, Key Remind S/W, Folding Mirror Unit, MAP Lamp, Room Lamp, Trunk Open Lamp, Trunk Open Switch
EF20 | LOW BEAM LT Fuse | 10A | Headlamp LO
EF21 | ENG SNSR Fuse | 15A | EVAP Canister Purge Solenoid, HO2S, Cooling Fan Relay
EF22 | INJECTOR Fuse | 15A | Injector, EGR, EEGR
EF23 | ILLUM LT Fuse | 10A | License Plate Lamp, Chime Bell, Tail Lamp, Headlamp
EF24 | FRT FOG Fuse | 15A | Fog Lamp Relay
EF25 | MIR HTD Fuse | 10A | Electric OSRV Mirror
EF26 | DR/LCK Fuse | 15A | Central Door Lock Unit
EF27 | LOW BEAM RT Fuse | 10A | Headlamp LO
EF28 | ILLUM RT Fuse | 10A | ILLUM Circuit, Headlamp, Tail Lamp
EF29 | SPARE | 10A | Not Used
EF30 | SPARE | 15A | Not Used
EF31 | SPARE | 25A | Not Used

### Fuse Block Underhood - Top View

### Fuse Block Underhood - Bottom View

### Fuse Block - Underhood Auxiliary Label Usage

No. | Device | Rating | Description
--- | --- | --- | ---
AF1 | Glow Plug Control Unit | 60A | Glow Plug Control Unit
AF2 | Fuel Filter Heater Relay | 30A | Fuel Filter Heater Relay
AF3 | PTC-1 Relay | 40A | PTC-1 Relay
AF4 | PTC-2 Relay | 40A | PTC-2 Relay
AF5 | PTC-3 Relay | 40A | PTC-3 Relay

### Fuse Block - I/P Label

#### Fuse Block - I/P Label Usage

No | Device | Rating | Description
--- | --- | --- | ---
F1 | AIRBAG Fuse | 10A | SDM
F2 | ECM Fuse | 10A | TCM, ECM, Generator, VGIS, VSS
F3 | TRN SIG LAMPS Fuse | 15A | Hazard Switch
F4 | CLSTR, BTSI Fuse | 10A | Cluster, Brake Switch, Chime Bell, Brake Switch, SSPS Module, A/C Control Switch
F5 | -- | -- | Not Used
F6 | ENG FUSE BOX DRL Fuse | 10A | A/C Comp Relay, Defog Relay, Power Window Relay, Headlamp Relay
F7 | HVAC Fuse | 20A | Blower Relay, A/C Control Switch, HVAC
F8 | S/ROOF Fuse | 15A | Electric Mirror Switch, Folding Mirror, Sun Roof Module
F9 | WPR Fuse | 25A | Wiper Motor, Wiper Switch, Rain Sensor Unit - RHD
F10 | AIRBAG Fuse | -- | Occupant Classification Sensor, Clock
F11 | ABS Fuse | 10A | EBCM, Oil Feeding Connector
F12 | IMMOBILIZER Fuse (Except North America) | 10A | Immobilizer, Theft Deterrent Control Unit, Rain Sensor Unit - LHD
F13 | TCM Fuse | 10A | TCM
F14 | HAZARD LAMPS Fuse | 15A | Hazard Switch
F15 | RKE Fuse | 15A | Theft Deterrent Control Unit
F16 | DLC Fuse | 10A | DLC
F17 | RADIO/CLK Fuse | 10A | Clock, Radio
F18 | AUT LTR Fuse | 15A | Extra Power Jack
F19 | LTR Fuse | 15A | Cigar Lighter
F20 | BCK/UP Fuse | 10A | Reverse Lamp Switch, PNP Switch
F21 | BATT SAVERFuse | 15A | Rear Fog Relay
F22 | AUTO A/C Fuse | 15A | Clock, HVAC, A/C Control Switch
F23 | RADIO Fuse | 15A | Radio
F24 | Immobilizer Fuse (Except North America) | 10A | Immobilizer (1.6L and 1.8L)

### Fuse Block I/P - Top View

### Fuse Block I/P - Bottom View