For 1990-2009 cars

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Notice: When you are jacking or lifting a vehicle at the frame side rails or other prescribed lift points, be certain that the lift pads do not contact the catalytic converter, the brake pipes or the fuel lines. If such contact occurs, vehicle damage or unsatisfactory vehicle performance may result.

#### Vehicle Lifting Points

(1) | Suspension Contact Lift - Rear Location
(2) | Floor Jacking - Rear Location
(3) | Frame Contact Lift - Rear Location
(4) | Floor Jacking - Side Location
(5) | Frame Contact Lift - Front Location
(6) | Suspension Contact Lift - Front Location

#### Frame and Suspension Lifting Points

(1) | Frame Contact Lift - Rearward of the Front Tire
(2) | Frame Contact Lift - Forward of the Rear Tire
(3) | Suspension Contact Lift - Under Front Lower Control Arm