For 1990-2009 cars

Table 1: | A/C Compressor Clutch
Table 2: | A/C Refrigerant Pressure Sensor - 1.4L/1.6L
Table 3: | A/C Refrigerant Pressure Sensor - 1.8L/2.0L
Table 4: | A/C Refrigerant Pressure Sensor - Diesel
Table 5: | Air Temperature Actuator
Table 6: | Ambient Air Temperature Sensor
Table 7: | Blower Motor
Table 8: | Blower Motor Control Module
Table 9: | Blower Motor Relay
Table 10: | Coolant Temperature Sensor
Table 11: | High Speed Blower Motor Relay
Table 12: | HVAC Control - A
Table 13: | HVAC Control - B
Table 14: | Inside Air Temperature
Table 15: | Mode Actuator
Table 16: | Recirculation Actuator
Table 17: | Sunload Sensor

#### A/C Compressor Clutch

Connector Part Information |

• | PED 12162017

• | 2-Way F Metri-Pack 150 Series, Sealed (M-GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-GN | 59 | A/C Compressor Clutch Supply Voltage
B | BK | 150 | Ground

#### A/C Refrigerant Pressure Sensor - 1.4L/1.6L

Connector Part Information |

• | PED 12078090

• | 3-Way F Metri-Pack 150 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | 413 | Low Reference
B | L-BU/BK | 1688 | 5-Volt Reference
C | RD/L-BU | 203 | A/C Refrigerant Pressure Sensor Signal

#### A/C Refrigerant Pressure Sensor - 1.8L/2.0L

Connector Part Information |

• | PED 12078090

• | 3-Way F Metri-Pack 150 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU/WH | 632 | Low Reference
B | GY | 605 | 5-Volt Reference
C | L-BU | 380 | A/C Refrigerant Pressure Sensor

#### A/C Refrigerant Pressure Sensor - Diesel

Connector Part Information |

• | PED 12078090

• | 3-Way F Metri-Pack 150 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN/WH | 1688 | 5-Volt Reference
B | BK/WH | 413 | Low Reference
C | BN/BK | 203 | A/C Refrigerant Pressure Sensor Signal

#### Air Temperature Actuator

Connector Part Information |

• | KET MG 610203

• | 7-Way F 118 (PA) Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | 1199 | Air Temperature Door Control
3 | BN | 1812 | Low Reference
4 | -- | -- | Not Used
5 | YE | 1791 | Low Reference
6 | YE/BK | 1814 | Lower Mode Door Position Signal
7 | L-BU | 1316 | Air Temperature Door Control

#### Ambient Air Temperature Sensor

Connector Part Information |

• | KET MG 610489

• | 2-Way F NMWP 04F-B Ass'y

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 61 | Low Reference
2 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal

#### Blower Motor

Connector Part Information |

• | KET MG 610043

• | 2-Way F 250 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 744 | Blower Motor Supply Voltage
2 | PK | 743 | Blower Motor Speed Signal

#### Blower Motor Control Module

Connector Part Information |

• | KET MG 610269

• | 6-Way F 250 D/L Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU | 188 | Blower Motor Resistor Assembly Supply Voltage
2 | -- | -- | Not Used
3 | BK | 350 | Ground
4 | GY/BK | 754 | Blower Motor Speed Control
5 | -- | -- | Not Used
6 | PK | 743 | Blower Motor Speed Signal

#### Blower Motor Relay

Connector Part Information |

• | AK 36409

• | 9-Way F Relay

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | BK | 350 | Battery Positive Voltage
85 | DK-BU/BK | 247 | Ground
86 | BN | 41 | Blower Motor High Control
87 | PK | 743 | Blower Motor Feed

#### Coolant Temperature Sensor

Connector Part Information |

• | KET MG 610070

• | 2-Way F 090 (2.3 mm) Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 61 | Low Reference
2 | GY/BK | 1596 | Coolant Temperature Sensor Signal

#### High Speed Blower Motor Relay

Connector Part Information |

• | AK 36409

• | 5-Way F (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | BK | 350 | Ground
85 | D-BU/BK | 247 | High Speed Blower Relay Control
86 | BN | 41 | Ignition 3 Voltage
87 | PK | 743 | Blower Motor Speed Control

#### HVAC Control - A

Connector Part Information |

• | MOLEX 51155-1615

• | 16-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BK | 350 | Ground
A2 | L-BU | 1316 | Air Temperature Door Control
A3 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
A4 | BN/WH | 309 | Right Park Lamp Voltage
A5 | BN | 41 | Ignition 3 Voltage
A6-A7 | -- | -- | Not Used
A8 | YE | 1791 | Low Reference
A9 | -- | -- | Not Used
A10 | D-BU/BK | 247 | High Speed Blower Relay Control
A11 | D-GN/WH | 762 | A/C Request Signal
A12 | WH | 193 | Rear Defog Relay Control
A13 | YE | 61 | Low Reference
A14 | OG | 1140 | Battery Positive Voltage
A15 | -- | -- | Not Used
A16 | D-GN | 1910 | Inside Air Temperature Sensor Signal

#### HVAC Control - B

Connector Part Information |

• | MOLEX 51155-2015

• | 20-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
B1 | GY/BK | 754 | Blower Motor Speed Signal
B2 | D-GN/RD | 817 | Vehicle Speed Signal
B3 | -- | -- | Not Used
B4 | BN | 1812 | Low Reference
B5 | YE/BK | 1814 | Lower Mode Door Position Signal
B6 | BK | 1199 | Air Temperature Door Control
B7 | D-GN | 95 | Windshield Washer Switch Signal
B8 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
B9 | GY/BK | 1596 | Coolant Temperature Sensor Signal
B10 | L-BU/BK | 590 | Sunload Sensor Signal
B11 | BK | 350 | Ground
B12 | D-BU | 188 | Blower Motor Resistor Assembly Supply Voltage
B13 | PK/WH | 1648 | Recirculation Door Control A
B14 | D-GN/BK | 1647 | Recirculation Door Control B
B15 | -- | -- | Not Used
B16 | D-GN/BK | 1395 | Upper Mode Valve Solenoid Control
B17 | PK | 1396 | Defrost Mode Valve Solenoid Control
B18 | YE | 1397 | Lower Mode Valve Solenoid Control
B19 | WH/BK | 1398 | Mode Valve Signal
B20 | PK/BK | 1399 | Mode Valve Signal

#### Inside Air Temperature

Connector Part Information |

• | KET MG 620074

• | 2-Way M 090 Connector (2.3 mm)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 1910 | Inside Air Temperature Sensor Signal
2 | YE | 61 | Low Reference

#### Mode Actuator

Connector Part Information |

• | KET MG 610203

• | 7-Way F 118 (PA) Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 1397 | Lower Mode Valve Solenoid Control
2 | PK | 1396 | Defrost Mode Valve Solenoid Control
3 | D-G/BK | 1395 | Upper Mode Valve Solenoid Control
4 | BN | 41 | Ignition 3 Voltage
5 | BK | 350 | Ground
6 | PK/BK | 1399 | Mode Valve Signal
7 | WH/BK | 1398 | Mode Valve Signal

#### Recirculation Actuator

Connector Part Information |

• | KET MG 610203

• | 7-Way F 118 (PA) Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | BN | 41 | Ignition 3 Voltage
5 | PK/WH | 1648 | Recirculation Door Control A
6 | -- | -- | Not Used
7 | D-GN/BK | 1647 | Recirculation Door Control B

#### Sunload Sensor

Connector Part Information |

• | KET MG 610489

• | 2-Way F 090 (2.3 mm) Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 61 | Low Reference
2 | L-BU/BK | 590 | Sunload Sensor Signal