For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Bleeder Screw | 8 N·m | 71 lb in
Booster-to-Bracket Nuts - Right Hand Drive | 22 N·m | 16 lb ft
Booster-to-Dash Panel Nut - Left Hand Drive | 22 N·m | 16 lb ft
Booster Hex Nut and Pushrod Clevis | 18 N·m | 13 lb ft
Brake Line Fittings | 16 N·m | 12 lb ft
Brake Lines | 16 N·m | 12 lb ft
Brake Pedal-to-Pedal Bracket Hex Nut | 18 N·m | 13 lb ft
Front Disc Brake Hose-to-Caliper Bolt | 40 N·m | 30 lb ft
Master Cylinder Attaching Nuts | 18 N·m | 13 lb ft
Proportioning Valves | 22 N·m | 16 lb ft
Rear Disc Brake Hose-to-Caliper Bolt | 32 N·m | 24 lb ft