For 1990-2009 cars

## Fastener Tightening Specifications Gasoline Engines

Application | Specification
--- | ---
Metric | English
Fan Assembly Mounting Bolts | 4 N·m | 35 lb in
Fan Motor Nut | 3.2 N·m | 28 lb in
Fan Motor Retaining Screws | 4 N·m | 35 lb in
Radiator Retaining Bolts, Upper Left and Upper Right | 8 N·m | 71 lb in
Surge Tank Attaching Bolt | 5 N·m | 44 lb in
Thermostat Housing Mounting Bolts - 1.6L DOHC | 20 N·m | 15 lb ft
Thermostat Housing Mounting Bolts - 1.8L L97/2.0L DOHC | 15 N·m | 11 lb ft
Thermostat Housing Mounting Bolts - 1.8L LDA | 20 N·m | 15 lb ft
Water Pump Mounting Bolts - 1.6L DOHC | 10 N·m | 89 lb in
Water Pump Mounting Bolts --1.8L L97 | 25 N·m | 18 lb ft
Water Pump Mounting Bolts - 1.8L LDA | 8 N·m | 71 lb in
Water Pump Mounting Bolts - 1.8L/2.0L DOHC | 25 N·m | 18 lb ft