For 1990-2009 cars

Table 1: | Door Lock Actuator - Driver
Table 2: | Door Lock Actuator - Left Rear
Table 3: | Door Lock Actuator - Right Rear
Table 4: | Door Lock Actuator - Front Passenger
Table 5: | Door Tamper Switch - Driver
Table 6: | Door Tamper Switch - Passenger
Table 7: | Door Lock Relay
Table 8: | Door Lock Switch (Optional)
Table 9: | Rear Compartment Latch (Notchback)
Table 10: | Rear Compartment Lid Release Switch (Notchback)
Table 11: | Rear Compartment Tamper Switch (Notchback)
Table 12: | Rear Liftgate Latch - C1 (Hatchback)
Table 13: | Rear Liftgate Latch - C2 (Hatchback)
Table 14: | Rear Liftgate Latch - C3 (Hatchback)

#### Door Lock Actuator - Driver

Connector Part Information |

• | PED 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU/WH | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

#### Door Lock Actuator - Left Rear

Connector Part Information |

• | PED 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

#### Door Lock Actuator - Right Rear

Connector Part Information |

• | PED 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU | 294 | Door Lock Actuator Unlock Control
B | WH | 295 | Door Lock Actuator Lock Control

#### Door Lock Actuator - Front Passenger

Connector Part Information |

• | PED 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU/WH | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

#### Door Tamper Switch - Driver

Connector Part Information |

• | AK 32421

• | 4-Way F Connector (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | L-BU/BK | 195 | Door Lock Control
B | BK | 1150 | Ground
C | WH | 194 | Door Unlock Control
D | L-GN | 1370 | Driver Door Lock Cylinder Signal

#### Door Tamper Switch - Passenger

Connector Part Information |

• | AK 32421

• | 4-Way F Connector (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU | 1371 | Passenger Door Lock Cylinder Signal
B | -- | -- | Not Used
C | BK | 350 | Ground
D | -- | -- | Not Used

#### Door Lock Relay

Connector Part Information |

• | KET MG 610896

• | 8-Way F PCB Connector SDL-II PCB Hsg (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
2 | GY | 295 | Door Lock Actuator Lock Control
3 | PU | 294 | Door Lock Actuator Unlock Control
4 | WH | 194 | Door Unlock Control
5 | OG/BK | 1340 | Battery Positive Voltage
6 | L-BU/BK | 195 | Door Lock Control
7 | YE | 356 | Driver Door Lock Relay Unlock Control
8 | BK | 350 | Ground

#### Door Lock Switch (Optional)

Connector Part Information |

• | KET MG 610394

• | 3-Way F SDL Series (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
2 | BK | 1150 | Ground
3 | WH | 356 | Driver Door Lock Relay Unlock Control

#### Rear Compartment Latch (Notchback)

Connector Part Information |

• | KET MG 651032

• | 3-Way F 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 1250 | Ground
2 | BN | 253 | Trunk Release Relay Control
3 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal

#### Rear Compartment Lid Release Switch (Notchback)

Connector Part Information |

• | KET MG 651201-4

• | 2-Way F 090-II Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 253 | Trunk Release Relay Control
2 | OG | 640 | Battery Positive Voltage

#### Rear Compartment Tamper Switch (Notchback)

Connector Part Information |

• | AMP 174463

• | 2-Way M 070 Series Multilock 2P (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 263 | Rear Compartment Lid Ajar Switch Signal
2 | BK | 1250 | Ground

#### Rear Liftgate Latch - C1 (Hatchback)

Connector Part Information |

• | KET MG 610047

• | 4-Way F 250 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 294 | Door Lock Actuator Unlock Control
2 | -- | -- | Not Used
3 | GY | 295 | Door Lock Actuator Lock Control
4 | -- | -- | Not Used

#### Rear Liftgate Latch - C2 (Hatchback)

Connector Part Information |

• | KET MG 610392

• | 2-Way F SDL Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal
2 | BK | 750 | Ground

#### Rear Liftgate Latch - C3 (Hatchback)

Connector Part Information |

• | AMP 174463

• | 2-Way M 070 Series Multilock 2P (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 263 | Rear Compartment Lid Ajar Switch
2 | BK | 750 | Ground