For 1990-2009 cars

Warning: Refer to Safety Glasses Warning in the Preface section.

1. Install the oil trays and the front sun gear to the planetary gear set.
2. Install the front gear set with the rear ring gear, the front sun gear, and the oil trays.
3. Install the axial needle bearing.
4. Install the planetary gear set.
5. Install the snap ring to the front ring gear.
6. Install the planetary gear set.
7. Install the rear sun gear.
8. Install the clutch B/E. Refer to Clutch B/E Assemble.