For 1990-2009 cars

### Removal Procedure

1. Remove the parking brake/gearshift console hood, detaching the parking brake lever boot. Refer to Front Floor Console Replacement .
2. Slip the parking brake handle off of the parking brake lever.

### Installation Procedure

1. Push the parking brake handle as far as it will go on the parking brake lever.
2. Install the parking brake/gearshift console hood with the parking brake lever boot. Refer to Front Floor Console Replacement .