For 1990-2009 cars

Table 1: | Power Steering Control Module
Table 2: | Steering Wheel Position Sensor
Table 3: | Variable Effort Steering Actuator

#### Power Steering Control Module

Connector Part Information |

• | AMP 173852-1

• | 14-Way F 070 Series Multilock Plug 14P (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 1738 | Variable Effort Steering Acuator Supply Voltage
2 | PU | 1703 | Variable Effort Steering Acuator Control
3 | BK/WH | 451 | Steering Wheel Sensor Ground
4 | -- | -- | Not Used
5 | GY | 1416 | Battery Positive Voltage
6 | D-GN/WH | 817 | Vehicle Speed Sensor (VSS) Signal
7 | -- | -- | Not Used
8 | PK | 239 | Ignition 1 Voltage
9 | BN | 956 | Speed Sensitive Power Steering (SSPS) Warning Lamp Control
10 | BK | 1050 | Ground
11-12 | -- | -- | Not Used
13 | D-BU | 555 | Serial Data
14 | L-BU | 1533 | Steering Wheel Sensor Signal

#### Steering Wheel Position Sensor

Connector Part Information |

• | PED 12064758

• | 3-Way F Metri-Pack 150 Series, Unsealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 1416 | Battery Positive Voltage
2 | L-BU | 1533 | Steering Wheel Sensor Signal
3 | BK/WH | 451 | Ground

#### Variable Effort Steering Actuator

Connector Part Information |

• | PED 12052643

• | 2-Way F Metri-Pack 150 Series, Sealed (BN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-GN | 1703 | Variable Effort Steering Actuator Control
B | BN/BK | 1738 | Variable Effort Steering Actuator Supply Voltage