For 1990-2009 cars

Table 1: | Clutch Start Switch
Table 2: | Generator

#### Clutch Start Switch

Connector Part Information |

• | PED 12010649

• | 2-Way F 56 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 5 | Crank Voltage
2 | GY | 48 | Clutch Start Switch Signal

#### Generator

Connector Part Information |

• | PED 12186568

• | 4-Way F Metri-Pack 150 Series (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BN | 25 | Charge Indicator Control/Signal
C | PK/D-BU | 539 | Ignition 1 Voltage
D | -- | -- | Not Used