For 1990-2009 cars

#### Door Lock Actuator - Driver

Connector Part Information |

• | PED 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU/WH | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

#### Door Lock Actuator - Left Rear

Connector Part Information |

• | PED 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

#### Door Lock Actuator - Right Rear

Connector Part Information |

• | PED 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU | 294 | Door Lock Actuator Unlock Control
B | WH | 295 | Door Lock Actuator Lock Control

#### Door Lock Actuator - Front Passenger

Connector Part Information |

• | PED 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU/WH | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

#### Door Tamper Switch - Driver

Connector Part Information |

• | AK 32421

• | 4-Way F Connector (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | L-BU/BK | 195 | Door Lock Control
B | BK | 1150 | Ground
C | WH | 194 | Door Unlock Control
D | L-GN | 1370 | Driver Door Lock Cylinder Signal

#### Door Tamper Switch - Passenger

Connector Part Information |

• | AK 32421

• | 4-Way F Connector (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU | 1371 | Passenger Door Lock Cylinder Signal
B | -- | -- | Not Used
C | BK | 350 | Ground
D | -- | -- | Not Used

#### Door Lock Relay

Connector Part Information |

• | KET MG 610896

• | 8-Way F PCB Connector SDL-II PCB Hsg (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
2 | GY | 295 | Door Lock Actuator Lock Control
3 | PU | 294 | Door Lock Actuator Unlock Control
4 | WH | 194 | Door Unlock Control
5 | OG/BK | 1340 | Battery Positive Voltage
6 | L-BU/BK | 195 | Door Lock Control
7 | YE | 356 | Driver Door Lock Relay Unlock Control
8 | BK | 350 | Ground

#### Door Lock Switch (Optional)

Connector Part Information |

• | KET MG 610394

• | 3-Way F SDL Series (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
2 | BK | 1150 | Ground
3 | WH | 356 | Driver Door Lock Relay Unlock Control

#### Outside Rearview Folding Module (Optional)

Connector Part Information |

• | KET MG 610896

• | 8-Way F PCB Connector SDL-II PCB Hsg (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | GY/RD | 2232 | Folding Mirror Switch Signal
2 | -- | -- | Not Used
3 | OG | 640 | Battery Positive Voltage
4 | BN | 641 | Ignition 3 Voltage
5 | BK | 350 | Ground
6 | -- | -- | Not Used
7 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control
8 | BN/WH | 2230 | Folding Mirror Motor Retract Control

#### Outside Rearview Mirror Driver

Connector Part Information |

• | AMP 173850

• | 8-Way F 070 Series Multilock Plug 8P (NA)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN/WH | 2230 | Folding Mirror Motor Retract Control (Optional)
2 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (Optional)
3 | OG/WH | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (Optional)
4 | GY | 90 | Passenger Mirror Motor Left Control
5 | -- | -- | Not Used
6 | WH | 81 | Driver Mirror Motor Right Control
7 | L-GN | 89 | Driver Mirror Motor Up Control
8 | BK | 1150 | Ground

#### Outside Rearview Mirror Passenger

Connector Part Information |

• | AMP 173850-1

• | 8-Way F 070 Series Multilock Plug 8P (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (Optional)
2 | BN/WH | 2230 | Folding Mirror Motor Retract Control (Optional)
3 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (Optional)
4 | GY/BK | 90 | Passenger Mirror Motor Left Control
5 | -- | -- | Not Used
6 | RD/WH | 881 | Passenger Mirror Motor Right Control
7 | PU/WH | 889 | Passenger Mirror Motor Down Control
8 | BK | 350 | Ground

#### Outside Rearview Mirror Switch

Connector Part Information |

• | AMP 173850

• | 8-Way M 070 Series Multilock Plug 8P (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | L-GN | 89 | Driver Mirror Motor Up Control
2 | GY/BK | 2232 | Folding Mirror Switch (Optional)
3 | PU/WH | 889 | Passenger Mirror Motor Down Control
4 | GY | 90 | Passenger Mirror Motor Left Control
5 | WH | 81 | Driver Mirror Motor Right Control
6 | BK | 1150 | Ground
7 | RD/WH | 881 | Passenger Mirror Motor Right Control
8 | BN | 141 | Ignition 3 Voltage

#### Window Motor - Left Front

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU | 164 | Power Window Motor Driver Front Up Control
2 | BN | 165 | Power Window Motor Driver Front Down Control

#### Window Motor - Right Front

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU | 666 | Power Window Motor Passenger Front Up Control
2 | BN | 667 | Power Window Motor Passenger Front Down Control

#### Window Motor - Left Rear

Connector Part Information |

• | AMP 174198-1

• | 2-Way M Connector (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU | 668 | Power Window Motor Left Rear Up Control
2 | BN | 669 | Power Window Motor Left Rear Down Control

#### Window Motor - Right Rear

Connector Part Information |

• | AMP 174198-1

• | 2-Way M Connector

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU | 668 | Power Window Motor Right Rear Up Control
2 | BN | 669 | Power Window Motor Right Rear Down Control

#### Window Switch - Driver - Front Power Only

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN | 165 | Power Window Motor Driver Front Down Control
2 | D-BU | 1307 | Power Window Master Switch Lockout Control
3 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal
4 | RD | 581 | Power Window Master Switch Lockout Control
5 | OG | 580 | Power Window Supply Voltage
6 | D-BU | 164 | Power Window Motor Driver Front Up Control
7 | BK | 1150 | Ground
8 | PU | 167 | Power Window Master Switch Passenger Front Down Signal

#### Window Switch - Left Front - Front/Rear Power

Connector Part Information |

• | KET MG 651110

• | 14-Way F 090-II Series (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN | 165 | Power Window Motor Driver Front Down Control
2 | D-BU | 164 | Power Window Motor Driver Front Up Control
3 | RD | 581 | Power Window Master Switch Lockout Control
4 | PU | 167 | Power Window Master Switch Passenger Front Down Signal
5 | OG/D-BU | 64 | Auto Up (A33)
6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal
7 | D-BU | 1307 | Power Window Master Switch Lockout Control
8 | PU/RD | 169 | Power Window Master Switch Lockout Control
9 | OG/D-BU | 64 | Auto Up (A33)
10 | OG | 580 | Power Window Supply Voltage
11 | BK | 1150 | Ground
12 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
13 | PU/WH | 171 | Power Window Master Switch Right Rear Down Signal
14 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal

#### Window Switch - Left Rear

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN | 669 | Power Window Motor Left Rear Down Control
2 | -- | -- | Not Used
3 | D-BU | 668 | Power Window Motor Left Rear Up Control
4 | PU | 169 | Power Window Master Switch Left Rear Down Signal
5 | -- | -- | Not Used
6 | D-BU | 1307 | Power Window Master Switch Lockout Control
7 | BK | 1250 | Ground
8 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal

#### Window Switch - Right Front

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN | 667 | Power Window Motor Right Rear Up Control
2 | -- | -- | Not Used
3 | D-BU | 666 | Power Window Motor Passenger Front Up Control
4 | PU | 167 | Power Window Master Switch Passenger Front Down Signal
5 | -- | -- | Not Used
6 | D-BU | 1307 | Power Window Master Switch Lockout Control
7 | BK | 350 | Ground
8 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal

#### Window Switch - Right Rear

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN | 669 | Power Window Motor Right Rear Down Control
2 | -- | -- | Not Used
3 | D-BU | 668 | Power Window Motor Right Rear Up Control
4 | PU | 169 | Power Window Master Switch Right Rear Down Signal
5 | -- | -- | Not Used
6 | D-BU | 1307 | Power Window Master Switch Lockout Control
7 | BK | 1250 | Ground
8 | D-GN | 168 | Power Window Master Switch Right Rear Up Signal