For 1990-2009 cars

### Removal Procedure

1. Remove the body hinge pillar trim pane. Refer to Body Hinge Pillar Trim Panel Replacement .
2. Remove the front door sill plate. Refer to Front Side Door Sill Plate Replacement .
3. Remove the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement
4. Remove the front door opening weatherstrip.

### Installation Procedure

1. Install the front door opening weatherstrip.
2. Install the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement
3. Install the front door sill plate. Refer to Front Side Door Sill Plate Replacement .
4. Install the body hinge pillar trim pane. Refer to Body Hinge Pillar Trim Panel Replacement .