For 1990-2009 cars

### Removal Procedure

1. Remove the sunroof. Refer to Sunroof Module Assembly Replacement .
2. Remove the sunshade steps.
3. Remove the bolts and the drain channel.
4. Remove the sunshade.

### Installation Procedure

1. Install the sunshade.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the drain channel with the bolts.

Tighten
Tighten the drain channel bolts to 3 N·m (27 lb in).

3. Install the sunshade stops.
4. Install the sunroof. Refer to Sunroof Module Assembly Replacement .