For 1990-2009 cars

## Clutch Slipping D16 and D20 Manual Transaxle

Checks | Actions
--- | ---
Check for a stuck concentric slave cylinder. | Replace the concentric slave cylinder.
Check for improper return of clutch oil. | Perform the air bleeding.
Check for a worn clutch disc or oil contamination. | Replace the clutch disc.
Check for a warped pressure plate. | Replace the pressure plate.

## Clutch Slipping D33 Manual Transaxle

Checks | Actions
--- | ---
Check for a stuck concentric slave cylinder. | Replace the concentric slave cylinder.
Check for improper return of clutch oil. | Perform the air bleeding.
Check for a worn clutch disc or oil contamination. | Replace the pressure plate and clutch disc.
Check for a warped pressure plate. | Replace the pressure plate and clutch disc.